calibrator              Calibrator HOBO data in CSV format
correction              Correction test for HOBO data from calibrator
correction.test         Correction Test for HOBO data from calibrator
count_NAs               HOBO count NA's This function counts the number
                        of NA's in your data set
hobinder                Reads HOBO data in CSV format
hobocleaner             Reads HOBO data in CSV format
hobocorrelations        Correlation plot for variables within a time
                        range
hoborange               Calculate Date Range Temperature Using HOBO
                        Data
hobotime                Summarise HOBO data by time intervals
impossiblevalues        HOBO impossible values
meanhobo                mean HOBO data in CSV format
sampling.rates          Calculates sampling rates from a CSV format
sensorfailures          HOBO Remove Values This function is designed to
                        identify and address values that are likely to
                        be out of range, such as temperatures exceeding
                        the maximum recorded in your study area or
                        relative humidity (RH) values exceeding 100%,
                        which are not feasible. The 'sensorfailure()'
                        function allows you to detect and flag these
                        anomalous readings, facilitating the cleansing
                        of your dataset by replacing all out-of-range
                        values with NA's, maintaining the integrity and
                        accuracy of of your data analysis.
testhobolist            Test HOBO data for calibration
timestamp               Timestamp for Specific Intervals
