Common YANG Data Types for Traffic Engineering
Italo Busi
Huawei
italo.busi@huawei.com
Aihua Guo
Futurewei Technologies
aihuaguo.ietf@gmail.com
Xufeng Liu
Alef Edge
xufeng.liu.ietf@gmail.com
Tarek Saad
Cisco Systems Inc.
tsaad.net@gmail.com
Igor Bryskin
Individual
i_bryskin@yahoo.com
25 July 2024
TEAS Working Group
This document defines a collection of common data types, identities, and groupings in YANG data modeling language. These derived common data types, identities and groupings are intended to be imported by other modules, e.g., those which model the Traffic Engineering (TE) configuration and state capabilities.
This document obsoletes RFC 8776.
Introduction
YANG [RFC6020] [RFC7950] is a data modeling language used to model configuration data, state data, Remote Procedure Calls, and notifications for network management protocols such as the Network Configuration Protocol (NETCONF) [RFC6241] or RESTCONF [RFC8040]. The YANG language supports a small set of built-in data types and provides mechanisms to derive other types from the built-in types.
This document introduces a collection of common data types derived from the built-in YANG data types. The derived data types, identities, and groupings are mainly designed to be the common definitions applicable for modeling Traffic Engineering (TE) features in model(s) defined outside of this document. Nevertheless, these common definitions can be used by any other module per the guidance in Section 4.12 of [I-D.ietf-netmod-rfc8407bis].
This document adds new common data types, identities, and groupings to both the "ietf-te-types" and the "ietf-te-packet-types" YANG models and obsoletes [RFC8776]. For further details, refer to Appendix A.
Terminology
The key words "MUST", "MUST NOT", "REQUIRED", "SHALL", "SHALL NOT", "SHOULD", "SHOULD NOT", "RECOMMENDED", "NOT RECOMMENDED", "MAY", and "OPTIONAL" in this document are to be interpreted as described in BCP 14 [RFC2119] [RFC8174] when, and only when, they appear in all capitals, as shown here.
The terminology for describing YANG data models is found in [RFC7950].
- RFC Editor: The document uses "CHANGE NOTE" to ease identifying the changes vs. RFC8776. Please remove these notes.
Prefixes in Data Node Names
Names of data nodes and other data model objects are prefixed using the standard prefix associated with the corresponding YANG imported modules, as shown in Table 1.

Prefixes and corresponding YANG modules
Prefix | YANG module | Reference
yang | ietf-yang-types | Section 3 of [RFC6991]
inet | ietf-inet-types | Section 4 of [RFC6991]
rt-types | ietf-routing-types | [RFC8294]
te-types | ietf-te-types | RFCXXXX
te-packet-types | ietf-te-packet-types | RFCXXXX
- RFC Editor: Please replace XXXX through this document with the RFC number assigned to this document. Please remove this note.
Acronyms and Abbreviations
GMPLS:
Generalized Multiprotocol Label Switching
LSP:
Label Switched Path
LSR:
Label Switching Router
LER:
Label Edge Router
MPLS:
Multiprotocol Label Switching
RSVP:
Resource Reservation Protocol
TE:
Traffic Engineering
DS-TE:
Differentiated Services Traffic Engineering
SRLG:
Shared Risk Link Group
NBMA:
Non-Broadcast Multi-Access
APS:
Automatic Protection Switching
SD:
Signal Degrade
SF:
Signal Fail
WTR:
Wait-to-Restore
PM:
Performance Metrics
Overview
This document defines two YANG modules for common TE types: "ietf-te-types" for TE generic types and "ietf-te-packet-types" for packet-specific types. Other technology-specific TE types are outside the scope of this document.
TE Types Module Contents
The "ietf-te-types" module (Section 4) contains common TE types that are independent and agnostic of any specific technology or control-plane instance.
The "ietf-te-types" module contains the following YANG reusable groupings:
te-bandwidth:
A YANG grouping that defines the generic TE bandwidth. The modeling structure allows augmentation for each technology. For unspecified technologies, the string-encoded "te-bandwidth" type is used.
te-label:
A YANG grouping that defines the generic TE label. The modeling structure allows augmentation for each technology. For unspecified technologies, "rt-types:generalized-label" is used.
performance-metrics-attributes:
A YANG grouping that defines one-way and two-way measured Performance Metrics (PM) and indications of anomalies on link(s) or the path as defined in [RFC7471], [RFC8570], and [RFC7823].
performance-metrics-throttle-container:
A YANG grouping that defines configurable thresholds for advertisement suppression and measurement intervals.
The "ietf-te-types" module contains the following YANG reusable data types:
te-ds-class:
A type representing the Differentiated Services (DS) Class-Type of traffic as defined in [RFC4124].
te-label-direction:
An enumerated type for specifying the forward or reverse direction of a label.
te-hop-type:
An enumerated type for specifying that a hop is loose or strict.
te-global-id:
A type representing the identifier that uniquely identifies an operator, which can be either a provider or a client. The definition of this type is taken from Section 3 of [RFC6370] and Section 3 of [RFC5003]. This attribute type is used solely to provide a globally unique context for TE topologies.
te-node-id:
A type representing the identifier for a node in a TE topology. The identifier is represented either as 4 octets in dotted-quad notation or as 16 octets in full, mixed, shortened, or shortened-mixed IPv6 address notation.
This attribute MAY be mapped to the Router Address TLV described in Section 2.4.1 of [RFC3630], the TE Router ID described in Section 6.2 of [RFC6827], the Traffic Engineering Router ID TLV described in Section 4.3 of [RFC5305], or the TE Router ID TLV described in Section 3.2.1 of [RFC6119].
The reachability of such a TE node MAY be achieved by a mechanism such as that described in Section 6.2 of [RFC6827].
te-topology-id:
A type representing the identifier for a topology. It is optional to have one or more prefixes at the beginning, separated by colons. The prefixes can be "network-types" as defined in the "ietf-network" module in [RFC8345], to help the user better understand the topology before further inquiry is made.
te-tp-id:
A type representing the identifier of a TE interface Link Termination Point (LTP) on a specific TE node where the TE link connects. This attribute is mapped to a local or remote link identifier [RFC3630] [RFC5305].
te-path-disjointness:
A type representing the different resource disjointness options for a TE tunnel path as defined in [RFC4872].
admin-groups:
A union type for a TE link's classic or extended administrative groups as defined in [RFC3630], [RFC5305], and [RFC7308].
srlg:
A type representing the Shared Risk Link Group (SRLG) as defined in [RFC4203] and [RFC5307].
te-metric:
A type representing the TE metric as defined in [RFC3785].
te-recovery-status:
An enumerated type for the different statuses of a recovery action as defined in [RFC4427] and [RFC6378].
The "ietf-te-types" module contains the following YANG reusable identities:
path-attribute-flags:
A base YANG identity for supported LSP path flags as defined in [RFC3209], [RFC4090], [RFC4736], [RFC5712], [RFC4920], [RFC5420], [RFC7570], [RFC4875], [RFC5151], [RFC5150], [RFC6001], [RFC6790], [RFC7260], [RFC8001], [RFC8149], and [RFC8169].
link-protection-type:
A base YANG identity for supported link protection types as defined in [RFC4872] and [RFC4427].
restoration-scheme-type:
A base YANG identity for supported LSP restoration schemes as defined in [RFC4872].
protection-external-commands:
A base YANG identity for supported protection-related external commands used for troubleshooting purposes, as defined in [RFC4427] and [ITU_G.808.1].
- CHANGE NOTE: The description and reference of the identity action-exercise, which applies only to APS and it is not defined in RFC4427, has been updated to reference ITU-T G.808.1.
association-type:
A base YANG identity for supported LSP association types as defined in [RFC6780], [RFC4872], [RFC4873], and [RFC8800].
- CHANGE NOTE: The association-type-diversity identity, defined in [RFC8800] has been added to the association-type base identity.
objective-function-type:
A base YANG identity for supported path objective functions as defined in [RFC5541].
- CHANGE NOTE: The objective-function-type identity has been redefined to be used only for path objective functions and a new svec-objective-function-type identity has been added for the Synchronization VECtor (SVEC) objective functions. Therefore the of-minimize-agg-bandwidth-consumption, of-minimize-load-most-loaded-link and of-minimize-cost-path-set identities, defined in [RFC5541] and derived from the objective-function-type identity, have been obsoleted because not applicable to paths but to Synchronization VECtor (SVEC) objects.
te-tunnel-type:
A base YANG identity for supported TE tunnel types as defined in [RFC3209] and [RFC4875].
lsp-encoding-types:
A base YANG identity for supported LSP encoding types as defined in [RFC3471].
lsp-protection-type:
A base YANG identity for supported LSP protection types as defined in [RFC4872] and [RFC4873].
switching-capabilities:
A base YANG identity for supported interface switching capabilities as defined in [RFC3471].
resource-affinities-type:
A base YANG identity for supported attribute filters associated with a tunnel that must be satisfied for a link to be acceptable as defined in [RFC2702] and [RFC3209].
- CHANGE NOTE: The description of the path-metric-type has been updated
path-metric-type:
A base YANG identity for supported path metric types as defined in [RFC3630] [RFC3785], [RFC5440], [RFC7471], [RFC8233], [RFC8570] and [I-D.ietf-pce-sid-algo].
The unit of the path metric value is interpreted in the context of the path metric type. The derived identities SHOULD describe the unit and maximum value of the path metric types they define.
For example, the bound of the 'path-metric-loss', defined in 'ietf-te-packet-types', is defined in multiples of the basic unit 0.000003% as described in [RFC7471] and [RFC8570].
explicit-route-hop:
A YANG grouping that defines supported explicit routes as defined in [RFC3209] and [RFC3477].
te-link-access-type:
An enumerated type for the different TE link access types as defined in [RFC3630].
- CHANGE NOTE: The module "ietf-te-types" has been updated to add the following YANG identities, types and groupings.
lsp-provisioning-error-reason:
A base YANG identity for reporting LSP provisioning error reasons. No standard LPS provisioning error reasons are defined in this document.
path-computation-error-reason:
A base YANG identity for reporting path computation error reasons as defined in Section 3.1.1.
protocol-origin-type:
A base YANG identity for the type of protocol origin as defined in Section 3.1.2.
svec-objective-function-type:
A base YANG identity for supported SVEC objective functions as defined in [RFC5541] and [RFC8685].
svec-metric-type:
A base YANG identity for supported SVEC objective functions as defined in [RFC5541].
encoding-and-switching-type:
This is a common grouping to define the LSP encoding and switching types.
- CHANGE NOTE: The tunnel-admin-state-auto YANG identity, derived from the tunnel-admin-status-type base YANG identity has also been added. No description is provided, since no description for the tunnel-admin-status-type base YANG identity has been provided in RFC8776.
- CHANGE NOTE: The lsp-restoration-restore-none YANG identity, derived from the lsp-restoration-type base YANG identity has also been added. No description is provided, since no description for the lsp-restoration-type base YANG identity has been provided in RFC8776.
Path Computation Errors
The "ietf-te-types" module contains the YANG reusable identities for reporting path computation error reasons as defined in [RFC5440], [RFC5441], [RFC5520], [RFC5557], [RFC8306], and [RFC8685].
It also defines the following additional YANG reusable identities for reporting also the following path computation error reasons:
path-computation-error-no-topology:
A YANG identity for reporting path computation error when there is no topology with the provided topology identifier.
Protocol Origin
The "ietf-te-types" module contains the YANG reusable identities for the type of protocol origin as defined in [RFC5440] and [RFC9012].
It also defines the following additional YANG reusable identities for the type of protocol origin:
protocol-origin-api:
A YANG identity to be used when the type of protocol origin is an Application Programmable Interface (API).
Packet TE Types Module Contents
The "ietf-te-packet-types" module (Section 5) covers the common types and groupings that are specific to packet technology.
The "ietf-te-packet-types" module contains the following YANG reusable types and groupings:
backup-protection-type:
A base YANG identity for supported protection types that a backup or bypass tunnel can provide as defined in [RFC4090].
te-class-type:
A type that represents the Diffserv-TE Class-Type as defined in [RFC4124].
bc-type:
A type that represents Diffserv-TE Bandwidth Constraints (BCs) as defined in [RFC4124].
bc-model-type:
A base YANG identity for supported Diffserv-TE Bandwidth Constraints Models as defined in [RFC4125], [RFC4126], and [RFC4127].
te-bandwidth-requested-type:
An enumerated type for the different options to request bandwidth for a specific tunnel.
performance-metrics-attributes-packet:
A YANG grouping that contains the generic performance metrics and additional packet-specific metrics.
- CHANGE NOTE: The module "ietf-te-packet-types" has been updated to add the following YANG identities and groupings.
bandwidth-profile-type:
A base YANG identity for various bandwidth profiles specified in [MEF_10.3], [RFC2697], [RFC2698] and [RFC4115] that may be used to limit bandwidth utilization of packet flows (e.g., MPLS-TE LSPs).
te-packet-path-bandwidth:
A YANG grouping that defines the path bandwidth information and could be used in any Packet TE model (e.g., MPLS-TE topology model) for the path bandwidth representation (e.g., the bandwidth of an MPLS-TE LSP).
All the path and LSP bandwidth related sections in the "ietf-te-types" generic module, Section 4, need to be augmented with this grouping for the usage of Packet TE technologies.
The Packet TE path bandwidth can be represented by a bandwidth profile.
- NOTE: Other formats for the MPLS-TE path bandwidth are defined in [I-D.ietf-teas-yang-te-mpls] and they could be added in a future update of this document.
te-packet-link-bandwidth:
A YANG grouping that defines the link bandwidth information and could be used in any Packet TE model (e.g., MPLS-TE topology) for link bandwidth representation.
All the link bandwidth related sections in the "ietf-te-types" generic module, Section 4, need to be augmented with this grouping for the usage of Packet TE technologies.
TE Types YANG Module
The "ietf-te-types" module imports from the following modules:
- "ietf-yang-types" and "ietf-inet-types" as defined in [RFC6991]
- "ietf-routing-types" as defined in [RFC8294]
In addition to [RFC6991] and [RFC8294], this module references the following documents in defining the types and YANG groupings: [RFC9522], [RFC4090], [RFC4202], [RFC4328], [RFC4561], [RFC4657], [RFC4736], [RFC6004], [RFC6511], [RFC7139], [RFC7308], [RFC7551], [RFC7571], [RFC7579], and [ITU-T_G.709].
- CHANGE NOTE: Please focus your review only on the updates to the YANG model: see also Appendix A.1.

TE Types YANG module

module ietf-te-types {
  yang-version 1.1;
  namespace "urn:ietf:params:xml:ns:yang:ietf-te-types";
  prefix te-types;

  import ietf-inet-types {
    prefix inet;
    reference
      "RFC 6991: Common YANG Data Types";
  }
  import ietf-yang-types {
    prefix yang;
    reference
      "RFC 6991: Common YANG Data Types";
  }
  import ietf-routing-types {
    prefix rt-types;
    reference
      "RFC 8294: Common YANG Data Types for the Routing Area";
  }

  import ietf-network {
    prefix "nw";
    reference
      "RFC 8345: A YANG Data Model for Network Topologies";
  }

  import ietf-network-topology {
    prefix "nt";
    reference
      "RFC 8345: A YANG Data Model for Network Topologies";
  }

  organization
    "IETF Traffic Engineering Architecture and Signaling (TEAS)
     Working Group";
  contact
    "WG Web:   <https://datatracker.ietf.org/wg/teas/>
     WG List:  <mailto:teas@ietf.org>

     Editor:   Tarek Saad
               <mailto:tsaad.net@gmail.com>

     Editor:   Rakesh Gandhi
               <mailto:rgandhi@cisco.com>

     Editor:   Vishnu Pavan Beeram
               <mailto:vbeeram@juniper.net>

     Editor:   Xufeng Liu
               <mailto:xufeng.liu.ietf@gmail.com>

     Editor:   Igor Bryskin
               <mailto:i_bryskin@yahoo.com>";
  description
    "This YANG module contains a collection of generally useful
     YANG data type definitions specific to TE.  The model fully
     conforms to the Network Management Datastore Architecture
     (NMDA).

     The key words 'MUST', 'MUST NOT', 'REQUIRED', 'SHALL', 'SHALL
     NOT', 'SHOULD', 'SHOULD NOT', 'RECOMMENDED', 'NOT RECOMMENDED',
     'MAY', and 'OPTIONAL' in this document are to be interpreted as
     described in BCP 14 (RFC 2119) (RFC 8174) when, and only when,
     they appear in all capitals, as shown here.

     Copyright (c) 2024 IETF Trust and the persons identified as
     authors of the code.  All rights reserved.

     Redistribution and use in source and binary forms, with or
     without modification, is permitted pursuant to, and subject to
     the license terms contained in, the Revised BSD License set
     forth in Section 4.c of the IETF Trust's Legal Provisions
     Relating to IETF Documents
     (https://trustee.ietf.org/license-info).

     This version of this YANG module is part of RFC XXXX
     (https://www.rfc-editor.org/info/rfcXXXX); see the RFC itself
     for full legal notices.";
  revision 2024-07-23 {
    description
      "This revision adds the following new identities:
      - lsp-provisioning-error-reason;
      - association-type-diversity;
      - tunnel-admin-state-auto;
      - lsp-restoration-restore-none;
      - restoration-scheme-rerouting;
      - path-metric-optimization-type;
      - link-path-metric-type;
      - link-metric-type and its derived identities;
      - path-computation-error-reason and its derived identities;
      - protocol-origin-type and its derived identities;
      - svec-objective-function-type and its derived identities;
      - svec-metric-type and its derived identities.

      This revision adds the following new data types:
      - path-type;
      - te-gen-node-id.

      This revision adds the following new groupings:
      - encoding-and-switching-type;
      - te-generic-node-id.

      This revision updates the following identities:
      - objective-function-type;
      - action-exercise;
      - path-metric-type;
      - path-metric-te;
      - path-metric-igp;
      - path-metric-hop;
      - path-metric-delay-average;
      - path-metric-delay-minimum;
      - path-metric-residual-bandwidth;
      - path-metric-optimize-includes;
      - path-metric-optimize-excludes;
      - te-optimization-criterion.

      This revision updates the following data types:
      - te-node-id.

      This revision updates the following groupings:
      - explicit-route-hop:
        - adds the following leaves:
          - node-id-uri;
          - link-tp-id-uri;
        - updates the following leaves:
          - node-id;
          - link-tp-id;
      - record-route-state:
        - adds the following leaves:
          - node-id-uri;
          - link-tp-id-uri;
        - updates the following leaves:
          - node-id;
          - link-tp-id;
      - optimization-metric-entry:
        - updates the following leaves:
          - metric-type;
      - tunnel-constraints;
        - adds the following leaves:
          - network-id;
      - path-constraints-route-objects:
        - updates the following containers:
          - explicit-route-objects-always;
      - generic-path-metric-bounds:
        - updates the following leaves:
          - metric-type;
      - generic-path-optimization
        - adds the following leaves:
          - tiebreaker;
        - deprecate the following containers:
          - tiebreakers.

      This revision obsoletes the following identities:
      - of-minimize-agg-bandwidth-consumption;
      - of-minimize-load-most-loaded-link;
      - of-minimize-cost-path-set;
      - lsp-protection-reroute-extra;
      - lsp-protection-reroute.

      This revision provides also few editorial changes.";
    reference
      "RFC XXXX: Common YANG Data Types for Traffic Engineering";
  }
  // RFC Editor: replace XXXX with actual RFC number, update date
  // information and remove this note

  revision 2020-06-10 {
    description
      "Initial Version of TE types.";
    reference
      "RFC 8776: Common YANG Data Types for Traffic Engineering";
  }

  /**
   * Typedefs
   */

  typedef admin-group {
    type yang:hex-string {
      /* 01:02:03:04 */
      length "1..11";
    }
    description
      "Administrative group / resource class / color representation
       in 'hex-string' type.

       The most significant byte in the hex-string is the farthest
       to the left in the byte sequence.  Leading zero bytes in the
       configured value may be omitted for brevity.";
    reference
      "RFC 3630: Traffic Engineering (TE) Extensions to OSPF
                 Version 2
       RFC 5305: IS-IS Extensions for Traffic Engineering
       RFC 7308: Extended Administrative Groups in MPLS Traffic
                 Engineering (MPLS-TE)";
  }

  typedef admin-groups {
    type union {
      type admin-group;
      type extended-admin-group;
    }
    description
      "Derived types for TE administrative groups.";
  }

  typedef extended-admin-group {
    type yang:hex-string;
    description
      "Extended administrative group / resource class / color
       representation in 'hex-string' type.

       The most significant byte in the hex-string is the farthest
       to the left in the byte sequence.  Leading zero bytes in the
       configured value may be omitted for brevity.";
    reference
      "RFC 7308: Extended Administrative Groups in MPLS Traffic
                 Engineering (MPLS-TE)";
  }

  typedef path-attribute-flags {
    type union {
      type identityref {
        base session-attributes-flags;
      }
      type identityref {
        base lsp-attributes-flags;
      }
    }
    description
      "Path attributes flags type.";
  }

  typedef performance-metrics-normality {
    type enumeration {
      enum unknown {
        value 0;
        description
          "Unknown.";
      }
      enum normal {
        value 1;
        description
          "Normal.  Indicates that the anomalous bit is not set.";
      }
      enum abnormal {
        value 2;
        description
          "Abnormal.  Indicates that the anomalous bit is set.";
      }
    }
    description
      "Indicates whether a performance metric is normal (anomalous
       bit not set), abnormal (anomalous bit set), or unknown.";
    reference
      "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions
       RFC 7823: Performance-Based Path Selection for Explicitly
                 Routed Label Switched Paths (LSPs) Using TE Metric
                 Extensions
       RFC 8570: IS-IS Traffic Engineering (TE) Metric Extensions";
  }

  typedef srlg {
    type uint32;
    description
      "SRLG type.";
    reference
      "RFC 4203: OSPF Extensions in Support of Generalized
                 Multi-Protocol Label Switching (GMPLS)
       RFC 5307: IS-IS Extensions in Support of Generalized
                 Multi-Protocol Label Switching (GMPLS)";
  }

  typedef te-common-status {
    type enumeration {
      enum up {
        description
          "Enabled.";
      }
      enum down {
        description
          "Disabled.";
      }
      enum testing {
        description
          "In some test mode.";
      }
      enum preparing-maintenance {
        description
          "The resource is disabled in the control plane to prepare
           for a graceful shutdown for maintenance purposes.";
        reference
          "RFC 5817: Graceful Shutdown in MPLS and Generalized MPLS
                     Traffic Engineering Networks";
      }
      enum maintenance {
        description
          "The resource is disabled in the data plane for maintenance
           purposes.";
      }
      enum unknown {
        description
          "Status is unknown.";
      }
    }
    description
      "Defines a type representing the common states of a TE
       resource.";
  }

  typedef te-bandwidth {
    type string {
      pattern '0[xX](0((\.0?)?[pP](\+)?0?|(\.0?))|'
            + '1(\.([\da-fA-F]{0,5}[02468aAcCeE]?)?)?'
            + '[pP](\+)?(12[0-7]|'
            + '1[01]\d|0?\d?\d)?)|0[xX][\da-fA-F]{1,8}|\d+'
            + '(,(0[xX](0((\.0?)?[pP](\+)?0?|(\.0?))|'
            + '1(\.([\da-fA-F]{0,5}[02468aAcCeE]?)?)?'
            + '[pP](\+)?(12[0-7]|'
            + '1[01]\d|0?\d?\d)?)|0[xX][\da-fA-F]{1,8}|\d+))*';
    }
    description
      "This is the generic bandwidth type.  It is a string containing
       a list of numbers separated by commas, where each of these
       numbers can be non-negative decimal, hex integer, or
       hex float:

       (dec | hex | float)[*(','(dec | hex | float))]

       For the packet-switching type, the string encoding follows
       the type 'bandwidth-ieee-float32' as defined in RFC 8294
       (e.g., 0x1p10), where the units are in bytes per second.

       For the Optical Transport Network (OTN) switching type,
       a list of integers can be used, such as '0,2,3,1', indicating
       two ODU0s and one ODU3.  ('ODU' stands for 'Optical Data
       Unit'.)  For Dense Wavelength Division Multiplexing (DWDM),
       a list of pairs of slot numbers and widths can be used,
       such as '0,2,3,3', indicating a frequency slot 0 with
       slot width 2 and a frequency slot 3 with slot width 3.
       Canonically, the string is represented as all lowercase and in
       hex, where the prefix '0x' precedes the hex number.";
    reference
      "RFC 8294: Common YANG Data Types for the Routing Area
       ITU-T G.709: Interfaces for the optical transport network -
                    Edition 6.0 (06/2020)";
  }

  typedef te-ds-class {
    type uint8 {
      range "0..7";
    }
    description
      "The Differentiated Services Class-Type of traffic.";
    reference
      "RFC 4124: Protocol Extensions for Support of Diffserv-aware
                 MPLS Traffic Engineering, Section 4.3.1";
  }

  typedef te-global-id {
    type uint32;
    description
      "An identifier to uniquely identify an operator, which can be
       either a provider or a client.

       The definition of this type is taken from RFCs 6370 and 5003.

       This attribute type is used solely to provide a globally
       unique context for TE topologies.";
    reference
      "RFC 5003: Attachment Individual Identifier (AII) Types for
                 Aggregation
       RFC 6370: MPLS Transport Profile (MPLS-TP) Identifiers";
  }

  typedef te-hop-type {
    type enumeration {
      enum loose {
        description
          "A loose hop in an explicit path.";
      }
      enum strict {
        description
          "A strict hop in an explicit path.";
      }
    }
    description
      "Enumerated type for specifying loose or strict paths.";
    reference
      "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels,
                 Section 4.3.3";
  }

  typedef te-link-access-type {
    type enumeration {
      enum point-to-point {
        description
          "The link is point-to-point.";
      }
      enum multi-access {
        description
          "The link is multi-access, including broadcast and NBMA.";
      }
    }
    description
      "Defines a type representing the access type of a TE link.";
    reference
      "RFC 3630: Traffic Engineering (TE) Extensions to OSPF
                 Version 2";
  }

  typedef te-label-direction {
    type enumeration {
      enum forward {
        description
          "Label allocated for the forward LSP direction.";
      }
      enum reverse {
        description
          "Label allocated for the reverse LSP direction.";
      }
    }
    description
      "Enumerated type for specifying the forward or reverse
       label.";
  }

  typedef te-link-direction {
    type enumeration {
      enum incoming {
        description
          "The explicit route represents an incoming link on
           a node.";
      }
      enum outgoing {
        description
          "The explicit route represents an outgoing link on
           a node.";
      }
    }
    description
      "Enumerated type for specifying the direction of a link on
       a node.";
  }

  typedef te-metric {
    type uint32;
    description
      "TE metric.";
    reference
      "RFC 3785: Use of Interior Gateway Protocol (IGP) Metric as a
                 second MPLS Traffic Engineering (TE) Metric";
  }

  // CHANGE NOTE: The typedef te-node-id below has been
  // updated in this module revision
  // RFC Editor: remove the note above and this note
  typedef te-node-id {
    type union {
      type yang:dotted-quad;
      type inet:ipv6-address-no-zone;
    }
    description
      "A type representing the identifier for a node in a TE
       topology.

       The identifier is represented either as 4 octets in
       dotted-quad notation, or as 16 octets in full, mixed,
       shortened, or shortened-mixed IPv6 address notation.

       This attribute MAY be mapped to the Router Address TLV
       described in Section 2.4.1 of RFC 3630, the TE Router ID
       described in Section 3 of RFC 6827, the Traffic Engineering
       Router ID TLV described in Section 4.3 of RFC 5305, the TE
       Router ID TLV described in Section 3.2.1 of RFC 6119, or the
       IPv6 TE Router ID TLV described in Section 4.1 of RFC 6119.

       The reachability of such a TE node MAY be achieved by a
       mechanism such as that described in Section 6.2 of RFC 6827.";
    reference
      "RFC 3630: Traffic Engineering (TE) Extensions to OSPF
                 Version 2, Section 2.4.1
       RFC 5305: IS-IS Extensions for Traffic Engineering,
                 Section 4.3
       RFC 6119: IPv6 Traffic Engineering in IS-IS, Section 3.2.1
       RFC 6827: Automatically Switched Optical Network (ASON)
                 Routing for OSPFv2 Protocols, Section 3";
  }

  typedef te-oper-status {
    type te-common-status;
    description
      "Defines a type representing the operational status of
       a TE resource.";
  }

  typedef te-admin-status {
    type te-common-status;
    description
      "Defines a type representing the administrative status of
       a TE resource.";
  }

  typedef te-path-disjointness {
    type bits {
      bit node {
        position 0;
        description
          "Node disjoint.";
      }
      bit link {
        position 1;
        description
          "Link disjoint.";
      }
      bit srlg {
        position 2;
        description
          "SRLG (Shared Risk Link Group) disjoint.";
      }
    }
    description
      "Type of the resource disjointness for a TE tunnel path.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  typedef te-recovery-status {
    type enumeration {
      enum normal {
        description
          "Both the recovery span and the working span are fully
           allocated and active, data traffic is being
           transported over (or selected from) the working
           span, and no trigger events are reported.";
      }
      enum recovery-started {
        description
          "The recovery action has been started but not completed.";
      }
      enum recovery-succeeded {
        description
          "The recovery action has succeeded.  The working span has
           reported a failure/degrade condition, and the user traffic
           is being transported (or selected) on the recovery span.";
      }
      enum recovery-failed {
        description
          "The recovery action has failed.";
      }
      enum reversion-started {
        description
          "The reversion has started.";
      }
      enum reversion-succeeded {
        description
          "The reversion action has succeeded.";
      }
      enum reversion-failed {
        description
          "The reversion has failed.";
      }
      enum recovery-unavailable {
        description
          "The recovery is unavailable, as a result of either an
           operator's lockout command or a failure condition
           detected on the recovery span.";
      }
      enum recovery-admin {
        description
          "The operator has issued a command to switch the user
           traffic to the recovery span.";
      }
      enum wait-to-restore {
        description
          "The recovery domain is recovering from a failure/degrade
           condition on the working span that is being controlled by
           the Wait-to-Restore (WTR) timer.";
      }
    }
    description
      "Defines the status of a recovery action.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)
       RFC 6378: MPLS Transport Profile (MPLS-TP) Linear Protection";
  }

  typedef te-template-name {
    type string {
      pattern '/?([a-zA-Z0-9\-_.]+)(/[a-zA-Z0-9\-_.]+)*';
    }
    description
      "A type for the name of a TE node template or TE link
       template.";
  }

  typedef te-topology-event-type {
    type enumeration {
      enum add {
        value 0;
        description
          "A TE node or TE link has been added.";
      }
      enum remove {
        value 1;
        description
          "A TE node or TE link has been removed.";
      }
      enum update {
        value 2;
        description
          "A TE node or TE link has been updated.";
      }
    }
    description
      "TE event type for notifications.";
  }

  typedef te-topology-id {
    type union {
      type string {
        length "0";
        // empty string
      }
      type string {
        pattern '([a-zA-Z0-9\-_.]+:)*'
              + '/?([a-zA-Z0-9\-_.]+)(/[a-zA-Z0-9\-_.]+)*';
      }
    }
    description
      "An identifier for a topology.

       It is optional to have one or more prefixes at the beginning,
       separated by colons.  The prefixes can be 'network-types' as
       defined in the 'ietf-network' module in RFC 8345, to help the
       user better understand the topology before further inquiry
       is made.";
    reference
      "RFC 8345: A YANG Data Model for Network Topologies";
  }

  typedef te-tp-id {
    type union {
      type uint32;
      // Unnumbered
      type inet:ip-address;
      // IPv4 or IPv6 address
    }
    description
      "An identifier for a TE link endpoint on a node.

       This attribute is mapped to a local or remote link identifier
       as defined in RFCs 3630 and 5305.";
    reference
      "RFC 3630: Traffic Engineering (TE) Extensions to OSPF
                 Version 2
       RFC 5305: IS-IS Extensions for Traffic Engineering";
  }

  // CHANGE NOTE: The typedef path-type below has been
  // added in this module revision
  // RFC Editor: remove the note above and this note
  typedef path-type {
    type enumeration {
      enum primary-path {
        description
          "Indicates that the TE path is a primary path.";
      }
      enum secondary-path {
        description
          "Indicates that the TE path is a secondary path.";
      }
      enum primary-reverse-path {
        description
          "Indicates that the TE path is a primary reverse path.";
      }
      enum secondary-reverse-path {
        description
          "Indicates that the TE path is a secondary reverse path.";
      }
    }
    description
      "The type of TE path, indicating whether a path is a primary,
       or a reverse primary, or a secondary, or a reverse secondary
       path.";
  }

  // CHANGE NOTE: The typedef te-gen-node-id below has been
  // added in this module revision
  // RFC Editor: remove the note above and this note
  typedef te-gen-node-id {
    type union {
      type te-node-id;
      type inet:ip-address;
      type nw:node-id;
    }
    description
      "Generic type that identifies a node in a TE topology.";
  }

  /* TE features */

  feature p2mp-te {
    description
      "Indicates support for Point-to-Multipoint TE (P2MP-TE).";
    reference
      "RFC 4875: Extensions to Resource Reservation Protocol -
                 Traffic Engineering (RSVP-TE) for
                 Point-to-Multipoint TE Label Switched Paths (LSPs)";
  }

  feature frr-te {
    description
      "Indicates support for TE Fast Reroute (FRR).";
    reference
      "RFC 4090: Fast Reroute Extensions to RSVP-TE for LSP Tunnels";
  }

  feature extended-admin-groups {
    description
      "Indicates support for TE link extended administrative
       groups.";
    reference
      "RFC 7308: Extended Administrative Groups in MPLS Traffic
                 Engineering (MPLS-TE)";
  }

  feature named-path-affinities {
    description
      "Indicates support for named path affinities.";
  }

  feature named-extended-admin-groups {
    description
      "Indicates support for named extended administrative groups.";
  }

  feature named-srlg-groups {
    description
      "Indicates support for named SRLG groups.";
  }

  feature named-path-constraints {
    description
      "Indicates support for named path constraints.";
  }

  feature path-optimization-metric {
    description
      "Indicates support for path optimization metrics.";
  }

  feature path-optimization-objective-function {
    description
      "Indicates support for path optimization objective functions.";
  }

  /*
   * Identities
   */

  // CHANGE NOTE: The base identity lsp-provisioning-error-reason
  // has been added in this module revision
  // RFC Editor: remove the note above and this note
  identity lsp-provisioning-error-reason {
    description
      "Base identity for LSP provisioning errors.";
  }

  identity session-attributes-flags {
    description
      "Base identity for the RSVP-TE session attributes flags.";
  }

  identity local-protection-desired {
    base session-attributes-flags;
    description
      "Local protection is desired.";
    reference
      "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels,
                 Section 4.7.1";
  }

  identity se-style-desired {
    base session-attributes-flags;
    description
      "Shared explicit style, to allow the LSP to be established
       and share resources with the old LSP.";
    reference
      "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels";
  }

  identity local-recording-desired {
    base session-attributes-flags;
    description
      "Label recording is desired.";
    reference
      "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels,
                 Section 4.7.1";
  }

  identity bandwidth-protection-desired {
    base session-attributes-flags;
    description
      "Requests FRR bandwidth protection on LSRs, if present.";
    reference
      "RFC 4090: Fast Reroute Extensions to RSVP-TE for LSP Tunnels";
  }

  identity node-protection-desired {
    base session-attributes-flags;
    description
      "Requests FRR node protection on LSRs, if present.";
    reference
      "RFC 4090: Fast Reroute Extensions to RSVP-TE for LSP Tunnels";
  }

  identity path-reevaluation-request {
    base session-attributes-flags;
    description
      "This flag indicates that a path re-evaluation (of the
       current path in use) is requested.  Note that this does
       not trigger any LSP reroutes but instead just signals a
       request to evaluate whether a preferable path exists.";
    reference
      "RFC 4736: Reoptimization of Multiprotocol Label Switching
                 (MPLS) Traffic Engineering (TE) Loosely Routed Label
                 Switched Path (LSP)";
  }

  identity soft-preemption-desired {
    base session-attributes-flags;
    description
      "Soft preemption of LSP resources is desired.";
    reference
      "RFC 5712: MPLS Traffic Engineering Soft Preemption";
  }

  identity lsp-attributes-flags {
    description
      "Base identity for LSP attributes flags.";
  }

  identity end-to-end-rerouting-desired {
    base lsp-attributes-flags;
    description
      "Indicates end-to-end rerouting behavior for an LSP
       undergoing establishment.  This MAY also be used to
       specify the behavior of end-to-end LSP recovery for
       established LSPs.";
    reference
      "RFC 4920: Crankback Signaling Extensions for MPLS and GMPLS
                 RSVP-TE
       RFC 5420: Encoding of Attributes for MPLS LSP Establishment
                 Using Resource Reservation Protocol Traffic
                 Engineering (RSVP-TE)
       RFC 7570: Label Switched Path (LSP) Attribute in the Explicit
                 Route Object (ERO)";
  }

  identity boundary-rerouting-desired {
    base lsp-attributes-flags;
    description
      "Indicates boundary rerouting behavior for an LSP undergoing
       establishment.  This MAY also be used to specify
       segment-based LSP recovery through nested crankback for
       established LSPs.  The boundary Area Border Router (ABR) /
       Autonomous System Border Router (ASBR) can decide to forward
       the PathErr message upstream to either an upstream boundary
       ABR/ASBR or the ingress LSR.  Alternatively, it can try to
       select another egress boundary LSR.";
    reference
      "RFC 4920: Crankback Signaling Extensions for MPLS and GMPLS
                 RSVP-TE
       RFC 5420: Encoding of Attributes for MPLS LSP Establishment
                 Using Resource Reservation Protocol Traffic
                 Engineering (RSVP-TE)
       RFC 7570: Label Switched Path (LSP) Attribute in the Explicit
                 Route Object (ERO)";
  }

  identity segment-based-rerouting-desired {
    base lsp-attributes-flags;
    description
      "Indicates segment-based rerouting behavior for an LSP
       undergoing establishment.  This MAY also be used to specify
       segment-based LSP recovery for established LSPs.";
    reference
      "RFC 4920: Crankback Signaling Extensions for MPLS and GMPLS
                 RSVP-TE
       RFC 5420: Encoding of Attributes for MPLS LSP Establishment
                 Using Resource Reservation Protocol
                 Traffic Engineering (RSVP-TE)
       RFC 7570: Label Switched Path (LSP) Attribute in the Explicit
                 Route Object (ERO)";
  }

  identity lsp-integrity-required {
    base lsp-attributes-flags;
    description
      "Indicates that LSP integrity is required.";
    reference
      "RFC 4875: Extensions to Resource Reservation Protocol -
                 Traffic Engineering (RSVP-TE) for
                 Point-to-Multipoint TE Label Switched Paths (LSPs)
       RFC 7570: Label Switched Path (LSP) Attribute in the Explicit
                 Route Object (ERO)";
  }

  identity contiguous-lsp-desired {
    base lsp-attributes-flags;
    description
      "Indicates that a contiguous LSP is desired.";
    reference
      "RFC 5151: Inter-Domain MPLS and GMPLS Traffic Engineering --
                 Resource Reservation Protocol-Traffic Engineering
                 (RSVP-TE) Extensions
       RFC 7570: Label Switched Path (LSP) Attribute in the Explicit
                 Route Object (ERO)";
  }

  identity lsp-stitching-desired {
    base lsp-attributes-flags;
    description
      "Indicates that LSP stitching is desired.";
    reference
      "RFC 5150: Label Switched Path Stitching with Generalized
                 Multiprotocol Label Switching Traffic Engineering
                 (GMPLS TE)
       RFC 7570: Label Switched Path (LSP) Attribute in the Explicit
                 Route Object (ERO)";
  }

  identity pre-planned-lsp-flag {
    base lsp-attributes-flags;
    description
      "Indicates that the LSP MUST be provisioned in the
       control plane only.";
    reference
      "RFC 6001: Generalized MPLS (GMPLS) Protocol Extensions for
                 Multi-Layer and Multi-Region Networks (MLN/MRN)
       RFC 7570: Label Switched Path (LSP) Attribute in the Explicit
                 Route Object (ERO)";
  }

  identity non-php-behavior-flag {
    base lsp-attributes-flags;
    description
      "Indicates that non-PHP (non-Penultimate Hop Popping) behavior
       for the LSP is desired.";
    reference
      "RFC 6511: Non-Penultimate Hop Popping Behavior and Out-of-Band
                 Mapping for RSVP-TE Label Switched Paths
       RFC 7570: Label Switched Path (LSP) Attribute in the Explicit
                 Route Object (ERO)";
  }

  identity oob-mapping-flag {
    base lsp-attributes-flags;
    description
      "Indicates that signaling of the egress binding information is
       out of band (e.g., via the Border Gateway Protocol (BGP)).";
    reference
      "RFC 6511: Non-Penultimate Hop Popping Behavior and Out-of-Band
                 Mapping for RSVP-TE Label Switched Paths
       RFC 7570: Label Switched Path (LSP) Attribute in the Explicit
                 Route Object (ERO)";
  }

  identity entropy-label-capability {
    base lsp-attributes-flags;
    description
      "Indicates entropy label capability.";
    reference
      "RFC 6790: The Use of Entropy Labels in MPLS Forwarding
       RFC 7570: Label Switched Path (LSP) Attribute in the Explicit
                 Route Object (ERO)";
  }

  identity oam-mep-entity-desired {
    base lsp-attributes-flags;
    description
      "OAM Maintenance Entity Group End Point (MEP) entities
       desired.";
    reference
      "RFC 7260: GMPLS RSVP-TE Extensions for Operations,
                 Administration, and Maintenance (OAM)
                 Configuration";
  }

  identity oam-mip-entity-desired {
    base lsp-attributes-flags;
    description
      "OAM Maintenance Entity Group Intermediate Points (MIP)
       entities desired.";
    reference
      "RFC 7260: GMPLS RSVP-TE Extensions for Operations,
                 Administration, and Maintenance (OAM)
                 Configuration";
  }

  identity srlg-collection-desired {
    base lsp-attributes-flags;
    description
      "SRLG collection desired.";
    reference
      "RFC 7570: Label Switched Path (LSP) Attribute in the Explicit
                 Route Object (ERO)
       RFC 8001: RSVP-TE Extensions for Collecting Shared Risk
                 Link Group (SRLG) Information";
  }

  identity loopback-desired {
    base lsp-attributes-flags;
    description
      "This flag indicates that a particular node on the LSP is
       required to enter loopback mode.  This can also be
       used to specify the loopback state of the node.";
    reference
      "RFC 7571: GMPLS RSVP-TE Extensions for Lock Instruct and
                 Loopback";
  }

  identity p2mp-te-tree-eval-request {
    base lsp-attributes-flags;
    description
      "P2MP-TE tree re-evaluation request.";
    reference
      "RFC 8149: RSVP Extensions for Reoptimization of Loosely Routed
                 Point-to-Multipoint Traffic Engineering Label
                 Switched Paths (LSPs)";
  }

  identity rtm-set-desired {
    base lsp-attributes-flags;
    description
      "Residence Time Measurement (RTM) attribute flag requested.";
    reference
      "RFC 8169: Residence Time Measurement in MPLS Networks";
  }

  identity link-protection-type {
    description
      "Base identity for the link protection type.";
  }

  identity link-protection-unprotected {
    base link-protection-type;
    description
      "Unprotected link type.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  identity link-protection-extra-traffic {
    base link-protection-type;
    description
      "Extra-Traffic protected link type.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity link-protection-shared {
    base link-protection-type;
    description
      "Shared protected link type.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  identity link-protection-1-for-1 {
    base link-protection-type;
    description
      "One-for-one (1:1) protected link type.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  identity link-protection-1-plus-1 {
    base link-protection-type;
    description
      "One-plus-one (1+1) protected link type.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  identity link-protection-enhanced {
    base link-protection-type;
    description
      "A compound link protection type derived from the underlay
       TE tunnel protection configuration supporting the TE link.";
  }

  identity association-type {
    description
      "Base identity for the tunnel association.";
  }

  identity association-type-recovery {
    base association-type;
    description
      "Association type for recovery, used to associate LSPs of the
       same tunnel for recovery.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery
       RFC 6780: RSVP ASSOCIATION Object Extensions";
  }

  identity association-type-resource-sharing {
    base association-type;
    description
      "Association type for resource sharing, used to enable
       resource sharing during make-before-break.";
    reference
      "RFC 4873: GMPLS Segment Recovery
       RFC 6780: RSVP ASSOCIATION Object Extensions";
  }

  identity association-type-double-sided-bidir {
    base association-type;
    description
      "Association type for double-sided bidirectional LSPs,
       used to associate two LSPs of two tunnels that are
       independently configured on either endpoint.";
    reference
      "RFC 7551: RSVP-TE Extensions for Associated Bidirectional
                 Label Switched Paths (LSPs)";
  }

  identity association-type-single-sided-bidir {
    base association-type;
    description
      "Association type for single-sided bidirectional LSPs,
       used to associate two LSPs of two tunnels, where one
       tunnel is configured on one side/endpoint and the other
       tunnel is dynamically created on the other endpoint.";
    reference
      "RFC 6780: RSVP ASSOCIATION Object Extensions
       RFC 7551: RSVP-TE Extensions for Associated Bidirectional
                 Label Switched Paths (LSPs)";
  }

  // CHANGE NOTE: The identity association-type-diversity below has
  // been added in this module revision
  // RFC Editor: remove the note above and this note
  identity association-type-diversity {
    base association-type;
    description
      "Association Type diversity used to associate LSPs whose
       paths are to be diverse from each other.";
    reference
      "RFC 8800: Path Computation Element Communication Protocol
                 (PCEP) Extension for Label Switched Path (LSP)
                 Diversity Constraint Signaling";
  }

  // CHANGE NOTE: The description of the base identity
  // objective-function-type has been updated
  // in this module revision
  // RFC Editor: remove the note above and this note
  identity objective-function-type {
    description
      "Base identity for path objective function types.";
  }

  identity of-minimize-cost-path {
    base objective-function-type;
    description
      "Objective function for minimizing path cost.";
    reference
      "RFC 5541: Encoding of Objective Functions in the Path
                 Computation Element Communication Protocol (PCEP)";
  }

  identity of-minimize-load-path {
    base objective-function-type;
    description
      "Objective function for minimizing the load on one or more
       paths.";
    reference
      "RFC 5541: Encoding of Objective Functions in the Path
                 Computation Element Communication Protocol (PCEP)";
  }

  identity of-maximize-residual-bandwidth {
    base objective-function-type;
    description
      "Objective function for maximizing residual bandwidth.";
    reference
      "RFC 5541: Encoding of Objective Functions in the Path
                 Computation Element Communication Protocol (PCEP)";
  }

  // CHANGE NOTE: The identity of-minimize-agg-bandwidth-consumption
  // below has been obsoleted in this module revision
  // RFC Editor: remove the note above and this note
  identity of-minimize-agg-bandwidth-consumption {
    base objective-function-type;
    status obsolete;
    description
      "Objective function for minimizing aggregate bandwidth
       consumption.

       This identity has been obsoleted: the
       'svec-of-minimize-agg-bandwidth-consumption' identity SHOULD
       be used instead.";
    reference
      "RFC 5541: Encoding of Objective Functions in the Path
                 Computation Element Communication Protocol (PCEP)";
  }

  // CHANGE NOTE: The identity of-minimize-load-most-loaded-link
  // below has been obsoleted in this module revision
  // RFC Editor: remove the note above and this note
  identity of-minimize-load-most-loaded-link {
    base objective-function-type;
    status obsolete;
    description
      "Objective function for minimizing the load on the link that
       is carrying the highest load.

       This identity has been obsoleted: the
       'svec-of-minimize-load-most-loaded-link' identity SHOULD
       be used instead.";
    reference
      "RFC 5541: Encoding of Objective Functions in the Path
                 Computation Element Communication Protocol (PCEP)";
  }

  // CHANGE NOTE: The identity of-minimize-cost-path-set
  // below has been obsoleted in this module revision
  // RFC Editor: remove the note above and this note
  identity of-minimize-cost-path-set {
    base objective-function-type;
    status obsolete;
    description
      "Objective function for minimizing the cost on a path set.

       This identity has been obsoleted: the
       'svec-of-minimize-cost-path-set' identity SHOULD
       be used instead.";
    reference
      "RFC 5541: Encoding of Objective Functions in the Path
                 Computation Element Communication Protocol (PCEP)";
  }

  identity path-computation-method {
    description
      "Base identity for supported path computation mechanisms.";
  }

  // CHANGE NOTE: The reference of the identity path-locally-computed
  // below has been updated in this module revision
  // RFC Editor: remove the note above and this note
  identity path-locally-computed {
    base path-computation-method;
    description
      "Indicates a constrained-path LSP in which the
       path is computed by the local LER.";
    reference
      "RFC 9522: Overview and Principles of Internet Traffic
                 Engineering, Section 4.4";
  }

  // CHANGE NOTE: The reference of the identity
  // path-externally-queried below has been updated
  // in this module revision
  // RFC Editor: remove the note above and this note
  identity path-externally-queried {
    base path-computation-method;
    description
      "Constrained-path LSP in which the path is obtained by
       querying an external source, such as a PCE server.
       In the case that an LSP is defined to be externally queried,
       it may also have associated explicit definitions (provided
       to the external source to aid computation).  The path that is
       returned by the external source may require further local
       computation on the device.";
    reference
      "RFC 9522: Overview and Principles of Internet Traffic
                 Engineering
       RFC 4657: Path Computation Element (PCE) Communication
                 Protocol Generic Requirements";
  }

  // CHANGE NOTE: The reference of the identity
  // path-explicitly-defined below has been updated
  // in this module revision
  // RFC Editor: remove the note above and this note
  identity path-explicitly-defined {
    base path-computation-method;
    description
      "Constrained-path LSP in which the path is
       explicitly specified as a collection of strict and/or loose
       hops.";
    reference
      "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels
       RFC 9522: Overview and Principles of Internet Traffic
                 Engineering";
  }

  identity lsp-metric-type {
    description
      "Base identity for the LSP metric specification types.";
  }

  identity lsp-metric-relative {
    base lsp-metric-type;
    description
      "The metric specified for the LSPs to which this identity
       refers is specified as a value relative to the IGP metric
       cost to the LSP's tail end.";
    reference
      "RFC 4657: Path Computation Element (PCE) Communication
                 Protocol Generic Requirements";
  }

  identity lsp-metric-absolute {
    base lsp-metric-type;
    description
      "The metric specified for the LSPs to which this identity
       refers is specified as an absolute value.";
    reference
      "RFC 4657: Path Computation Element (PCE) Communication
                 Protocol Generic Requirements";
  }

  identity lsp-metric-inherited {
    base lsp-metric-type;
    description
      "The metric for the LSPs to which this identity refers is
       not specified explicitly; rather, it is directly inherited
       from the IGP cost.";
    reference
      "RFC 4657: Path Computation Element (PCE) Communication
                 Protocol Generic Requirements";
  }

  identity te-tunnel-type {
    description
      "Base identity from which specific tunnel types are derived.";
  }

  identity te-tunnel-p2p {
    base te-tunnel-type;
    description
      "TE Point-to-Point (P2P) tunnel type.";
    reference
      "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels";
  }

  identity te-tunnel-p2mp {
    base te-tunnel-type;
    description
      "TE P2MP tunnel type.";
    reference
      "RFC 4875: Extensions to Resource Reservation Protocol -
                 Traffic Engineering (RSVP-TE) for
                 Point-to-Multipoint TE Label Switched Paths (LSPs)";
  }

  identity tunnel-action-type {
    description
      "Base identity from which specific tunnel action types
       are derived.";
  }

  identity tunnel-action-resetup {
    base tunnel-action-type;
    description
      "TE tunnel action that tears down the tunnel's current LSP
       (if any) and attempts to re-establish a new LSP.";
  }

  identity tunnel-action-reoptimize {
    base tunnel-action-type;
    description
      "TE tunnel action that reoptimizes the placement of the
       tunnel LSP(s).";
  }

  identity tunnel-action-switchpath {
    base tunnel-action-type;
    description
      "TE tunnel action that switches the tunnel's LSP to use the
       specified path.";
  }

  identity te-action-result {
    description
      "Base identity from which specific TE action results
       are derived.";
  }

  identity te-action-success {
    base te-action-result;
    description
      "TE action was successful.";
  }

  identity te-action-fail {
    base te-action-result;
    description
      "TE action failed.";
  }

  identity tunnel-action-inprogress {
    base te-action-result;
    description
      "TE action is in progress.";
  }

  identity tunnel-admin-state-type {
    description
      "Base identity for TE tunnel administrative states.";
  }

  identity tunnel-admin-state-up {
    base tunnel-admin-state-type;
    description
      "Tunnel's administrative state is up.";
  }

  identity tunnel-admin-state-down {
    base tunnel-admin-state-type;
    description
      "Tunnel's administrative state is down.";
  }

  // CHANGE NOTE: The identity tunnel-admin-state-auto below
  // has been added in this module revision
  // RFC Editor: remove the note above and this note
  identity tunnel-admin-state-auto {
    base tunnel-admin-state-type;
    description
      "Tunnel administrative auto state. The administrative status
       in state datastore transitions to 'tunnel-admin-up' when the
       tunnel used by the client layer, and to 'tunnel-admin-down'
       when it is not used by the client layer.";
  }

  identity tunnel-state-type {
    description
      "Base identity for TE tunnel states.";
  }

  identity tunnel-state-up {
    base tunnel-state-type;
    description
      "Tunnel's state is up.";
  }

  identity tunnel-state-down {
    base tunnel-state-type;
    description
      "Tunnel's state is down.";
  }

  identity lsp-state-type {
    description
      "Base identity for TE LSP states.";
  }

  identity lsp-path-computing {
    base lsp-state-type;
    description
      "State path computation is in progress.";
  }

  identity lsp-path-computation-ok {
    base lsp-state-type;
    description
      "State path computation was successful.";
  }

  identity lsp-path-computation-failed {
    base lsp-state-type;
    description
      "State path computation failed.";
  }

  identity lsp-state-setting-up {
    base lsp-state-type;
    description
      "State is being set up.";
  }

  identity lsp-state-setup-ok {
    base lsp-state-type;
    description
      "State setup was successful.";
  }

  identity lsp-state-setup-failed {
    base lsp-state-type;
    description
      "State setup failed.";
  }

  identity lsp-state-up {
    base lsp-state-type;
    description
      "State is up.";
  }

  identity lsp-state-tearing-down {
    base lsp-state-type;
    description
      "State is being torn down.";
  }

  identity lsp-state-down {
    base lsp-state-type;
    description
      "State is down.";
  }

  identity path-invalidation-action-type {
    description
      "Base identity for TE path invalidation action types.";
  }

  identity path-invalidation-action-drop {
    base path-invalidation-action-type;
    description
      "Upon invalidation of the TE tunnel path, the tunnel remains
       valid, but any packet mapped over the tunnel is dropped.";
    reference
      "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels,
                 Section 2.5";
  }

  identity path-invalidation-action-teardown {
    base path-invalidation-action-type;
    description
      "TE path invalidation action teardown.";
    reference
      "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels,
                 Section 2.5";
  }

  identity lsp-restoration-type {
    description
      "Base identity from which LSP restoration types are derived.";
  }

    // CHANGE NOTE: The identity lsp-restoration-restore-none
    // below has been added in this module revision
    // RFC Editor: remove the note above and this note
    identity lsp-restoration-restore-none {
      base lsp-restoration-type;
      description
        "No LSP affected by a failure is restored.";
    }

  identity lsp-restoration-restore-any {
    base lsp-restoration-type;
    description
      "Any LSP affected by a failure is restored.";
  }

  identity lsp-restoration-restore-all {
    base lsp-restoration-type;
    description
      "Affected LSPs are restored after all LSPs of the tunnel are
       broken.";
  }

  identity restoration-scheme-type {
    description
      "Base identity for LSP restoration schemes.";
  }

    // CHANGE NOTE: The identity restoration-scheme-rerouting
    // below has been added in this module revision
    // RFC Editor: remove the note above and this note
    identity restoration-scheme-rerouting {
      base restoration-scheme-type;
      description
        "Restoration LSP is computed after the failure detection.

         This restoration scheme is also known as
         'Full LSP Re-routing.'";
      reference
        "RFC 4427: Recovery (Protection and Restoration) Terminology
                   for Generalized Multi-Protocol Label Switching
                   (GMPLS)";
    }

  identity restoration-scheme-preconfigured {
    base restoration-scheme-type;
    description
      "Restoration LSP is preconfigured prior to the failure.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity restoration-scheme-precomputed {
    base restoration-scheme-type;
    description
      "Restoration LSP is precomputed prior to the failure.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity restoration-scheme-presignaled {
    base restoration-scheme-type;
    description
      "Restoration LSP is presignaled prior to the failure.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity lsp-protection-type {
    description
      "Base identity from which LSP protection types are derived.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  identity lsp-protection-unprotected {
    base lsp-protection-type;
    description
      "'Unprotected' LSP protection type.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  // CHANGE NOTE: The identity lsp-protection-reroute-extra
  // below has been obsoleted in this module revision
  // RFC Editor: remove the note above and this note
  identity lsp-protection-reroute-extra {
    base lsp-protection-type;
    status obsolete;
    description
      "'(Full) Rerouting' LSP protection type.

       This identity has been obsoleted: the
       'restoration-scheme-rerouting' identity SHOULD be used
       instead.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  // CHANGE NOTE: The identity lsp-protection-reroute
  // below has been obsoleted in this module revision
  // RFC Editor: remove the note above and this note
  identity lsp-protection-reroute {
    base lsp-protection-type;
    status obsolete;
    description
      "'Rerouting without Extra-Traffic' LSP protection type.

       This identity has been obsoleted: the
       'restoration-scheme-rerouting' identity SHOULD be used
       instead.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  identity lsp-protection-1-for-n {
    base lsp-protection-type;
    description
      "'1:N Protection with Extra-Traffic' LSP protection type.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  identity lsp-protection-1-for-1 {
    base lsp-protection-type;
    description
      "LSP protection '1:1 Protection Type'.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  identity lsp-protection-unidir-1-plus-1 {
    base lsp-protection-type;
    description
      "'1+1 Unidirectional Protection' LSP protection type.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  identity lsp-protection-bidir-1-plus-1 {
    base lsp-protection-type;
    description
      "'1+1 Bidirectional Protection' LSP protection type.";
    reference
      "RFC 4872: RSVP-TE Extensions in Support of End-to-End
                 Generalized Multi-Protocol Label Switching (GMPLS)
                 Recovery";
  }

  identity lsp-protection-extra-traffic {
    base lsp-protection-type;
    description
      "Extra-Traffic LSP protection type.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity lsp-protection-state {
    description
      "Base identity of protection states for reporting purposes.";
  }

  identity normal {
    base lsp-protection-state;
    description
      "Normal state.";
  }

  identity signal-fail-of-protection {
    base lsp-protection-state;
    description
      "The protection transport entity has a signal fail condition
       that is of higher priority than the forced switchover
       command.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity lockout-of-protection {
    base lsp-protection-state;
    description
      "A Loss of Protection (LoP) command is active.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity forced-switch {
    base lsp-protection-state;
    description
      "A forced switchover command is active.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity signal-fail {
    base lsp-protection-state;
    description
      "There is a signal fail condition on either the working path
       or the protection path.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity signal-degrade {
    base lsp-protection-state;
    description
      "There is a signal degrade condition on either the working
       path or the protection path.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity manual-switch {
    base lsp-protection-state;
    description
      "A manual switchover command is active.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity wait-to-restore {
    base lsp-protection-state;
    description
      "A WTR timer is running.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity do-not-revert {
    base lsp-protection-state;
    description
      "A Do Not Revert (DNR) condition is active because of
       non-revertive behavior.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity failure-of-protocol {
    base lsp-protection-state;
    description
      "LSP protection is not working because of a protocol failure
       condition.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity protection-external-commands {
    description
      "Base identity from which protection-related external commands
       used for troubleshooting purposes are derived.";
  }

  identity action-freeze {
    base protection-external-commands;
    description
      "A temporary configuration action initiated by an operator
       command that prevents any switchover action from being taken
       and, as such, freezes the current state.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity clear-freeze {
    base protection-external-commands;
    description
      "An action that clears the active freeze state.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity action-lockout-of-normal {
    base protection-external-commands;
    description
      "A temporary configuration action initiated by an operator
       command to ensure that the normal traffic is not allowed
       to use the protection transport entity.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity clear-lockout-of-normal {
    base protection-external-commands;
    description
      "An action that clears the active lockout of the
       normal state.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity action-lockout-of-protection {
    base protection-external-commands;
    description
      "A temporary configuration action initiated by an operator
       command to ensure that the protection transport entity is
       temporarily not available to transport a traffic signal
       (either normal or Extra-Traffic).";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity action-forced-switch {
    base protection-external-commands;
    description
      "A switchover action initiated by an operator command to switch
       the Extra-Traffic signal, the normal traffic signal, or the
       null signal to the protection transport entity, unless a
       switchover command of equal or higher priority is in effect.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity action-manual-switch {
    base protection-external-commands;
    description
      "A switchover action initiated by an operator command to switch
       the Extra-Traffic signal, the normal traffic signal, or
       the null signal to the protection transport entity, unless
       a fault condition exists on other transport entities or a
       switchover command of equal or higher priority is in effect.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  // CHANGE NOTE: The description and reference of the
  // identity action-exercise have been updated in this module
  // revision
  // RFC Editor: remove the note above and this note
  identity action-exercise {
    base protection-external-commands;
    description
      "An action that starts testing whether or not Automatic
       Protection Switching (APS) communication is operating
       correctly.  It is of lower priority than any
       other state or command.";
    reference
      "ITU-T G.808.1: Generic protection switching - Linear trail and
                      subnetwork protection - Edition 4.0 (05/2014)";
  }

  identity clear {
    base protection-external-commands;
    description
      "An action that clears the active near-end lockout of a
       protection, forced switchover, manual switchover, WTR state,
       or exercise command.";
    reference
      "RFC 4427: Recovery (Protection and Restoration) Terminology
                 for Generalized Multi-Protocol Label Switching
                 (GMPLS)";
  }

  identity switching-capabilities {
    description
      "Base identity for interface switching capabilities.";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity switching-psc1 {
    base switching-capabilities;
    description
      "Packet-Switch Capable-1 (PSC-1).";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity switching-evpl {
    base switching-capabilities;
    description
      "Ethernet Virtual Private Line (EVPL).";
    reference
      "RFC 6004: Generalized MPLS (GMPLS) Support for Metro Ethernet
                 Forum and G.8011 Ethernet Service Switching";
  }

  identity switching-l2sc {
    base switching-capabilities;
    description
      "Layer-2 Switch Capable (L2SC).";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity switching-tdm {
    base switching-capabilities;
    description
      "Time-Division-Multiplex Capable (TDM).";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity switching-otn {
    base switching-capabilities;
    description
      "OTN-TDM capable.";
    reference
      "RFC 7138: Traffic Engineering Extensions to OSPF for GMPLS
                 Control of Evolving G.709 Optical Transport
                 Networks";
  }

  identity switching-dcsc {
    base switching-capabilities;
    description
      "Data Channel Switching Capable (DCSC).";
    reference
      "RFC 6002: Generalized MPLS (GMPLS) Data Channel
                 Switching Capable (DCSC) and Channel Set Label
                 Extensions";
  }

  identity switching-lsc {
    base switching-capabilities;
    description
      "Lambda-Switch Capable (LSC).";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity switching-fsc {
    base switching-capabilities;
    description
      "Fiber-Switch Capable (FSC).";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity lsp-encoding-types {
    description
      "Base identity for encoding types.";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity lsp-encoding-packet {
    base lsp-encoding-types;
    description
      "Packet LSP encoding.";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity lsp-encoding-ethernet {
    base lsp-encoding-types;
    description
      "Ethernet LSP encoding.";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity lsp-encoding-pdh {
    base lsp-encoding-types;
    description
      "ANSI/ETSI PDH LSP encoding.";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity lsp-encoding-sdh {
    base lsp-encoding-types;
    description
      "SDH ITU-T G.707 / SONET ANSI T1.105 LSP encoding.";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity lsp-encoding-digital-wrapper {
    base lsp-encoding-types;
    description
      "Digital Wrapper LSP encoding.";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity lsp-encoding-lambda {
    base lsp-encoding-types;
    description
      "Lambda (photonic) LSP encoding.";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity lsp-encoding-fiber {
    base lsp-encoding-types;
    description
      "Fiber LSP encoding.";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity lsp-encoding-fiber-channel {
    base lsp-encoding-types;
    description
      "FiberChannel LSP encoding.";
    reference
      "RFC 3471: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Functional Description";
  }

  identity lsp-encoding-oduk {
    base lsp-encoding-types;
    description
      "G.709 ODUk (Digital Path) LSP encoding.";
    reference
      "RFC 4328: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Extensions for G.709 Optical Transport
                 Networks Control";
  }

  identity lsp-encoding-optical-channel {
    base lsp-encoding-types;
    description
      "G.709 Optical Channel LSP encoding.";
    reference
      "RFC 4328: Generalized Multi-Protocol Label Switching (GMPLS)
                 Signaling Extensions for G.709 Optical Transport
                 Networks Control";
  }

  identity lsp-encoding-line {
    base lsp-encoding-types;
    description
      "Line (e.g., 8B/10B) LSP encoding.";
    reference
      "RFC 6004: Generalized MPLS (GMPLS) Support for Metro
                 Ethernet Forum and G.8011 Ethernet Service
                 Switching";
  }

  identity path-signaling-type {
    description
      "Base identity from which specific LSP path setup types
       are derived.";
  }

  identity path-setup-static {
    base path-signaling-type;
    description
      "Static LSP provisioning path setup.";
  }

  identity path-setup-rsvp {
    base path-signaling-type;
    description
      "RSVP-TE signaling path setup.";
    reference
      "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels";
  }

  identity path-setup-sr {
    base path-signaling-type;
    description
      "Segment-routing path setup.";
  }

  identity path-scope-type {
    description
      "Base identity from which specific path scope types are
       derived.";
  }

  identity path-scope-segment {
    base path-scope-type;
    description
      "Path scope segment.";
    reference
      "RFC 4873: GMPLS Segment Recovery";
  }

  identity path-scope-end-to-end {
    base path-scope-type;
    description
      "Path scope end to end.";
    reference
      "RFC 4873: GMPLS Segment Recovery";
  }

  identity route-usage-type {
    description
      "Base identity for route usage.";
  }

  identity route-include-object {
    base route-usage-type;
    description
      "'Include route' object.";
  }

  identity route-exclude-object {
    base route-usage-type;
    description
      "'Exclude route' object.";
    reference
      "RFC 4874: Exclude Routes - Extension to Resource ReserVation
                 Protocol-Traffic Engineering (RSVP-TE)";
  }

  identity route-exclude-srlg {
    base route-usage-type;
    description
      "Excludes SRLGs.";
    reference
      "RFC 4874: Exclude Routes - Extension to Resource ReserVation
                 Protocol-Traffic Engineering (RSVP-TE)";
  }

  // CHANGE NOTE: The path-metric-optimization-type base identity
  // has been added in this module revision
  // RFC Editor: remove the note above and this note
  identity path-metric-optimization-type {
    description
      "Base identity used to define the path metric optimization
       types.";
  }

  // CHANGE NOTE: The link-path-metric-type base identity
  // has been added in this module revision
  // RFC Editor: remove the note above and this note
  identity link-path-metric-type {
    description
      "Base identity used to define the link and the path metric
       types.

       The unit of the path metric value is interpreted in the
       context of the path metric type and the derived identities
       SHOULD describe the unit of the path metric types they
       define.";
  }

    // CHANGE NOTE: The link-metric-type base identity
    // and its derived identities
    // have been added in this module revision
    // RFC Editor: remove the note above and this note
    identity link-metric-type {
      base link-path-metric-type;
      description
        "Base identity for the link metric types.";
    }

      identity link-metric-te {
        base link-metric-type;
        description
          "Traffic Engineering (TE) Link Metric.";
        reference
          "RFC 3630: Traffic Engineering (TE) Extensions to OSPF
                     Version 2, Section 2.5.5
           RFC 5305: IS-IS Extensions for Traffic Engineering,
                     Section 3.7";
      }

      identity link-metric-igp {
        base link-metric-type;
        description
          "Interior Gateway Protocol (IGP) Link Metric.";
        reference
          "RFC 3785: Use of Interior Gateway Protocol (IGP) Metric
                     as a second MPLS Traffic Engineering (TE)
                     Metric";
      }

      identity link-metric-delay-average {
        base link-metric-type;
        description
          "Unidirectional Link Delay, measured in units of
           microseconds.";
        reference
          "RFC 7471: OSPF Traffic Engineering (TE) Metric
                     Extensions, Section 4.1
           RFC 8570: IS-IS Traffic Engineering (TE) Metric
                     Extensions, Section 4.1";
      }

      identity link-metric-delay-minimum {
        base link-metric-type;
        description
          "Minimum unidirectional Link Delay, measured in units of
           microseconds.";
        reference
          "RFC 7471: OSPF Traffic Engineering (TE) Metric
                     Extensions, Section 4.2
           RFC 8570: IS-IS Traffic Engineering (TE) Metric
                     Extensions, Section 4.2";
      }

      identity link-metric-delay-maximum {
        base link-metric-type;
        description
          "Maximum unidirectional Link Delay, measured in units of
           microseconds.";
        reference
          "RFC 7471: OSPF Traffic Engineering (TE) Metric
                     Extensions, Section 4.2
           RFC 8570: IS-IS Traffic Engineering (TE) Metric
                     Extensions, Section 4.2";
      }

      identity link-metric-residual-bandwidth {
        base link-metric-type;
        description
          "Unidirectional Residual Bandwidth, measured in units of
           bytes per second.

           It is defined to be Maximum Bandwidth minus the bandwidth
           currently allocated to LSPs.";
        reference
          "RFC 7471: OSPF Traffic Engineering (TE) Metric
                     Extensions, Section 4.5
           RFC 8570: IS-IS Traffic Engineering (TE) Metric
                     Extensions, Section 4.5";
      }

    // CHANGE NOTE: The base and the description of the
    // path-metric-type identity
    // has been updated in this module revision
    // RFC Editor: remove the note above and this note
    identity path-metric-type {
      base link-path-metric-type;
      base path-metric-optimization-type;
      description
        "Base identity for the path metric types.";
    }

      // CHANGE NOTE: The description and the reference of the
      // path-metric-te identity have been updated
      // in this module revision
      // RFC Editor: remove the note above and this note
      identity path-metric-te {
        base path-metric-type;
        description
          "Traffic Engineering (TE) Path Metric.";
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
                     Protocol (PCEP), Section 7.8";
      }

      // CHANGE NOTE: The description and the reference of the
      // path-metric-igp identity have been updated
      // in this module revision
      // RFC Editor: remove the note above and this note
      identity path-metric-igp {
        base path-metric-type;
        description
          "Interior Gateway Protocol (IGP) Path Metric.";
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
                     Protocol (PCEP), section 7.8";
      }

      // CHANGE NOTE: The description and the reference of the
      // path-metric-hop identity have been updated
      // in this module revision
      // RFC Editor: remove the note above and this note
      identity path-metric-hop {
        base path-metric-type;
        description
          "Hop Count Path Metric.";
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
                     Protocol (PCEP), Section 7.8";
      }

      // CHANGE NOTE: The description and the reference of the
      // path-metric-delay-average identity have been updated
      // in this module revision
      // RFC Editor: remove the note above and this note
      identity path-metric-delay-average {
        base path-metric-type;
        description
          "The Path Delay Metric, measured in units of
           microseconds.";
        reference
          "RFC8233: Extensions to the Path Computation Element
                    Communication Protocol (PCEP) to Compute
                    Service-Aware Label Switched Paths (LSPs),
                    Section 3.1.1";
      }

      // CHANGE NOTE: The description and the reference of the
      // path-metric-delay-minimum identity have been updated
      // in this module revision
      // RFC Editor: remove the note above and this note
      identity path-metric-delay-minimum {
        base path-metric-type;
        description
          "The Path Min Delay Metric, measured in units of
           microseconds.";
        reference
          "RFC YYYY: Carrying SR-Algorithm information in PCE-based
                     Networks, Section 3.5.1";
      }
      // RFC Editor: replace YYYY with actual RFC number assigned to
      // [I-D.ietf-pce-sid-algo] and remove this note

      // CHANGE NOTE: The description and the reference of the
      // path-metric-residual-bandwidth identity have been updated
      // in this module revision
      // RFC Editor: remove the note above and this note
      identity path-metric-residual-bandwidth {
        base path-metric-type;
        description
          "The Path Residual Bandwidth, defined as the minimum Link
           Residual Bandwidth all the links along the path.

           The Path Residual Bandwidth can be seen as the path
           metric associated with the Maximum residual Bandwidth Path
           (MBP) objective function.";
        reference
          "RFC 5541: Encoding of Objective Functions in the Path
                     Computation Element Communication Protocol
                     (PCEP)";
      }

    // CHANGE NOTE: The base of the path-metric-optimize-includes
    // identity has been updated in this module revision
    // RFC Editor: remove the note above and this note
    identity path-metric-optimize-includes {
      base path-metric-optimization-type;
      description
        "A metric that optimizes the number of included resources
         specified in a set.";
    }

    // CHANGE NOTE: The base of the path-metric-optimize-excludes
    // identity has been updated in this module revision
    // RFC Editor: remove the note above and this note
    identity path-metric-optimize-excludes {
      base path-metric-optimization-type;
      description
        "A metric that optimizes to a maximum the number of excluded
         resources specified in a set.";
    }

  identity path-tiebreaker-type {
    description
      "Base identity for the path tiebreaker type.";
  }

  identity path-tiebreaker-minfill {
    base path-tiebreaker-type;
    description
      "Min-Fill LSP path placement: selects the path with the most
       available bandwidth (load balance LSPs over more links).";
  }

  identity path-tiebreaker-maxfill {
    base path-tiebreaker-type;
    description
      "Max-Fill LSP path placement: selects the path with the least
       available bandwidth (packing more LSPs over few links).";
  }

  identity path-tiebreaker-random {
    base path-tiebreaker-type;
    description
      "Random LSP path placement.";
  }

  identity resource-affinities-type {
    description
      "Base identity for resource class affinities.";
    reference
      "RFC 2702: Requirements for Traffic Engineering Over MPLS";
  }

  identity resource-aff-include-all {
    base resource-affinities-type;
    description
      "The set of attribute filters associated with a
       tunnel, all of which must be present for a link
       to be acceptable.";
    reference
      "RFC 2702: Requirements for Traffic Engineering Over MPLS
       RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels";
  }

  identity resource-aff-include-any {
    base resource-affinities-type;
    description
      "The set of attribute filters associated with a
       tunnel, any of which must be present for a link
       to be acceptable.";
    reference
      "RFC 2702: Requirements for Traffic Engineering Over MPLS
       RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels";
  }

  identity resource-aff-exclude-any {
    base resource-affinities-type;
    description
      "The set of attribute filters associated with a
       tunnel, any of which renders a link unacceptable.";
    reference
      "RFC 2702: Requirements for Traffic Engineering Over MPLS
       RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels";
  }

  // CHANGE NOTE: The reference of the identity
  // te-optimization-criterion below has been updated
  // in this module revision
  // RFC Editor: remove the note above and this note
  identity te-optimization-criterion {
    description
      "Base identity for the TE optimization criteria.";
    reference
      "RFC 9522: Overview and Principles of Internet Traffic
                 Engineering";
  }

  identity not-optimized {
    base te-optimization-criterion;
    description
      "Optimization is not applied.";
  }

  identity cost {
    base te-optimization-criterion;
    description
      "Optimized on cost.";
    reference
      "RFC 5541: Encoding of Objective Functions in the Path
                 Computation Element Communication Protocol (PCEP)";
  }

  identity delay {
    base te-optimization-criterion;
    description
      "Optimized on delay.";
    reference
      "RFC 5541: Encoding of Objective Functions in the Path
                 Computation Element Communication Protocol (PCEP)";
  }

  identity path-computation-srlg-type {
    description
      "Base identity for SRLG path computation.";
  }

  identity srlg-ignore {
    base path-computation-srlg-type;
    description
      "Ignores SRLGs in the path computation.";
  }

  identity srlg-strict {
    base path-computation-srlg-type;
    description
      "Includes a strict SRLG check in the path computation.";
  }

  identity srlg-preferred {
    base path-computation-srlg-type;
    description
      "Includes a preferred SRLG check in the path computation.";
  }

  identity srlg-weighted {
    base path-computation-srlg-type;
    description
      "Includes a weighted SRLG check in the path computation.";
  }

  // CHANGE NOTE: The base identity path-computation-error-reason
  // and its derived identities below have been
  // added in this module revision
  // RFC Editor: remove the note above and this note
  identity path-computation-error-reason {
    description
      "Base identity for path computation error reasons.";
  }

    identity path-computation-error-path-not-found {
      base path-computation-error-reason;
      description
        "Path computation has failed because of an unspecified
         reason.";
      reference
        "RFC 5440: Path Computation Element (PCE) Communication
                   Protocol (PCEP), Section 7.5";
    }

    identity path-computation-error-no-topology {
      base path-computation-error-reason;
      description
        "Path computation has failed because there is no topology
         with the provided topology-identifier.";
    }

    identity path-computation-error-no-dependent-server {
      base path-computation-error-reason;
      description
        "Path computation has failed because one or more dependent
         path computation servers are unavailable.

         The dependent path computation server could be
         a Backward-Recursive Path Computation (BRPC) downstream
         PCE or a child PCE.";
      reference
        "RFC 5441: A Backward-Recursive PCE-Based Computation (BRPC)
                   Procedure to Compute Shortest Constrained
                   Inter-Domain Traffic Engineering Label Switched
                   Paths
         RFC 8685: Path Computation Element Communication Protocol
                   (PCEP) Extensions for the Hierarchical Path
                   Computation Element (H-PCE) Architecture";
    }

    identity path-computation-error-pce-unavailable {
      base path-computation-error-reason;
      description
        "Path computation has failed because PCE is not available.

         It corresponds to bit 31 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 5440: Path Computation Element (PCE) Communication
                   Protocol (PCEP)

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-no-inclusion-hop {
      base path-computation-error-reason;
      description
        "Path computation has failed because there is no
         node or link provided by one or more inclusion hops.";
    }

    identity path-computation-error-destination-unknown-in-domain {
      base path-computation-error-reason;
      description
        "Path computation has failed because the destination node is
         unknown in indicated destination domain.

         It corresponds to bit 19 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 8685: Path Computation Element Communication Protocol
                   (PCEP) Extensions for the Hierarchical Path
                   Computation Element (H-PCE) Architecture

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-no-resource {
      base path-computation-error-reason;
      description
        "Path computation has failed because there is no
         available resource in one or more domains.

         It corresponds to bit 20 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 8685: Path Computation Element Communication Protocol
                   (PCEP) Extensions for the Hierarchical Path
                   Computation Element (H-PCE) Architecture

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-child-pce-unresponsive {
      base path-computation-error-no-dependent-server;
      description
        "Path computation has failed because child PCE is not
         responsive.

         It corresponds to bit 21 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 8685: Path Computation Element Communication Protocol
                   (PCEP) Extensions for the Hierarchical Path
                   Computation Element (H-PCE) Architecture

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-destination-domain-unknown {
      base path-computation-error-reason;
      description
        "Path computation has failed because the destination domain
         was unknown.

         It corresponds to bit 22 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 8685: Path Computation Element Communication Protocol
                   (PCEP) Extensions for the Hierarchical Path
                   Computation Element (H-PCE) Architecture

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-p2mp {
      base path-computation-error-reason;
      description
        "Path computation has failed because of P2MP reachability
         problem.

         It corresponds to bit 24 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 8306: Extensions to the Path Computation Element
                   Communication Protocol (PCEP) for
                   Point-to-Multipoint Traffic Engineering Label
                   Switched Paths

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-no-gco-migration {
      base path-computation-error-reason;
      description
        "Path computation has failed because of no Global Concurrent
         Optimization (GCO) migration path found.

         It corresponds to bit 26 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 5557: Path Computation Element Communication Protocol
                   (PCEP) Requirements and Protocol Extensions in
                   Support of Global Concurrent Optimization

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-no-gco-solution {
      base path-computation-error-reason;
      description
        "Path computation has failed because of no GCO solution
         found.

         It corresponds to bit 25 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 5557: Path Computation Element Communication Protocol
                   (PCEP) Requirements and Protocol Extensions in
                   Support of Global Concurrent Optimization

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-pks-expansion {
      base path-computation-error-reason;
      description
        "Path computation has failed because of Path-Key Subobject
         (PKS)  expansion failure.

         It corresponds to bit 27 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 5520: Preserving Topology Confidentiality in
                   Inter-Domain Path Computation Using a
                   Path-Key-Based Mechanism

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-brpc-chain-unavailable {
      base path-computation-error-no-dependent-server;
      description
        "Path computation has failed because PCE BRPC chain
         unavailable.

         It corresponds to bit 28 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 5441: A Backward-Recursive PCE-Based Computation (BRPC)
                   Procedure to Compute Shortest Constrained
                   Inter-Domain Traffic Engineering Label Switched
                   Paths

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-source-unknown {
      base path-computation-error-reason;
      description
        "Path computation has failed because source node is
         unknown.

         It corresponds to bit 29 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 5440: Path Computation Element (PCE) Communication
                   Protocol (PCEP);

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-destination-unknown {
      base path-computation-error-reason;
      description
        "Path computation has failed because destination node is
         unknown.

         It corresponds to bit 30 of the Flags field of the
         NO-PATH-VECTOR TLV.";
      reference
        "RFC 5440: Path Computation Element (PCE) Communication
        Protocol (PCEP);

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

    identity path-computation-error-no-server {
      base path-computation-error-reason;
      description
        "Path computation has failed because path computation
         server is unavailable.";
      reference
        "RFC 5440: Path Computation Element (PCE) Communication
                   Protocol (PCEP);

         https://www.iana.org/assignments/pcep
         /pcep.xhtml#no-path-vector-tlv";
    }

  // CHANGE NOTE: The base identity protocol-origin-type and
  // its derived identities below have been
  // added in this module revision
  // RFC Editor: remove the note above and this note
  identity protocol-origin-type {
    description
      "Base identity for protocol origin type.";
  }

    identity protocol-origin-api {
      base protocol-origin-type;
      description
        "Protocol origin is via Application Programming Interface
         (API).";
    }

    identity protocol-origin-pcep {
      base protocol-origin-type;
      description
        "Protocol origin is Path Computation Engine Protocol
         (PCEP).";
      reference
        "RFC 5440: Path Computation Element (PCE) Communication
                   Protocol (PCEP)";
    }

    identity protocol-origin-bgp {
      base protocol-origin-type;
      description
        "Protocol origin is Border Gateway Protocol (BGP).";
      reference
        "RFC 9012: The BGP Tunnel Encapsulation Attribute";
    }

  // CHANGE NOTE: The base identity svec-objective-function-type
  // and its derived identities below have been
  // added in this module revision
  // RFC Editor: remove the note above and this note
  identity svec-objective-function-type {
    description
      "Base identity for SVEC objective function type.";
    reference
      "RFC 5541: Encoding of Objective Functions in the Path
                 Computation Element Communication Protocol (PCEP)";
  }

    identity svec-of-minimize-agg-bandwidth-consumption {
      base svec-objective-function-type;
      description
        "Objective function for minimizing aggregate bandwidth
         consumption (MBC).";
      reference
        "RFC 5541: Encoding of Objective Functions in the Path
                   Computation Element Communication Protocol
                   (PCEP)";
    }

    identity svec-of-minimize-load-most-loaded-link {
      base svec-objective-function-type;
      description
        "Objective function for minimizing the load on the link that
         is carrying the highest load (MLL).";
      reference
        "RFC 5541: Encoding of Objective Functions in the Path
                   Computation Element Communication Protocol
                   (PCEP)";
    }

    identity svec-of-minimize-cost-path-set {
      base svec-objective-function-type;
      description
        "Objective function for minimizing the cost on a path set
         (MCC).";
      reference
        "RFC 5541: Encoding of Objective Functions in the Path
                   Computation Element Communication Protocol
                   (PCEP)";
    }

    identity svec-of-minimize-common-transit-domain {
      base svec-objective-function-type;
      description
        "Objective function for minimizing the number of common
         transit domains (MCTD).";
      reference
        "RFC 8685: Path Computation Element Communication Protocol
                   (PCEP) Extensions for the Hierarchical Path
                   Computation Element (H-PCE) Architecture.";
    }

    identity svec-of-minimize-shared-link {
      base svec-objective-function-type;
      description
        "Objective function for minimizing the number of shared
         links (MSL).";
      reference
        "RFC 8685: Path Computation Element Communication Protocol
                   (PCEP) Extensions for the Hierarchical Path
                   Computation Element (H-PCE) Architecture.";
    }

    identity svec-of-minimize-shared-srlg {
      base svec-objective-function-type;
      description
        "Objective function for minimizing the number of shared
         Shared Risk Link Groups (SRLG) (MSS).";
      reference
        "RFC 8685: Path Computation Element Communication Protocol
                   (PCEP) Extensions for the Hierarchical Path
                   Computation Element (H-PCE) Architecture.";
    }

    identity svec-of-minimize-shared-nodes {
      base svec-objective-function-type;
      description
        "Objective function for minimizing the number of shared
         nodes (MSN).";
      reference
        "RFC 8685: Path Computation Element Communication Protocol
                   (PCEP) Extensions for the Hierarchical Path
                   Computation Element (H-PCE) Architecture.";
    }

  // CHANGE NOTE: The base identity svec-metric-type and
  // its derived identities below have been
  // added in this module revision
  // RFC Editor: remove the note above and this note
  identity svec-metric-type {
    description
      "Base identity for SVEC metric type.";
    reference
      "RFC 5541: Encoding of Objective Functions in the Path
                 Computation Element Communication Protocol (PCEP)";
  }

    identity svec-metric-cumulative-te {
      base svec-metric-type;
      description
        "Cumulative TE cost.";
      reference
        "RFC 5541: Encoding of Objective Functions in the Path
                   Computation Element Communication Protocol
                   (PCEP)";
    }

    identity svec-metric-cumulative-igp {
      base svec-metric-type;
      description
        "Cumulative IGP cost.";
      reference
        "RFC 5541: Encoding of Objective Functions in the Path
                   Computation Element Communication Protocol
                   (PCEP)";
    }

    identity svec-metric-cumulative-hop {
      base svec-metric-type;
      description
        "Cumulative Hop path metric.";
      reference
        "RFC 5541: Encoding of Objective Functions in the Path
                   Computation Element Communication Protocol
                   (PCEP)";
    }

    identity svec-metric-aggregate-bandwidth-consumption {
      base svec-metric-type;
      description
        "Aggregate bandwidth consumption.";
      reference
        "RFC 5541: Encoding of Objective Functions in the Path
                   Computation Element Communication Protocol
                   (PCEP)";
    }

    identity svec-metric-load-of-the-most-loaded-link {
      base svec-metric-type;
      description
        "Load of the most loaded link.";
      reference
        "RFC 5541: Encoding of Objective Functions in the Path
                   Computation Element Communication Protocol
                   (PCEP)";
    }

  /**
   * TE bandwidth groupings
   **/

  grouping te-bandwidth {
    description
      "This grouping defines the generic TE bandwidth.
       For some known data-plane technologies, specific modeling
       structures are specified.  The string-encoded 'te-bandwidth'
       type is used for unspecified technologies.
       The modeling structure can be augmented later for other
       technologies.";
    container te-bandwidth {
      description
        "Container that specifies TE bandwidth.  The choices
         can be augmented for specific data-plane technologies.";
      choice technology {
        default "generic";
        description
          "Data-plane technology type.";
        case generic {
          leaf generic {
            type te-bandwidth;
            description
              "Bandwidth specified in a generic format.";
          }
        }
      }
    }
  }

  /**
   * TE label groupings
   **/

  grouping te-label {
    description
      "This grouping defines the generic TE label.
       The modeling structure can be augmented for each technology.
       For unspecified technologies, 'rt-types:generalized-label'
       is used.";
    container te-label {
      description
        "Container that specifies the TE label.  The choices can
         be augmented for specific data-plane technologies.";
      choice technology {
        default "generic";
        description
          "Data-plane technology type.";
        case generic {
          leaf generic {
            type rt-types:generalized-label;
            description
              "TE label specified in a generic format.";
          }
        }
      }
      leaf direction {
        type te-label-direction;
        default "forward";
        description
          "Label direction.";
      }
    }
  }

  grouping te-topology-identifier {
    description
      "Augmentation for a TE topology.";
    container te-topology-identifier {
      description
        "TE topology identifier container.";
      leaf provider-id {
        type te-global-id;
        default "0";
        description
          "An identifier to uniquely identify a provider.
           If omitted, it assumes that the topology provider ID
           value = 0 (the default).";
      }
      leaf client-id {
        type te-global-id;
        default "0";
        description
          "An identifier to uniquely identify a client.
           If omitted, it assumes that the topology client ID
           value = 0 (the default).";
      }
      leaf topology-id {
        type te-topology-id;
        default "";
        description
          "When the datastore contains several topologies,
           'topology-id' distinguishes between them.  If omitted,
           the default (empty) string for this leaf is assumed.";
      }
    }
  }

  /**
   * TE performance metrics groupings
   **/

  grouping performance-metrics-one-way-delay-loss {
    description
      "Performance Metrics (PM) information in real time that can
       be applicable to links or connections.  PM defined in this
       grouping are applicable to generic TE PM as well as packet TE
       PM.";
    reference
      "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions
       RFC 7823: Performance-Based Path Selection for Explicitly
                 Routed Label Switched Paths (LSPs) Using TE Metric
                 Extensions
       RFC 8570: IS-IS Traffic Engineering (TE) Metric Extensions";
    leaf one-way-delay {
      type uint32 {
        range "0..16777215";
      }
      description
        "One-way delay or latency in microseconds.";
    }
    leaf one-way-delay-normality {
      type te-types:performance-metrics-normality;
      description
        "One-way delay normality.";
    }
  }

  grouping performance-metrics-two-way-delay-loss {
    description
      "PM information in real time that can be applicable to links or
       connections.  PM defined in this grouping are applicable to
       generic TE PM as well as packet TE PM.";
    reference
      "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions
       RFC 7823: Performance-Based Path Selection for Explicitly
                 Routed Label Switched Paths (LSPs) Using TE Metric
                 Extensions
       RFC 8570: IS-IS Traffic Engineering (TE) Metric Extensions";
    leaf two-way-delay {
      type uint32 {
        range "0..16777215";
      }
      description
        "Two-way delay or latency in microseconds.";
    }
    leaf two-way-delay-normality {
      type te-types:performance-metrics-normality;
      description
        "Two-way delay normality.";
    }
  }

  grouping performance-metrics-one-way-bandwidth {
    description
      "PM information in real time that can be applicable to links.
       PM defined in this grouping are applicable to generic TE PM
       as well as packet TE PM.";
    reference
      "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions
       RFC 7823: Performance-Based Path Selection for Explicitly
                 Routed Label Switched Paths (LSPs) Using TE Metric
                 Extensions
       RFC 8570: IS-IS Traffic Engineering (TE) Metric Extensions";
    leaf one-way-residual-bandwidth {
      type rt-types:bandwidth-ieee-float32;
      units "bytes per second";
      default "0x0p0";
      description
        "Residual bandwidth that subtracts tunnel reservations from
         Maximum Bandwidth (or link capacity) (RFC 3630) and
         provides an aggregated remainder across QoS classes.";
      reference
        "RFC 3630: Traffic Engineering (TE) Extensions to OSPF
                   Version 2";
    }
    leaf one-way-residual-bandwidth-normality {
      type te-types:performance-metrics-normality;
      default "normal";
      description
        "Residual bandwidth normality.";
    }
    leaf one-way-available-bandwidth {
      type rt-types:bandwidth-ieee-float32;
      units "bytes per second";
      default "0x0p0";
      description
        "Available bandwidth that is defined to be residual
         bandwidth minus the measured bandwidth used for the
         actual forwarding of non-RSVP-TE LSP packets.  For a
         bundled link, available bandwidth is defined to be the
         sum of the component link available bandwidths.";
    }
    leaf one-way-available-bandwidth-normality {
      type te-types:performance-metrics-normality;
      default "normal";
      description
        "Available bandwidth normality.";
    }
    leaf one-way-utilized-bandwidth {
      type rt-types:bandwidth-ieee-float32;
      units "bytes per second";
      default "0x0p0";
      description
        "Bandwidth utilization that represents the actual
         utilization of the link (i.e., as measured in the router).
         For a bundled link, bandwidth utilization is defined to
         be the sum of the component link bandwidth utilizations.";
    }
    leaf one-way-utilized-bandwidth-normality {
      type te-types:performance-metrics-normality;
      default "normal";
      description
        "Bandwidth utilization normality.";
    }
  }

  grouping one-way-performance-metrics {
    description
      "One-way PM throttle grouping.";
    leaf one-way-delay {
      type uint32 {
        range "0..16777215";
      }
      default "0";
      description
        "One-way delay or latency in microseconds.";
    }
    leaf one-way-residual-bandwidth {
      type rt-types:bandwidth-ieee-float32;
      units "bytes per second";
      default "0x0p0";
      description
        "Residual bandwidth that subtracts tunnel reservations from
         Maximum Bandwidth (or link capacity) (RFC 3630) and
         provides an aggregated remainder across QoS classes.";
      reference
        "RFC 3630: Traffic Engineering (TE) Extensions to OSPF
                   Version 2";
    }
    leaf one-way-available-bandwidth {
      type rt-types:bandwidth-ieee-float32;
      units "bytes per second";
      default "0x0p0";
      description
        "Available bandwidth that is defined to be residual
         bandwidth minus the measured bandwidth used for the
         actual forwarding of non-RSVP-TE LSP packets.  For a
         bundled link, available bandwidth is defined to be the
         sum of the component link available bandwidths.";
    }
    leaf one-way-utilized-bandwidth {
      type rt-types:bandwidth-ieee-float32;
      units "bytes per second";
      default "0x0p0";
      description
        "Bandwidth utilization that represents the actual
         utilization of the link (i.e., as measured in the router).
         For a bundled link, bandwidth utilization is defined to
         be the sum of the component link bandwidth utilizations.";
    }
  }

  grouping two-way-performance-metrics {
    description
      "Two-way PM throttle grouping.";
    leaf two-way-delay {
      type uint32 {
        range "0..16777215";
      }
      default "0";
      description
        "Two-way delay or latency in microseconds.";
    }
  }

  grouping performance-metrics-thresholds {
    description
      "Grouping for configurable thresholds for measured
       attributes.";
    uses one-way-performance-metrics;
    uses two-way-performance-metrics;
  }

  grouping performance-metrics-attributes {
    description
      "Contains PM attributes.";
    container performance-metrics-one-way {
      description
        "One-way link performance information in real time.";
      reference
        "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions
         RFC 7823: Performance-Based Path Selection for Explicitly
                   Routed Label Switched Paths (LSPs) Using TE Metric
                   Extensions
         RFC 8570: IS-IS Traffic Engineering (TE) Metric Extensions";
      uses performance-metrics-one-way-delay-loss;
      uses performance-metrics-one-way-bandwidth;
    }
    container performance-metrics-two-way {
      description
        "Two-way link performance information in real time.";
      reference
        "RFC 6374: Packet Loss and Delay Measurement for MPLS
                   Networks";
      uses performance-metrics-two-way-delay-loss;
    }
  }

  grouping performance-metrics-throttle-container {
    description
      "Controls PM throttling.";
    container throttle {
      must 'suppression-interval >= measure-interval' {
        error-message "'suppression-interval' cannot be less than "
                    + "'measure-interval'.";
        description
          "Constraint on 'suppression-interval' and
           'measure-interval'.";
      }
      description
        "Link performance information in real time.";
      reference
        "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions
         RFC 7823: Performance-Based Path Selection for Explicitly
                   Routed Label Switched Paths (LSPs) Using TE Metric
                   Extensions
         RFC 8570: IS-IS Traffic Engineering (TE) Metric Extensions";
      leaf one-way-delay-offset {
        type uint32 {
          range "0..16777215";
        }
        default "0";
        description
          "Offset value to be added to the measured delay value.";
      }
      leaf measure-interval {
        type uint32;
        default "30";
        description
          "Interval, in seconds, to measure the extended metric
           values.";
      }
      leaf advertisement-interval {
        type uint32;
        default "0";
        description
          "Interval, in seconds, to advertise the extended metric
           values.";
      }
      leaf suppression-interval {
        type uint32 {
          range "1..max";
        }
        default "120";
        description
          "Interval, in seconds, to suppress advertisement of the
           extended metric values.";
        reference
          "RFC 8570: IS-IS Traffic Engineering (TE) Metric
                     Extensions, Section 6";
      }
      container threshold-out {
        uses performance-metrics-thresholds;
        description
          "If the measured parameter falls outside an upper bound
           for all but the minimum-delay metric (or a lower bound
           for the minimum-delay metric only) and the advertised
           value is not already outside that bound, an 'anomalous'
           announcement (anomalous bit set) will be triggered.";
      }
      container threshold-in {
        uses performance-metrics-thresholds;
        description
          "If the measured parameter falls inside an upper bound
           for all but the minimum-delay metric (or a lower bound
           for the minimum-delay metric only) and the advertised
           value is not already inside that bound, a 'normal'
           announcement (anomalous bit cleared) will be triggered.";
      }
      container threshold-accelerated-advertisement {
        description
          "When the difference between the last advertised value and
           the current measured value exceeds this threshold, an
           'anomalous' announcement (anomalous bit set) will be
           triggered.";
        uses performance-metrics-thresholds;
      }
    }
  }

  /**
   * TE tunnel generic groupings
   **/

  // CHANGE NOTE: The explicit-route-hop grouping below has been
  // updated in this module revision
  // RFC Editor: remove the note above and this note
  grouping explicit-route-hop {
    description
      "The explicit route entry grouping.";
    choice type {
      description
        "The explicit route entry type.";
      case numbered-node-hop {
        container numbered-node-hop {
          must "node-id-uri or node-id" {
            description
              "At least one node identifier MUST be present.";
          }
          leaf node-id-uri {
            type nw:node-id;
            description
              "The identifier of a node in the topology.";
          }
          leaf node-id {
            type te-node-id;
            description
              "The identifier of a node in the TE topology.";
          }
          leaf hop-type {
            type te-hop-type;
            default "strict";
            description
              "Strict or loose hop.";
          }
          description
            "Numbered node route hop.";
          reference
            "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels,
                       Section 4.3, EXPLICIT_ROUTE in RSVP-TE
             RFC 3477: Signalling Unnumbered Links in Resource
                       ReSerVation Protocol - Traffic Engineering
                       (RSVP-TE)";
        }
      }
      case numbered-link-hop {
        container numbered-link-hop {
          leaf link-tp-id {
            type te-tp-id;
            mandatory true;
            description
              "TE Link Termination Point (LTP) identifier.";
          }
          leaf hop-type {
            type te-hop-type;
            default "strict";
            description
              "Strict or loose hop.";
          }
          leaf direction {
            type te-link-direction;
            default "outgoing";
            description
              "Link route object direction.";
          }
          description
            "Numbered link explicit route hop.";
          reference
            "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels,
                       Section 4.3, EXPLICIT_ROUTE in RSVP-TE
             RFC 3477: Signalling Unnumbered Links in Resource
                       ReSerVation Protocol - Traffic Engineering
                       (RSVP-TE)";
        }
      }
      case unnumbered-link-hop {
        container unnumbered-link-hop {
          must "(link-tp-id-uri or link-tp-id) and " +
                "(node-id-uri or node-id)" {
            description
              "At least one node identifier and at least one Link
              Termination Point (LTP) identifier MUST be present.";
          }
          leaf link-tp-id-uri {
            type nt:tp-id;
            description
              "Link Termination Point (LTP) identifier.";
          }
          leaf link-tp-id {
            type te-tp-id;
            description
              "TE LTP identifier.  The combination of the TE link ID
               and the TE node ID is used to identify an unnumbered
               TE link.";
          }
          leaf node-id-uri {
            type nw:node-id;
            description
              "The identifier of a node in the topology.";
          }
          leaf node-id {
            type te-node-id;
            description
              "The identifier of a node in the TE topology.";
          }
          leaf hop-type {
            type te-hop-type;
            default "strict";
            description
              "Strict or loose hop.";
          }
          leaf direction {
            type te-link-direction;
            default "outgoing";
            description
              "Link route object direction.";
          }
          description
            "Unnumbered link explicit route hop.";
          reference
            "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels,
                       Section 4.3, EXPLICIT_ROUTE in RSVP-TE
             RFC 3477: Signalling Unnumbered Links in Resource
                       ReSerVation Protocol - Traffic Engineering
                       (RSVP-TE)";
        }
      }
      case as-number {
        container as-number-hop {
          leaf as-number {
            type inet:as-number;
            mandatory true;
            description
              "The Autonomous System (AS) number.";
          }
          leaf hop-type {
            type te-hop-type;
            default "strict";
            description
              "Strict or loose hop.";
          }
          description
            "AS explicit route hop.";
        }
      }
      case label {
        container label-hop {
          description
            "Label hop type.";
          uses te-label;
        }
        description
          "The label explicit route hop type.";
      }
    }
  }

  // CHANGE NOTE: The explicit-route-hop grouping below has been
  // updated in this module revision
  // RFC Editor: remove the note above and this note
  grouping record-route-state {
    description
      "The Record Route grouping.";
    leaf index {
      type uint32;
      description
        "Record Route hop index.  The index is used to
         identify an entry in the list.  The order of entries
         is defined by the user without relying on key values.";
    }
    choice type {
      description
        "The Record Route entry type.";
      case numbered-node-hop {
        container numbered-node-hop {
          must "node-id-uri or node-id" {
            description
              "At least one node identifier MUST be present.";
          }
          description
            "Numbered node route hop container.";
          leaf node-id-uri {
            type nw:node-id;
            description
              "The identifier of a node in the topology.";
          }
          leaf node-id {
            type te-node-id;
            description
              "The identifier of a node in the TE topology.";
          }
          leaf-list flags {
            type path-attribute-flags;
            description
              "Path attributes flags.";
            reference
              "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels
               RFC 4090: Fast Reroute Extensions to RSVP-TE for LSP
                         Tunnels
               RFC 4561: Definition of a Record Route Object (RRO)
                         Node-Id Sub-Object";
          }
        }
        description
          "Numbered node route hop.";
      }
      case numbered-link-hop {
        container numbered-link-hop {
          description
            "Numbered link route hop container.";
          leaf link-tp-id {
            type te-tp-id;
            mandatory true;
            description
              "Numbered TE LTP identifier.";
          }
          leaf-list flags {
            type path-attribute-flags;
            description
              "Path attributes flags.";
            reference
              "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels
               RFC 4090: Fast Reroute Extensions to RSVP-TE for LSP
                         Tunnels
               RFC 4561: Definition of a Record Route Object (RRO)
                         Node-Id Sub-Object";
          }
        }
        description
          "Numbered link route hop.";
      }
      case unnumbered-link-hop {
        container unnumbered-link-hop {
          must "(link-tp-id-uri or link-tp-id) and " +
              "(node-id-uri or node-id)" {
            description
              "At least one node identifier and at least one Link
              Termination Point (LTP) identifier MUST be present.";
          }
          leaf link-tp-id-uri {
            type nt:tp-id;
            description
              "Link Termination Point (LTP) identifier.";
          }
          leaf link-tp-id {
            type te-tp-id;
            description
              "TE LTP identifier.  The combination of the TE link ID
               and the TE node ID is used to identify an unnumbered
               TE link.";
          }
          leaf node-id-uri {
            type nw:node-id;
            description
              "The identifier of a node in the topology.";
          }
          leaf node-id {
            type te-node-id;
            description
              "The identifier of a node in the TE topology.";
          }
          leaf-list flags {
            type path-attribute-flags;
            description
              "Path attributes flags.";
            reference
              "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels
               RFC 4090: Fast Reroute Extensions to RSVP-TE for LSP
                         Tunnels
               RFC 4561: Definition of a Record Route Object (RRO)
                         Node-Id Sub-Object";
          }
          description
            "Unnumbered link Record Route hop.";
          reference
            "RFC 3477: Signalling Unnumbered Links in Resource
                       ReSerVation Protocol - Traffic Engineering
                       (RSVP-TE)";
        }
        description
          "Unnumbered link route hop.";
      }
      case label {
        container label-hop {
          description
            "Label route hop type.";
          uses te-label;
          leaf-list flags {
            type path-attribute-flags;
            description
              "Path attributes flags.";
            reference
              "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels
               RFC 4090: Fast Reroute Extensions to RSVP-TE for LSP
                         Tunnels
               RFC 4561: Definition of a Record Route Object (RRO)
                         Node-Id Sub-Object";
          }
        }
        description
          "The label Record Route entry types.";
      }
    }
  }

  grouping label-restriction-info {
    description
      "Label set item information.";
    leaf restriction {
      type enumeration {
        enum inclusive {
          description
            "The label or label range is inclusive.";
        }
        enum exclusive {
          description
            "The label or label range is exclusive.";
        }
      }
      default "inclusive";
      description
        "Indicates whether the list item is inclusive or exclusive.";
    }
    leaf index {
      type uint32;
      description
        "The index of the label restriction list entry.";
    }
    container label-start {
      must "(not(../label-end/te-label/direction) and"
         + " not(te-label/direction))"
         + " or "
         + "(../label-end/te-label/direction = te-label/direction)"
         + " or "
         + "(not(te-label/direction) and"
         + " (../label-end/te-label/direction = 'forward'))"
         + " or "
         + "(not(../label-end/te-label/direction) and"
         + " (te-label/direction = 'forward'))" {
        error-message "'label-start' and 'label-end' must have the "
                    + "same direction.";
      }
      description
        "This is the starting label if a label range is specified.
         This is the label value if a single label is specified,
         in which case the 'label-end' attribute is not set.";
      uses te-label;
    }
    container label-end {
      must "(not(../label-start/te-label/direction) and"
         + " not(te-label/direction))"
         + " or "
         + "(../label-start/te-label/direction = te-label/direction)"
         + " or "
         + "(not(te-label/direction) and"
         + " (../label-start/te-label/direction = 'forward'))"
         + " or "
         + "(not(../label-start/te-label/direction) and"
         + " (te-label/direction = 'forward'))" {
        error-message "'label-start' and 'label-end' must have the "
                    + "same direction.";
      }
      description
        "This is the ending label if a label range is specified.
         This attribute is not set if a single label is specified.";
      uses te-label;
    }
    container label-step {
      description
        "The step increment between labels in the label range.
         The label start/end values will have to be consistent
         with the sign of label step.  For example,
         'label-start' < 'label-end' enforces 'label-step' > 0
         'label-start' > 'label-end' enforces 'label-step' < 0.";
      choice technology {
        default "generic";
        description
          "Data-plane technology type.";
        case generic {
          leaf generic {
            type int32;
            default "1";
            description
              "Label range step.";
          }
        }
      }
    }
    leaf range-bitmap {
      type yang:hex-string;
      description
        "When there are gaps between 'label-start' and 'label-end',
         this attribute is used to specify the positions
         of the used labels.  This is represented in big endian as
         'hex-string'.

         In case the restriction is 'inclusive', the bit-position is
         set if the corresponding mapped label is available.
         In this case, if the range-bitmap is not present, all the
         labels in the range are available.

         In case the restriction is 'exclusive', the bit-position is
         set if the corresponding mapped label is not available.
         In this case, if the range-bitmap is not present, all the
         labels in the range are not available.

         The most significant byte in the hex-string is the farthest
         to the left in the byte sequence.  Leading zero bytes in the
         configured value may be omitted for brevity.
         Each bit position in the 'range-bitmap' 'hex-string' maps
         to a label in the range derived from 'label-start'.

         For example, assuming that 'label-start' = 16000 and
         'range-bitmap' = 0x01000001, then:

         - bit position (0) is set, and the corresponding mapped
           label from the range is 16000 + (0 * 'label-step') or
           16000 for default 'label-step' = 1.
         - bit position (24) is set, and the corresponding mapped
           label from the range is 16000 + (24 * 'label-step') or
           16024 for default 'label-step' = 1.";
    }
  }

  grouping label-set-info {
    description
      "Grouping for the list of label restrictions specifying what
       labels may or may not be used.";
    container label-restrictions {
      description
        "The label restrictions container.";
      list label-restriction {
        key "index";
        description
          "The absence of the label restrictions container implies
           that all labels are acceptable; otherwise, only restricted
           labels are available.";
        reference
          "RFC 7579: General Network Element Constraint Encoding
                     for GMPLS-Controlled Networks";
        uses label-restriction-info;
      }
    }
  }

  // CHANGE NOTE: The grouping optimization-metric-entry below has
  // been updated in this module revision
  // RFC Editor: remove the note above and this note
  grouping optimization-metric-entry {
    description
      "Optimization metrics configuration grouping.";
    leaf metric-type {
      type identityref {
        base path-metric-optimization-type;
      }
      description
        "Identifies the 'metric-type' that the path computation
         process uses for optimization.";
    }
    leaf weight {
      type uint8;
      default "1";
      description
        "TE path metric normalization weight.";
    }
    container explicit-route-exclude-objects {
      when "../metric-type = "
         + "'te-types:path-metric-optimize-excludes'";
      description
        "Container for the 'exclude route' object list.";
      uses path-route-exclude-objects;
    }
    container explicit-route-include-objects {
      when "../metric-type = "
         + "'te-types:path-metric-optimize-includes'";
      description
        "Container for the 'include route' object list.";
      uses path-route-include-objects;
    }
  }

  grouping common-constraints {
    description
      "Common constraints grouping that can be set on
       a constraint set or directly on the tunnel.";
    uses te-bandwidth {
      description
        "A requested bandwidth to use for path computation.";
    }
    leaf link-protection {
      type identityref {
        base link-protection-type;
      }
      default "te-types:link-protection-unprotected";
      description
        "Link protection type required for the links included
         in the computed path.";
      reference
        "RFC 4202: Routing Extensions in Support of
                   Generalized Multi-Protocol Label Switching
                   (GMPLS)";
    }
    leaf setup-priority {
      type uint8 {
        range "0..7";
      }
      default "7";
      description
        "TE LSP requested setup priority.";
      reference
        "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels";
    }
    leaf hold-priority {
      type uint8 {
        range "0..7";
      }
      default "7";
      description
        "TE LSP requested hold priority.";
      reference
        "RFC 3209: RSVP-TE: Extensions to RSVP for LSP Tunnels";
    }
    leaf signaling-type {
      type identityref {
        base path-signaling-type;
      }
      default "te-types:path-setup-rsvp";
      description
        "TE tunnel path signaling type.";
    }
  }

  // CHANGE NOTE: The grouping tunnel-constraints below has
  // been updated in this module revision
  // RFC Editor: remove the note above and this note
  grouping tunnel-constraints {
    description
      "Tunnel constraints grouping that can be set on
       a constraint set or directly on the tunnel.";
    leaf network-id {
      type nw:network-id;
      description
        "The network topology identifier.";
    }
    uses te-topology-identifier;
    uses common-constraints;
  }

  // CHANGE NOTE: The grouping path-constraints-route-objects below
  // has been updated in this module revision
  // RFC Editor: remove the note above and this note
  grouping path-constraints-route-objects {
    description
      "List of route entries to be included or excluded when
       performing the path computation.";
    container explicit-route-objects {
      description
        "Container for the explicit route object lists.";
      list route-object-exclude-always {
        key "index";
        ordered-by user;
        description
          "List of route objects to always exclude from the path
           computation.";
        leaf index {
          type uint32;
          description
            "Explicit Route Object index.  The index is used to
             identify an entry in the list.  The order of entries
             is defined by the user without relying on key values.";
        }
        uses explicit-route-hop;
      }
      list route-object-include-exclude {
        key "index";
        ordered-by user;
        description
          "List of route objects to include or exclude in the path
           computation.";
        leaf explicit-route-usage {
          type identityref {
            base route-usage-type;
          }
          default "te-types:route-include-object";
          description
            "Indicates whether to include or exclude the
             route object.  The default is to include it.";
        }
        leaf index {
          type uint32;
          description
            "Route object include-exclude index.  The index is used
             to identify an entry in the list.  The order of entries
             is defined by the user without relying on key values.";
        }
        uses explicit-route-hop {
          augment "type" {
            case srlg {
              container srlg {
                description
                  "SRLG container.";
                leaf srlg {
                  type uint32;
                  description
                    "SRLG value.";
                }
              }
              description
                "An SRLG value to be included or excluded.";
            }
            description
              "Augmentation for a generic explicit route for SRLG
               exclusion.";
          }
        }
      }
    }
  }

  grouping path-route-include-objects {
    description
      "List of route objects to be included when performing
       the path computation.";
    list route-object-include-object {
      key "index";
      ordered-by user;
      description
        "List of Explicit Route Objects to be included in the
         path computation.";
      leaf index {
        type uint32;
        description
          "Route object entry index.  The index is used to
           identify an entry in the list.  The order of entries
           is defined by the user without relying on key values.";
      }
      uses explicit-route-hop;
    }
  }

  grouping path-route-exclude-objects {
    description
      "List of route objects to be excluded when performing
       the path computation.";
    list route-object-exclude-object {
      key "index";
      ordered-by user;
      description
        "List of Explicit Route Objects to be excluded in the
         path computation.";
      leaf index {
        type uint32;
        description
          "Route object entry index.  The index is used to
           identify an entry in the list.  The order of entries
           is defined by the user without relying on key values.";
      }
      uses explicit-route-hop {
        augment "type" {
          case srlg {
            container srlg {
              description
                "SRLG container.";
              leaf srlg {
                type uint32;
                description
                  "SRLG value.";
              }
            }
            description
              "An SRLG value to be included or excluded.";
          }
          description
            "Augmentation for a generic explicit route for SRLG
             exclusion.";
        }
      }
    }
  }

  // CHANGE NOTE: The grouping generic-path-metric-bounds below
  // has been updated in this module revision
  // RFC Editor: remove the note above and this note
  grouping generic-path-metric-bounds {
    description
      "TE path metric bounds grouping.";
    container path-metric-bounds {
      description
        "Top-level container for the list of path metric bounds.";
      list path-metric-bound {
        key "metric-type";
        description
          "List of path metric bounds, which can apply to link and
           path metrics.

           TE paths which have at least one path metric which
           exceeds the specified bounds MUST NOT be selected.

           TE paths that traverse TE links which have at least one
           link metric which exceeds the specified bounds MUST NOT
           be selected.";
        leaf metric-type {
          type identityref {
            base link-path-metric-type;
          }
          description
            "Identifies an entry in the list of 'metric-type' items
             bound for the TE path.";
        }
        leaf upper-bound {
          type uint64;
          default "0";
          description
            "Upper bound on the specified 'metric-type'.

             A zero indicates an unbounded upper limit for the
             specificied 'metric-type'.

             The unit of is interpreted in the context of the
             'metric-type' identity.";
        }
      }
    }
  }

  // CHANGE NOTE: The grouping generic-path-metric-bounds below
  // has been updated in this module revision
  // RFC Editor: remove the note above and this note
  grouping generic-path-optimization {
    description
      "TE generic path optimization grouping.";
    container optimizations {
      description
        "The objective function container that includes
         attributes to impose when computing a TE path.";
      choice algorithm {
        description
          "Optimizations algorithm.";
        case metric {
          if-feature "path-optimization-metric";
          /* Optimize by metric */
          list optimization-metric {
            key "metric-type";
            description
              "TE path metric type.";
            uses optimization-metric-entry;
          }
          /* Tiebreakers */
          container tiebreakers {
            status deprecated;
            description
              "Container for the list of tiebreakers.

               This container has been deprecated by the tiebreaker
               leaf.";
            list tiebreaker {
              key "tiebreaker-type";
              status deprecated;
              description
                "The list of tiebreaker criteria to apply on an
                 equally favored set of paths, in order to pick
                 the best.";
              leaf tiebreaker-type {
                type identityref {
                  base path-metric-type;
                }
                status deprecated;
                description
                  "Identifies an entry in the list of tiebreakers.";
              }
            }
          }
        }
        case objective-function {
          if-feature "path-optimization-objective-function";
          /* Objective functions */
          container objective-function {
            description
              "The objective function container that includes
               attributes to impose when computing a TE path.";
            leaf objective-function-type {
              type identityref {
                base objective-function-type;
              }
              default "te-types:of-minimize-cost-path";
              description
                "Objective function entry.";
            }
          }
        }
      }
    }
    leaf tiebreaker {
      type identityref {
        base path-tiebreaker-type;
      }
      default "te-types:path-tiebreaker-random";
      description
        "The tiebreaker criteria to apply on an equally favored set
         of paths, in order to pick the best.";
    }
  }

  grouping generic-path-affinities {
    description
      "Path affinities grouping.";
    container path-affinities-values {
      description
        "Path affinities represented as values.";
      list path-affinities-value {
        key "usage";
        description
          "List of named affinity constraints.";
        leaf usage {
          type identityref {
            base resource-affinities-type;
          }
          description
            "Identifies an entry in the list of value affinity
             constraints.";
        }
        leaf value {
          type admin-groups;
          default "";
          description
            "The affinity value.  The default is empty.";
        }
      }
    }
    container path-affinity-names {
      description
        "Path affinities represented as names.";
      list path-affinity-name {
        key "usage";
        description
          "List of named affinity constraints.";
        leaf usage {
          type identityref {
            base resource-affinities-type;
          }
          description
            "Identifies an entry in the list of named affinity
             constraints.";
        }
        list affinity-name {
          key "name";
          leaf name {
            type string;
            description
              "Identifies a named affinity entry.";
          }
          description
            "List of named affinities.";
        }
      }
    }
  }

  grouping generic-path-srlgs {
    description
      "Path SRLG grouping.";
    container path-srlgs-lists {
      description
        "Path SRLG properties container.";
      list path-srlgs-list {
        key "usage";
        description
          "List of SRLG values to be included or excluded.";
        leaf usage {
          type identityref {
            base route-usage-type;
          }
          description
            "Identifies an entry in a list of SRLGs to either
             include or exclude.";
        }
        leaf-list values {
          type srlg;
          description
            "List of SRLG values.";
        }
      }
    }
    container path-srlgs-names {
      description
        "Container for the list of named SRLGs.";
      list path-srlgs-name {
        key "usage";
        description
          "List of named SRLGs to be included or excluded.";
        leaf usage {
          type identityref {
            base route-usage-type;
          }
          description
            "Identifies an entry in a list of named SRLGs to either
             include or exclude.";
        }
        leaf-list names {
          type string;
          description
            "List of named SRLGs.";
        }
      }
    }
  }

  grouping generic-path-disjointness {
    description
      "Path disjointness grouping.";
    leaf disjointness {
      type te-path-disjointness;
      description
        "The type of resource disjointness.
         When configured for a primary path, the disjointness level
         applies to all secondary LSPs.  When configured for a
         secondary path, the disjointness level overrides the level
         configured for the primary path.";
    }
  }

  grouping common-path-constraints-attributes {
    description
      "Common path constraints configuration grouping.";
    uses common-constraints;
    uses generic-path-metric-bounds;
    uses generic-path-affinities;
    uses generic-path-srlgs;
  }

  grouping generic-path-constraints {
    description
      "Global named path constraints configuration grouping.";
    container path-constraints {
      description
        "TE named path constraints container.";
      uses common-path-constraints-attributes;
      uses generic-path-disjointness;
    }
  }

  grouping generic-path-properties {
    description
      "TE generic path properties grouping.";
    container path-properties {
      config false;
      description
        "The TE path properties.";
      list path-metric {
        key "metric-type";
        description
          "TE path metric type.";
        leaf metric-type {
          type identityref {
            base path-metric-type;
          }
          description
            "TE path metric type.";
        }
        leaf accumulative-value {
          type uint64;
          description
            "TE path metric accumulative value.";
        }
      }
      uses generic-path-affinities;
      uses generic-path-srlgs;
      container path-route-objects {
        description
          "Container for the list of route objects either returned by
           the computation engine or actually used by an LSP.";
        list path-route-object {
          key "index";
          ordered-by user;
          description
            "List of route objects either returned by the computation
             engine or actually used by an LSP.";
          leaf index {
            type uint32;
            description
              "Route object entry index.  The index is used to
               identify an entry in the list.  The order of entries
               is defined by the user without relying on key
               values.";
          }
          uses explicit-route-hop;
        }
      }
    }
  }

  // NOTE: The grouping encoding-and-switching-type below has been
  // added in this module revision
  // RFC Editor: remove the note above and this note
  grouping encoding-and-switching-type {
    description
      "Common grouping to define the LSP encoding and
       switching types";
    leaf encoding {
      type identityref {
        base te-types:lsp-encoding-types;
      }
      description
        "LSP encoding type.";
      reference
        "RFC 3945: Generalized Multi-Protocol Label Switching (GMPLS)
                   Architecture";
    }
    leaf switching-type {
      type identityref {
        base te-types:switching-capabilities;
      }
      description
        "LSP switching type.";
      reference
        "RFC 3945: Generalized Multi-Protocol Label Switching (GMPLS)
                   Architecture";
    }
  }

  // CHANGE NOTE: The typedef te-gen-node-id below has been
  // added in this module revision
  // RFC Editor: remove the note above and this note
  grouping te-generic-node-id {
    description
      "A reusable grouping for a TE generic node identifier.";
    leaf id {
      type te-gen-node-id;
      description
        "The identifier of the node. Can be represented as IP
         address or dotted quad address or as an URI.";
    }
    leaf type {
      type enumeration {
        enum ip {
          description
            "IP address representation of the node identifier.";
        }
        enum te-id {
          description
            "TE identifier of the node";
        }
        enum node-id {
          description
            "URI representation of the node identifier.";
        }
      }
      description
        "Type of node identifier representation.";
    }
  }
}

Packet TE Types YANG Module
The "ietf-te-packet-types" module imports from the "ietf-te-types" module defined in Section 4 of this document.
- CHANGE NOTE: Please focus your review only on the updates to the YANG model: see also Appendix A.1.

Packet TE Types YANG module

module ietf-te-packet-types {
  yang-version 1.1;
  namespace "urn:ietf:params:xml:ns:yang:ietf-te-packet-types";
  prefix te-packet-types;

  import ietf-yang-types {
    prefix yang;
    reference
      "RFC 6991: Common YANG Data Types";
  }

  import ietf-te-types {
    prefix te-types;
    reference
      "RFC XXXX: Common YANG Data Types for Traffic Engineering";
  }
  // RFC Editor: replace XXXX with actual RFC number
  // and remove this note

  organization
    "IETF Traffic Engineering Architecture and Signaling (TEAS)
     Working Group";
  contact
    "WG Web:   <https://datatracker.ietf.org/wg/teas/>
     WG List:  <mailto:teas@ietf.org>

     Editor:   Tarek Saad
               <mailto:tsaad.net@gmail.com>

     Editor:   Rakesh Gandhi
               <mailto:rgandhi@cisco.com>

     Editor:   Vishnu Pavan Beeram
               <mailto:vbeeram@juniper.net>

     Editor:   Xufeng Liu
               <mailto:xufeng.liu.ietf@gmail.com>

     Editor:   Igor Bryskin
               <mailto:i_bryskin@yahoo.com>";
  description
    "This YANG module contains a collection of generally useful YANG
     data type definitions specific to Packet Traffic Enginnering
     (TE).

     The model fully conforms to the Network Management Datastore
     Architecture (NMDA).

     The key words 'MUST', 'MUST NOT', 'REQUIRED', 'SHALL', 'SHALL
     NOT', 'SHOULD', 'SHOULD NOT', 'RECOMMENDED', 'NOT RECOMMENDED',
     'MAY', and 'OPTIONAL' in this document are to be interpreted as
     described in BCP 14 (RFC 2119) (RFC 8174) when, and only when,
     they appear in all capitals, as shown here.

     Copyright (c) 2024 IETF Trust and the persons identified as
     authors of the code.  All rights reserved.

     Redistribution and use in source and binary forms, with or
     without modification, is permitted pursuant to, and subject to
     the license terms contained in, the Revised BSD License set
     forth in Section 4.c of the IETF Trust's Legal Provisions
     Relating to IETF Documents
     (https://trustee.ietf.org/license-info).

     This version of this YANG module is part of RFC XXXX
     (https://www.rfc-editor.org/info/rfcXXXX); see the RFC itself
     for full legal notices.";
  revision 2024-07-23 {
    description
      "This revision adds the following new identities:
       - bandwidth-profile-type;
       - link-metric-delay-variation;
       - link-metric-loss;
       - path-metric-delay-variation;
       - path-metric-loss.

      This revision adds the following new groupings:
       - te-packet-path-bandwidth;
       - te-packet-link-bandwidth.

      This revision provides also few editorial changes.";
    reference
      "RFC XXXX: Common YANG Data Types for Traffic Engineering";
  }
  // RFC Editor: replace XXXX with actual RFC number, update date
  // information and remove this note

  revision 2020-06-10 {
    description
      "Latest revision of TE MPLS types.";
    reference
      "RFC 8776: Common YANG Data Types for Traffic Engineering";
  }

  /*
   * Identities
   */

  // CHANGE NOTE: The base identity bandwidth-profile-type and
  // its derived identities below have been
  // added in this module revision
  // RFC Editor: remove the note above and this note
  identity bandwidth-profile-type {
    description
      "Bandwidth Profile Types";
  }

    identity mef-10 {
      base bandwidth-profile-type;
      description
        "MEF 10 Bandwidth Profile";
      reference
        "MEF 10.3: Ethernet Services Attributes Phase 3";
    }

    identity rfc-2697 {
      base bandwidth-profile-type;
      description
        "RFC 2697 Bandwidth Profile";
      reference
        "RFC 2697: A Single Rate Three Color Marker";
    }

    identity rfc-2698 {
      base bandwidth-profile-type;
      description
        "RFC 2698 Bandwidth Profile";
      reference
        "RFC 2698: A Two Rate Three Color Marker";
    }

    identity rfc-4115 {
      base bandwidth-profile-type;
      description
        "RFC 4115 Bandwidth Profile";
      reference
        "RFC 4115: A Differentiated Service Two-Rate, Three-Color
                   Marker with Efficient Handling of in-Profile
                   Traffic";
    }

    // CHANGE NOTE: The identity link-metric-delay-variation
    // below has been added in this module revision
    // RFC Editor: remove the note above and this note
    identity link-metric-delay-variation {
      base te-types:link-metric-type;
      description
        "The Unidirectional Delay Variation Metric,
         measured in units of microseconds.";
      reference
        "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions,
                   Section 4.3
         RFC 8570: IS-IS Traffic Engineering (TE) Metric Extensions,
                   Section 4.3";
    }

    // CHANGE NOTE: The identity link-metric-loss below has
    // been added in this module revision
    // RFC Editor: remove the note above and this note
    identity link-metric-loss {
      base te-types:link-metric-type;
      description
        "The Unidirectional Link Loss Metric,
         measured in units of 0.000003%.";
      reference
        "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions,
                   Section 4.4
         RFC 8570: IS-IS Traffic Engineering (TE) Metric Extensions,
                   Section 4.4";
    }

    // CHANGE NOTE: The identity path-metric-delay-variation
    // below has been added in this module revision
    // RFC Editor: remove the note above and this note
    identity path-metric-delay-variation {
      base te-types:path-metric-type;
      description
        "The Path Delay Variation Metric,
         measured in units of microseconds.";
      reference
        "RFC 8233: Extensions to the Path Computation Element
                   Communication Protocol (PCEP) to Compute
                   Service-Aware Label Switched Paths (LSPs),
                   Section 3.1.2";
    }

    // CHANGE NOTE: The identity path-metric-loss below has
    // been added in this module revision
    // RFC Editor: remove the note above and this note
    identity path-metric-loss {
      base te-types:path-metric-type;
      description
        "The Path Loss Metric, measured in units of 0.000003%.";
      reference
        "RFC 8233: Extensions to the Path Computation Element
                   Communication Protocol (PCEP) to Compute
                   Service-Aware Label Switched Paths (LSPs),
                   Section 3.1.3";
    }

  /*
   * Typedefs
   */

  typedef te-bandwidth-requested-type {
    type enumeration {
      enum specified {
        description
          "Bandwidth is explicitly specified.";
      }
      enum auto {
        description
          "Bandwidth is automatically computed.";
      }
    }
    description
      "Enumerated type for specifying whether bandwidth is
       explicitly specified or automatically computed.";
  }

  typedef te-class-type {
    type uint8;
    description
      "Diffserv-TE Class-Type.  Defines a set of Traffic Trunks
       crossing a link that is governed by a specific set of
       bandwidth constraints.  Class-Type is used for the purposes
       of link bandwidth allocation, constraint-based routing, and
       admission control.";
    reference
      "RFC 4124: Protocol Extensions for Support of Diffserv-aware
                 MPLS Traffic Engineering";
  }

  typedef bc-type {
    type uint8 {
      range "0..7";
    }
    description
      "Diffserv-TE bandwidth constraints as defined in RFC 4124.";
    reference
      "RFC 4124: Protocol Extensions for Support of Diffserv-aware
                 MPLS Traffic Engineering";
  }

  typedef bandwidth-kbps {
    type uint64;
    units "Kbps";
    description
      "Bandwidth values, expressed in kilobits per second.";
  }

  typedef bandwidth-mbps {
    type uint64;
    units "Mbps";
    description
      "Bandwidth values, expressed in megabits per second.";
  }

  typedef bandwidth-gbps {
    type uint64;
    units "Gbps";
    description
      "Bandwidth values, expressed in gigabits per second.";
  }

  identity backup-protection-type {
    description
      "Base identity for the backup protection type.";
  }

  identity backup-protection-link {
    base backup-protection-type;
    description
      "Backup provides link protection only.";
  }

  identity backup-protection-node-link {
    base backup-protection-type;
    description
      "Backup offers node (preferred) or link protection.";
  }

  identity bc-model-type {
    description
      "Base identity for the Diffserv-TE Bandwidth Constraints
       Model type.";
    reference
      "RFC 4124: Protocol Extensions for Support of Diffserv-aware
                 MPLS Traffic Engineering";
  }

  identity bc-model-rdm {
    base bc-model-type;
    description
      "Russian Dolls Bandwidth Constraints Model type.";
    reference
      "RFC 4127: Russian Dolls Bandwidth Constraints Model for
                 Diffserv-aware MPLS Traffic Engineering";
  }

  identity bc-model-mam {
    base bc-model-type;
    description
      "Maximum Allocation Bandwidth Constraints Model type.";
    reference
      "RFC 4125: Maximum Allocation Bandwidth Constraints Model for
                 Diffserv-aware MPLS Traffic Engineering";
  }

  identity bc-model-mar {
    base bc-model-type;
    description
      "Maximum Allocation with Reservation Bandwidth Constraints
       Model type.";
    reference
      "RFC 4126: Max Allocation with Reservation Bandwidth
                 Constraints Model for Diffserv-aware MPLS Traffic
                 Engineering & Performance Comparisons";
  }

  /*
   * Groupings
   */

  grouping performance-metrics-attributes-packet {
    description
      "Contains PM attributes.";
    uses te-types:performance-metrics-attributes {
      augment "performance-metrics-one-way" {
        leaf one-way-min-delay {
          type uint32 {
            range "0..16777215";
          }
          description
            "One-way minimum delay or latency in microseconds.";
        }
        leaf one-way-min-delay-normality {
          type te-types:performance-metrics-normality;
          default "normal";
          description
            "One-way minimum delay or latency normality.";
        }
        leaf one-way-max-delay {
          type uint32 {
            range "0..16777215";
          }
          description
            "One-way maximum delay or latency in microseconds.";
        }
        leaf one-way-max-delay-normality {
          type te-types:performance-metrics-normality;
          default "normal";
          description
            "One-way maximum delay or latency normality.";
        }
        leaf one-way-delay-variation {
          type uint32 {
            range "0..16777215";
          }
          description
            "One-way delay variation in microseconds.";
          reference
            "RFC 5481: Packet Delay Variation Applicability
                       Statement, Section 4.2";
        }
        leaf one-way-delay-variation-normality {
          type te-types:performance-metrics-normality;
          default "normal";
          description
            "One-way delay variation normality.";
          reference
            "RFC 7471: OSPF Traffic Engineering (TE) Metric
                       Extensions
             RFC 7823: Performance-Based Path Selection for
                       Explicitly Routed Label Switched Paths (LSPs)
                       Using TE Metric Extensions
             RFC 8570: IS-IS Traffic Engineering (TE) Metric
                       Extensions";
        }
        leaf one-way-packet-loss {
          type decimal64 {
            fraction-digits 6;
            range "0..50.331642";
          }
          description
            "One-way packet loss as a percentage of the total traffic
             sent over a configurable interval.  The finest precision
             is 0.000003%, where the maximum is 50.331642%.";
          reference
            "RFC 8570: IS-IS Traffic Engineering (TE) Metric
                       Extensions, Section 4.4";
        }
        leaf one-way-packet-loss-normality {
          type te-types:performance-metrics-normality;
          default "normal";
          description
            "Packet loss normality.";
          reference
            "RFC 7471: OSPF Traffic Engineering (TE) Metric
                       Extensions
             RFC 7823: Performance-Based Path Selection for
                       Explicitly Routed Label Switched Paths (LSPs)
                       Using TE Metric Extensions
             RFC 8570: IS-IS Traffic Engineering (TE) Metric
                       Extensions";
        }
        description
          "PM one-way packet-specific augmentation for a generic PM
           grouping.";
      }
      augment "performance-metrics-two-way" {
        leaf two-way-min-delay {
          type uint32 {
            range "0..16777215";
          }
          default "0";
          description
            "Two-way minimum delay or latency in microseconds.";
        }
        leaf two-way-min-delay-normality {
          type te-types:performance-metrics-normality;
          default "normal";
          description
            "Two-way minimum delay or latency normality.";
          reference
            "RFC 7471: OSPF Traffic Engineering (TE) Metric
                       Extensions
             RFC 7823: Performance-Based Path Selection for
                       Explicitly Routed Label Switched Paths (LSPs)
                       Using TE Metric Extensions
             RFC 8570: IS-IS Traffic Engineering (TE) Metric
                       Extensions";
        }
        leaf two-way-max-delay {
          type uint32 {
            range "0..16777215";
          }
          default "0";
          description
            "Two-way maximum delay or latency in microseconds.";
        }
        leaf two-way-max-delay-normality {
          type te-types:performance-metrics-normality;
          default "normal";
          description
            "Two-way maximum delay or latency normality.";
          reference
            "RFC 7471: OSPF Traffic Engineering (TE) Metric
                       Extensions
             RFC 7823: Performance-Based Path Selection for
                       Explicitly Routed Label Switched Paths (LSPs)
                       Using TE Metric Extensions
             RFC 8570: IS-IS Traffic Engineering (TE) Metric
                       Extensions";
        }
        leaf two-way-delay-variation {
          type uint32 {
            range "0..16777215";
          }
          default "0";
          description
            "Two-way delay variation in microseconds.";
          reference
            "RFC 5481: Packet Delay Variation Applicability
                       Statement, Section 4.2";
        }
        leaf two-way-delay-variation-normality {
          type te-types:performance-metrics-normality;
          default "normal";
          description
            "Two-way delay variation normality.";
          reference
            "RFC 7471: OSPF Traffic Engineering (TE) Metric
                       Extensions
             RFC 7823: Performance-Based Path Selection for
                       Explicitly Routed Label Switched Paths (LSPs)
                       Using TE Metric Extensions
             RFC 8570: IS-IS Traffic Engineering (TE) Metric
                       Extensions";
        }
        leaf two-way-packet-loss {
          type decimal64 {
            fraction-digits 6;
            range "0..50.331642";
          }
          default "0";
          description
            "Two-way packet loss as a percentage of the total traffic
             sent over a configurable interval.  The finest precision
             is 0.000003%.";
        }
        leaf two-way-packet-loss-normality {
          type te-types:performance-metrics-normality;
          default "normal";
          description
            "Two-way packet loss normality.";
        }
        description
          "PM two-way packet-specific augmentation for a generic PM
           grouping.";
        reference
            "RFC 7471: OSPF Traffic Engineering (TE) Metric
                       Extensions
             RFC 7823: Performance-Based Path Selection for
                       Explicitly Routed Label Switched Paths (LSPs)
                       Using TE Metric Extensions
             RFC 8570: IS-IS Traffic Engineering (TE) Metric
                       Extensions";
      }
    }
  }

  grouping one-way-performance-metrics-packet {
    description
      "One-way packet PM throttle grouping.";
    leaf one-way-min-delay {
      type uint32 {
        range "0..16777215";
      }
      default "0";
      description
        "One-way minimum delay or latency in microseconds.";
    }
    leaf one-way-max-delay {
      type uint32 {
        range "0..16777215";
      }
      default "0";
      description
        "One-way maximum delay or latency in microseconds.";
    }
    leaf one-way-delay-variation {
      type uint32 {
        range "0..16777215";
      }
      default "0";
      description
        "One-way delay variation in microseconds.";
    }
    leaf one-way-packet-loss {
      type decimal64 {
        fraction-digits 6;
        range "0..50.331642";
      }
      default "0";
      description
        "One-way packet loss as a percentage of the total traffic
         sent over a configurable interval.  The finest precision is
         0.000003%.";
    }
  }

  // CHANGE NOTE: The grouping
  // one-way-performance-metrics-gauge-packet has been added in
  // this module revision
  // RFC Editor: remove the note above and this note
  grouping one-way-performance-metrics-gauge-packet {
    description
      "One-way packet PM throttle grouping.

       This grouping is used to report the same metrics defined in
       the one-way-performance-metrics-packet grouping, using gauges
       instead of uint32 data types and referencing IPPM RFCs
       instead of IGP-TE RFCs.";
    leaf one-way-min-delay {
      type yang:gauge64;
      description
        "One-way minimum delay or latency in microseconds.";
    }
    leaf one-way-max-delay {
      type yang:gauge64;
      description
        "One-way maximum delay or latency in microseconds.";
      reference
        "RFC 7679: A One-Way Delay Metric for IP Performance
                   Metrics (IPPM)";
    }
    leaf one-way-delay-variation {
      type yang:gauge64;
      description
        "One-way delay variation in microseconds.";
      reference
        "RFC 3393: IP Packet Delay Variation Metric for IP
                   Performance Metrics (IPPM)";
    }
    leaf one-way-packet-loss {
      type decimal64 {
        fraction-digits 5;
        range "0..100";
      }
      description
        "The ratio of packets dropped to packets transmitted between
         two endpoints.";
      reference
        "RFC 7680: A One-Way Loss Metric for IP Performance
                   Metrics (IPPM)";
    }
  }

  grouping two-way-performance-metrics-packet {
    description
      "Two-way packet PM throttle grouping.";
    leaf two-way-min-delay {
      type uint32 {
        range "0..16777215";
      }
      default "0";
      description
        "Two-way minimum delay or latency in microseconds.";
    }
    leaf two-way-max-delay {
      type uint32 {
        range "0..16777215";
      }
      default "0";
      description
        "Two-way maximum delay or latency in microseconds.";
    }
    leaf two-way-delay-variation {
      type uint32 {
        range "0..16777215";
      }
      default "0";
      description
        "Two-way delay variation in microseconds.";
    }
    leaf two-way-packet-loss {
      type decimal64 {
        fraction-digits 6;
        range "0..50.331642";
      }
      default "0";
      description
        "Two-way packet loss as a percentage of the total traffic
         sent over a configurable interval.  The finest precision is
         0.000003%.";
    }
  }

  // CHANGE NOTE: The grouping
  // two-way-performance-metrics-gauge-packet has been added in
  // this module revision
  // RFC Editor: remove the note above and this note
  grouping two-way-performance-metrics-gauge-packet {
    description
      "Two-way packet PM throttle grouping.

       This grouping is used to report the same metrics defined in
       the two-way-performance-metrics-packet grouping, using gauges
       instead of uint32 data types and referencing IPPM RFCs
       instead of IGP-TE RFCs.";
    leaf two-way-min-delay {
      type yang:gauge64;
      description
        "Two-way minimum delay or latency in microseconds.";
      reference
        "RFC 2681: A Round-trip Delay Metric for IPPM";
    }
    leaf two-way-max-delay {
      type yang:gauge64;
      description
        "Two-way maximum delay or latency in microseconds.";
      reference
        "RFC 2681: A Round-trip Delay Metric for IPPM";
    }
    leaf two-way-delay-variation {
      type yang:gauge64;
      description
        "Two-way delay variation in microseconds.";
      reference
        "RFC 5481: Packet Delay Variation Applicability Statement";
    }
    leaf two-way-packet-loss {
      type decimal64 {
        fraction-digits 5;
        range "0..100";
      }
      description
        "The ratio of packets dropped to packets transmitted between
         two endpoints.";
    }
  }

  grouping performance-metrics-throttle-container-packet {
    description
      "Packet PM threshold grouping.";
    uses te-types:performance-metrics-throttle-container {
      augment "throttle/threshold-out" {
        uses one-way-performance-metrics-packet;
        uses two-way-performance-metrics-packet;
        description
          "PM threshold-out packet augmentation for a
           generic grouping.";
      }
      augment "throttle/threshold-in" {
        uses one-way-performance-metrics-packet;
        uses two-way-performance-metrics-packet;
        description
          "PM threshold-in packet augmentation for a
           generic grouping.";
      }
      augment "throttle/threshold-accelerated-advertisement" {
        uses one-way-performance-metrics-packet;
        uses two-way-performance-metrics-packet;
        description
          "PM accelerated advertisement packet augmentation for a
           generic grouping.";
      }
    }
  }

  // CHANGE NOTE: The te-packet-path-bandwidth below has been
  // added in this module revision
  // RFC Editor: remove the note above and this note
  grouping te-packet-path-bandwidth {
    description
      "Path bandwidth for Packet. ";
    leaf bandwidth-profile-name {
      type string;
      description
        "Name of Bandwidth Profile.";
    }
    leaf bandwidth-profile-type {
      type identityref {
        base bandwidth-profile-type;
      }
      description
        "Type of Bandwidth Profile.";
    }
    leaf cir {
      type uint64;
      units "bits/second";
      mandatory true;
      description
        "Committed Information Rate (CIR).";
    }
    leaf cbs {
      type uint64;
      units "bits/second";
      mandatory true;
      description
        "Committed Burst Size (CBS).";
    }
    leaf eir {
      type uint64;
      units "bits/second";
      description
        "Excess Information Rate (EIR).";
    }
    leaf ebs {
      type uint64;
      units "bytes";
      description
        "Excess Burst Size (EBS).";
    }
    leaf pir {
      type uint64;
      units "bits/second";
      description
        "Peak Information Rate (PIR).";
    }
    leaf pbs {
      type uint64;
      units "bytes";
      description
        "Peak Burst Size (PBS).";
    }
  }

  // CHANGE NOTE: The te-packet-path-bandwidth below has been
  // added in this module revision
  // RFC Editor: remove the note above and this note
  grouping te-packet-link-bandwidth {
    description
      "Link Bandwidth for Packet. ";
    leaf packet-bandwidth {
      type uint64;
      units "bits/second";
      description
        "Available bandwith value.";
    }
  }
}

IANA Considerations
This document requests IANA to update the following URIs in the "IETF XML Registry" [RFC3688] to refer to this document:

      URI: urn:ietf:params:xml:ns:yang:ietf-te-types
      Registrant Contact:  The IESG.
      XML: N/A, the requested URI is an XML namespace.

      URI: urn:ietf:params:xml:ns:yang:ietf-te-packet-types
      Registrant Contact:  The IESG.
      XML: N/A, the requested URI is an XML namespace.

This document also requests IANA to update the following YANG modules to the "YANG Module Names" registry [RFC7950]:

      name:      ietf-te-types
      Maintained by IANA?  N
      namespace: urn:ietf:params:xml:ns:yang:ietf-te-types
      prefix:    te-types
      reference: RFC XXXX

      name:      ietf-te-packet-types
      Maintained by IANA?  N
      namespace: urn:ietf:params:xml:ns:yang:ietf-te-packet-types
      prefix:    te-packet-types
      reference: RFC XXXX

Security Considerations
The YANG module specified in this document defines a schema for data that is designed to be accessed via network management protocols such as NETCONF [RFC6241] or RESTCONF [RFC8040]. The lowest NETCONF layer is the secure transport layer, and the mandatory-to-implement secure transport is Secure Shell (SSH) [RFC6242]. The lowest RESTCONF layer is HTTPS, and the mandatory-to-implement secure transport is TLS [RFC8446].
The Network Configuration Access Control Model (NACM) [RFC8341] provides the means to restrict access for particular NETCONF or RESTCONF users to a preconfigured subset of all available NETCONF or RESTCONF protocol operations and content.
The YANG module in this document defines common TE type definitions (e.g., typedef, identity, and grouping statements) in YANG data modeling language to be imported and used by other TE modules. When imported and used, the resultant schema will have data nodes that can be writable or readable. Access to such data nodes may be considered sensitive or vulnerable in some network environments. Write operations (e.g., edit-config) to these data nodes without proper protection can have a negative effect on network operations.

Normative References
[ITU_G.808.1]

Generic protection switching - Linear trail and subnetwork protection
ITU-T Recommendation G.808.1
May 2014
ITU-T Recommendation G.808.1
[MEF_10.3]

Ethernet Services Attributes Phase 3
MEF
October 2013
MEF 10.3
[ITU-T_G.709]

Interfaces for the optical transport network
International Telecommunication Union
June 2020
ITU-T G.709
[RFC6020]

YANG - A Data Modeling Language for the Network Configuration Protocol (NETCONF)
M. Bjorklund, Ed.
October 2010
RFC 6020
DOI 10.17487/RFC6020
[RFC7950]

The YANG 1.1 Data Modeling Language
M. Bjorklund, Ed.
August 2016
RFC 7950
DOI 10.17487/RFC7950
[RFC6241]

Network Configuration Protocol (NETCONF)
R. Enns, Ed.
M. Bjorklund, Ed.
J. Schoenwaelder, Ed.
A. Bierman, Ed.
June 2011
RFC 6241
DOI 10.17487/RFC6241
[RFC8040]

RESTCONF Protocol
A. Bierman
M. Bjorklund
K. Watsen
January 2017
RFC 8040
DOI 10.17487/RFC8040
[RFC8776]

Common YANG Data Types for Traffic Engineering
T. Saad
R. Gandhi
X. Liu
V. Beeram
I. Bryskin
June 2020
RFC 8776
DOI 10.17487/RFC8776
[RFC2119]

Key words for use in RFCs to Indicate Requirement Levels
S. Bradner
March 1997
BCP 14
RFC 2119
DOI 10.17487/RFC2119
[RFC8174]

Ambiguity of Uppercase vs Lowercase in RFC 2119 Key Words
B. Leiba
May 2017
BCP 14
RFC 8174
DOI 10.17487/RFC8174
[RFC6991]

Common YANG Data Types
J. Schoenwaelder, Ed.
July 2013
RFC 6991
DOI 10.17487/RFC6991
[RFC8294]

Common YANG Data Types for the Routing Area
X. Liu
Y. Qu
A. Lindem
C. Hopps
L. Berger
December 2017
RFC 8294
DOI 10.17487/RFC8294
[RFC8345]

A YANG Data Model for Network Topologies
A. Clemm
J. Medved
R. Varga
N. Bahadur
H. Ananthakrishnan
X. Liu
March 2018
RFC 8345
DOI 10.17487/RFC8345
[RFC8800]

Path Computation Element Communication Protocol (PCEP) Extension for Label Switched Path (LSP) Diversity Constraint Signaling
S. Litkowski
S. Sivabalan
C. Barth
M. Negi
July 2020
RFC 8800
DOI 10.17487/RFC8800
[RFC5541]

Encoding of Objective Functions in the Path Computation Element Communication Protocol (PCEP)
JL. Le Roux
JP. Vasseur
Y. Lee
June 2009
RFC 5541
DOI 10.17487/RFC5541
[RFC5440]

Path Computation Element (PCE) Communication Protocol (PCEP)
JP. Vasseur, Ed.
JL. Le Roux, Ed.
March 2009
RFC 5440
DOI 10.17487/RFC5440
[RFC8685]

Path Computation Element Communication Protocol (PCEP) Extensions for the Hierarchical Path Computation Element (H-PCE) Architecture
F. Zhang
Q. Zhao
O. Gonzalez de Dios
R. Casellas
D. King
December 2019
RFC 8685
DOI 10.17487/RFC8685
[RFC5441]

A Backward-Recursive PCE-Based Computation (BRPC) Procedure to Compute Shortest Constrained Inter-Domain Traffic Engineering Label Switched Paths
JP. Vasseur, Ed.
R. Zhang
N. Bitar
JL. Le Roux
April 2009
RFC 5441
DOI 10.17487/RFC5441
[RFC5520]

Preserving Topology Confidentiality in Inter-Domain Path Computation Using a Path-Key-Based Mechanism
R. Bradford, Ed.
JP. Vasseur
A. Farrel
April 2009
RFC 5520
DOI 10.17487/RFC5520
[RFC5557]

Path Computation Element Communication Protocol (PCEP) Requirements and Protocol Extensions in Support of Global Concurrent Optimization
Y. Lee
JL. Le Roux
D. King
E. Oki
July 2009
RFC 5557
DOI 10.17487/RFC5557
[RFC8306]

Extensions to the Path Computation Element Communication Protocol (PCEP) for Point-to-Multipoint Traffic Engineering Label Switched Paths
Q. Zhao
D. Dhody, Ed.
R. Palleti
D. King
November 2017
RFC 8306
DOI 10.17487/RFC8306
[RFC9012]

The BGP Tunnel Encapsulation Attribute
K. Patel
G. Van de Velde
S. Sangli
J. Scudder
April 2021
RFC 9012
DOI 10.17487/RFC9012
[RFC6242]

Using the NETCONF Protocol over Secure Shell (SSH)
M. Wasserman
June 2011
RFC 6242
DOI 10.17487/RFC6242
[RFC8446]

The Transport Layer Security (TLS) Protocol Version 1.3
E. Rescorla
August 2018
RFC 8446
DOI 10.17487/RFC8446
[RFC8341]

Network Configuration Access Control Model
A. Bierman
M. Bjorklund
March 2018
STD 91
RFC 8341
DOI 10.17487/RFC8341

Informative References
[I-D.ietf-netmod-rfc8407bis]

Guidelines for Authors and Reviewers of Documents Containing YANG Data Models
Andy Bierman
YumaWorks
Mohamed Boucadair
Orange
Qin Wu
Huawei
5 July 2024
Internet-Draft draft-ietf-netmod-rfc8407bis-14
[RFC7471]

OSPF Traffic Engineering (TE) Metric Extensions
S. Giacalone
D. Ward
J. Drake
A. Atlas
S. Previdi
March 2015
RFC 7471
DOI 10.17487/RFC7471
[RFC8570]

IS-IS Traffic Engineering (TE) Metric Extensions
L. Ginsberg, Ed.
S. Previdi, Ed.
S. Giacalone
D. Ward
J. Drake
Q. Wu
March 2019
RFC 8570
DOI 10.17487/RFC8570
[RFC7823]

Performance-Based Path Selection for Explicitly Routed Label Switched Paths (LSPs) Using TE Metric Extensions
A. Atlas
J. Drake
S. Giacalone
S. Previdi
May 2016
RFC 7823
DOI 10.17487/RFC7823
[RFC4124]

Protocol Extensions for Support of Diffserv-aware MPLS Traffic Engineering
F. Le Faucheur, Ed.
June 2005
RFC 4124
DOI 10.17487/RFC4124
[RFC6370]

MPLS Transport Profile (MPLS-TP) Identifiers
M. Bocci
G. Swallow
E. Gray
September 2011
RFC 6370
DOI 10.17487/RFC6370
[RFC5003]

Attachment Individual Identifier (AII) Types for Aggregation
C. Metz
L. Martini
F. Balus
J. Sugimoto
September 2007
RFC 5003
DOI 10.17487/RFC5003
[RFC3630]

Traffic Engineering (TE) Extensions to OSPF Version 2
D. Katz
K. Kompella
D. Yeung
September 2003
RFC 3630
DOI 10.17487/RFC3630
[RFC6827]

Automatically Switched Optical Network (ASON) Routing for OSPFv2 Protocols
A. Malis, Ed.
A. Lindem, Ed.
D. Papadimitriou, Ed.
January 2013
RFC 6827
DOI 10.17487/RFC6827
[RFC5305]

IS-IS Extensions for Traffic Engineering
T. Li
H. Smit
October 2008
RFC 5305
DOI 10.17487/RFC5305
[RFC6119]

IPv6 Traffic Engineering in IS-IS
J. Harrison
J. Berger
M. Bartlett
February 2011
RFC 6119
DOI 10.17487/RFC6119
[RFC4872]

RSVP-TE Extensions in Support of End-to-End Generalized Multi-Protocol Label Switching (GMPLS) Recovery
J.P. Lang, Ed.
Y. Rekhter, Ed.
D. Papadimitriou, Ed.
May 2007
RFC 4872
DOI 10.17487/RFC4872
[RFC7308]

Extended Administrative Groups in MPLS Traffic Engineering (MPLS-TE)
E. Osborne
July 2014
RFC 7308
DOI 10.17487/RFC7308
[RFC4203]

OSPF Extensions in Support of Generalized Multi-Protocol Label Switching (GMPLS)
K. Kompella, Ed.
Y. Rekhter, Ed.
October 2005
RFC 4203
DOI 10.17487/RFC4203
[RFC5307]

IS-IS Extensions in Support of Generalized Multi-Protocol Label Switching (GMPLS)
K. Kompella, Ed.
Y. Rekhter, Ed.
October 2008
RFC 5307
DOI 10.17487/RFC5307
[RFC3785]

Use of Interior Gateway Protocol (IGP) Metric as a second MPLS Traffic Engineering (TE) Metric
F. Le Faucheur
R. Uppili
A. Vedrenne
P. Merckx
T. Telkamp
May 2004
BCP 87
RFC 3785
DOI 10.17487/RFC3785
[RFC4427]

Recovery (Protection and Restoration) Terminology for Generalized Multi-Protocol Label Switching (GMPLS)
E. Mannie, Ed.
D. Papadimitriou, Ed.
March 2006
RFC 4427
DOI 10.17487/RFC4427
[RFC6378]

MPLS Transport Profile (MPLS-TP) Linear Protection
Y. Weingarten, Ed.
S. Bryant
E. Osborne
N. Sprecher
A. Fulignoli, Ed.
October 2011
RFC 6378
DOI 10.17487/RFC6378
[RFC3209]

RSVP-TE: Extensions to RSVP for LSP Tunnels
D. Awduche
L. Berger
D. Gan
T. Li
V. Srinivasan
G. Swallow
December 2001
RFC 3209
DOI 10.17487/RFC3209
[RFC4090]

Fast Reroute Extensions to RSVP-TE for LSP Tunnels
P. Pan, Ed.
G. Swallow, Ed.
A. Atlas, Ed.
May 2005
RFC 4090
DOI 10.17487/RFC4090
[RFC4736]

Reoptimization of Multiprotocol Label Switching (MPLS) Traffic Engineering (TE) Loosely Routed Label Switched Path (LSP)
JP. Vasseur, Ed.
Y. Ikejiri
R. Zhang
November 2006
RFC 4736
DOI 10.17487/RFC4736
[RFC5712]

MPLS Traffic Engineering Soft Preemption
M. Meyer, Ed.
JP. Vasseur, Ed.
January 2010
RFC 5712
DOI 10.17487/RFC5712
[RFC4920]

Crankback Signaling Extensions for MPLS and GMPLS RSVP-TE
A. Farrel, Ed.
A. Satyanarayana
A. Iwata
N. Fujita
G. Ash
July 2007
RFC 4920
DOI 10.17487/RFC4920
[RFC5420]

Encoding of Attributes for MPLS LSP Establishment Using Resource Reservation Protocol Traffic Engineering (RSVP-TE)
A. Farrel, Ed.
D. Papadimitriou
JP. Vasseur
A. Ayyangar
February 2009
RFC 5420
DOI 10.17487/RFC5420
[RFC7570]

Label Switched Path (LSP) Attribute in the Explicit Route Object (ERO)
C. Margaria, Ed.
G. Martinelli
S. Balls
B. Wright
July 2015
RFC 7570
DOI 10.17487/RFC7570
[RFC4875]

Extensions to Resource Reservation Protocol - Traffic Engineering (RSVP-TE) for Point-to-Multipoint TE Label Switched Paths (LSPs)
R. Aggarwal, Ed.
D. Papadimitriou, Ed.
S. Yasukawa, Ed.
May 2007
RFC 4875
DOI 10.17487/RFC4875
[RFC5151]

Inter-Domain MPLS and GMPLS Traffic Engineering -- Resource Reservation Protocol-Traffic Engineering (RSVP-TE) Extensions
A. Farrel, Ed.
A. Ayyangar
JP. Vasseur
February 2008
RFC 5151
DOI 10.17487/RFC5151
[RFC5150]

Label Switched Path Stitching with Generalized Multiprotocol Label Switching Traffic Engineering (GMPLS TE)
A. Ayyangar
K. Kompella
JP. Vasseur
A. Farrel
February 2008
RFC 5150
DOI 10.17487/RFC5150
[RFC6001]

Generalized MPLS (GMPLS) Protocol Extensions for Multi-Layer and Multi-Region Networks (MLN/MRN)
D. Papadimitriou
M. Vigoureux
K. Shiomoto
D. Brungard
JL. Le Roux
October 2010
RFC 6001
DOI 10.17487/RFC6001
[RFC6790]

The Use of Entropy Labels in MPLS Forwarding
K. Kompella
J. Drake
S. Amante
W. Henderickx
L. Yong
November 2012
RFC 6790
DOI 10.17487/RFC6790
[RFC7260]

GMPLS RSVP-TE Extensions for Operations, Administration, and Maintenance (OAM) Configuration
A. Takacs
D. Fedyk
J. He
June 2014
RFC 7260
DOI 10.17487/RFC7260
[RFC8001]

RSVP-TE Extensions for Collecting Shared Risk Link Group (SRLG) Information
F. Zhang, Ed.
O. Gonzalez de Dios, Ed.
C. Margaria
M. Hartley
Z. Ali
January 2017
RFC 8001
DOI 10.17487/RFC8001
[RFC8149]

RSVP Extensions for Reoptimization of Loosely Routed Point-to-Multipoint Traffic Engineering Label Switched Paths (LSPs)
T. Saad, Ed.
R. Gandhi, Ed.
Z. Ali
R. Venator
Y. Kamite
April 2017
RFC 8149
DOI 10.17487/RFC8149
[RFC8169]

Residence Time Measurement in MPLS Networks
G. Mirsky
S. Ruffini
E. Gray
J. Drake
S. Bryant
A. Vainshtein
May 2017
RFC 8169
DOI 10.17487/RFC8169
[RFC6780]

RSVP ASSOCIATION Object Extensions
L. Berger
F. Le Faucheur
A. Narayanan
October 2012
RFC 6780
DOI 10.17487/RFC6780
[RFC4873]

GMPLS Segment Recovery
L. Berger
I. Bryskin
D. Papadimitriou
A. Farrel
May 2007
RFC 4873
DOI 10.17487/RFC4873
[RFC3471]

Generalized Multi-Protocol Label Switching (GMPLS) Signaling Functional Description
L. Berger, Ed.
January 2003
RFC 3471
DOI 10.17487/RFC3471
[RFC2702]

Requirements for Traffic Engineering Over MPLS
D. Awduche
J. Malcolm
J. Agogbua
M. O'Dell
J. McManus
September 1999
RFC 2702
DOI 10.17487/RFC2702
[RFC8233]

Extensions to the Path Computation Element Communication Protocol (PCEP) to Compute Service-Aware Label Switched Paths (LSPs)
D. Dhody
Q. Wu
V. Manral
Z. Ali
K. Kumaki
September 2017
RFC 8233
DOI 10.17487/RFC8233
[I-D.ietf-pce-sid-algo]

Carrying SR-Algorithm information in PCE-based Networks.
Samuel Sidor
Cisco Systems, Inc.
Alex Tokar
Cisco Systems, Inc.
Shaofu Peng
ZTE Corporation
Shuping Peng
Huawei Technologies
Andrew Stone
Nokia
23 July 2024
Internet-Draft draft-ietf-pce-sid-algo-12
[RFC3477]

Signalling Unnumbered Links in Resource ReSerVation Protocol - Traffic Engineering (RSVP-TE)
K. Kompella
Y. Rekhter
January 2003
RFC 3477
DOI 10.17487/RFC3477
[RFC4125]

Maximum Allocation Bandwidth Constraints Model for Diffserv-aware MPLS Traffic Engineering
F. Le Faucheur
W. Lai
June 2005
RFC 4125
DOI 10.17487/RFC4125
[RFC4126]

Max Allocation with Reservation Bandwidth Constraints Model for Diffserv-aware MPLS Traffic Engineering & Performance Comparisons
J. Ash
June 2005
RFC 4126
DOI 10.17487/RFC4126
[RFC4127]

Russian Dolls Bandwidth Constraints Model for Diffserv-aware MPLS Traffic Engineering
F. Le Faucheur, Ed.
June 2005
RFC 4127
DOI 10.17487/RFC4127
[RFC2697]

A Single Rate Three Color Marker
J. Heinanen
R. Guerin
September 1999
RFC 2697
DOI 10.17487/RFC2697
[RFC2698]

A Two Rate Three Color Marker
J. Heinanen
R. Guerin
September 1999
RFC 2698
DOI 10.17487/RFC2698
[RFC4115]

A Differentiated Service Two-Rate, Three-Color Marker with Efficient Handling of in-Profile Traffic
O. Aboul-Magd
S. Rabie
July 2005
RFC 4115
DOI 10.17487/RFC4115
[I-D.ietf-teas-yang-te-mpls]

A YANG Data Model for MPLS Traffic Engineering Tunnels
Tarek Saad
Cisco Systems Inc
Rakesh Gandhi
Cisco Systems Inc
Xufeng Liu
IBM Corporation
Vishnu Pavan Beeram
Juniper Networks
Igor Bryskin
Individual
26 May 2023
Internet-Draft draft-ietf-teas-yang-te-mpls-04
[RFC9522]

Overview and Principles of Internet Traffic Engineering
A. Farrel, Ed.
January 2024
RFC 9522
DOI 10.17487/RFC9522
[RFC4202]

Routing Extensions in Support of Generalized Multi-Protocol Label Switching (GMPLS)
K. Kompella, Ed.
Y. Rekhter, Ed.
October 2005
RFC 4202
DOI 10.17487/RFC4202
[RFC4328]

Generalized Multi-Protocol Label Switching (GMPLS) Signaling Extensions for G.709 Optical Transport Networks Control
D. Papadimitriou, Ed.
January 2006
RFC 4328
DOI 10.17487/RFC4328
[RFC4561]

Definition of a Record Route Object (RRO) Node-Id Sub-Object
J.-P. Vasseur, Ed.
Z. Ali
S. Sivabalan
June 2006
RFC 4561
DOI 10.17487/RFC4561
[RFC4657]

Path Computation Element (PCE) Communication Protocol Generic Requirements
J. Ash, Ed.
J.L. Le Roux, Ed.
September 2006
RFC 4657
DOI 10.17487/RFC4657
[RFC6004]

Generalized MPLS (GMPLS) Support for Metro Ethernet Forum and G.8011 Ethernet Service Switching
L. Berger
D. Fedyk
October 2010
RFC 6004
DOI 10.17487/RFC6004
[RFC6511]

Non-Penultimate Hop Popping Behavior and Out-of-Band Mapping for RSVP-TE Label Switched Paths
Z. Ali
G. Swallow
R. Aggarwal
February 2012
RFC 6511
DOI 10.17487/RFC6511
[RFC7139]

GMPLS Signaling Extensions for Control of Evolving G.709 Optical Transport Networks
F. Zhang, Ed.
G. Zhang
S. Belotti
D. Ceccarelli
K. Pithewan
March 2014
RFC 7139
DOI 10.17487/RFC7139
[RFC7551]

RSVP-TE Extensions for Associated Bidirectional Label Switched Paths (LSPs)
F. Zhang, Ed.
R. Jing
R. Gandhi, Ed.
May 2015
RFC 7551
DOI 10.17487/RFC7551
[RFC7571]

GMPLS RSVP-TE Extensions for Lock Instruct and Loopback
J. Dong
M. Chen
Z. Li
D. Ceccarelli
July 2015
RFC 7571
DOI 10.17487/RFC7571
[RFC7579]

General Network Element Constraint Encoding for GMPLS-Controlled Networks
G. Bernstein, Ed.
Y. Lee, Ed.
D. Li
W. Imajuku
J. Han
June 2015
RFC 7579
DOI 10.17487/RFC7579
[RFC3688]

The IETF XML Registry
M. Mealling
January 2004
BCP 81
RFC 3688
DOI 10.17487/RFC3688
[RFC9314]

YANG Data Model for Bidirectional Forwarding Detection (BFD)
M. Jethanandani, Ed.
R. Rahman, Ed.
L. Zheng, Ed.
S. Pallagatti
G. Mirsky
September 2022
RFC 9314
DOI 10.17487/RFC9314
Changes from RFC 8776
This version adds new common data types, identities, and groupings to the YANG modules. It also updates some of the existing data types, identities, and groupings in the YANG modules and fixes few bugs in [RFC8776].
The following new identities have been added to the 'ietf-te-types' module:
- lsp-provisioning-error-reason;
- association-type-diversity;
- tunnel-admin-state-auto;
- lsp-restoration-restore-none;
- restoration-scheme-rerouting;
- path-metric-optimization-type;
- link-path-metric-type;
- link-metric-type and its derived identities;
- path-computation-error-reason and its derived identities;
- protocol-origin-type and its derived identities;
- svec-objective-function-type and its derived identities;
- svec-metric-type and its derived identities.
The following new data types have been added to the 'ietf-te-types' module:
- path-type;
- te-gen-node-id.
The following new groupings have been added to the 'ietf-te-types' module:
- encoding-and-switching-type;
- te-generic-node-id.
The following new identities have been added to the 'ietf-te-packet-types' module:
- bandwidth-profile-type;
- link-metric-delay-variation;
- link-metric-loss;
- path-metric-delay-variation;
- path-metric-loss.
The following new groupings have been added to the 'ietf-te-packet-types' module:
- te-packet-path-bandwidth;
- te-packet-link-bandwidth.
The following identities, already defined in [RFC8776], have been updated in the 'ietf-te-types' module:
- objective-function-type (editorial);
- action-exercise (bug fix);
- path-metric-type:
new base identities have been added;
- path-metric-te (bug fix);
- path-metric-igp (bug fix);
- path-metric-hop (bug fix);
- path-metric-delay-average (bug fix);
- path-metric-delay-minimum (bug fix);
- path-metric-residual-bandwidth (bug fix);
- path-metric-optimize-includes (bug fix);
- path-metric-optimize-excludes (bug fix);
- te-optimization-criterion (editorial).
The following data type, already defined in [RFC8776], has been updated in the 'ietf-te-types' module:
- te-node-id;
The data type has been changed to be a union.
The following groupings, already defined in [RFC8776], have been updated in the 'ietf-te-types' module:
- explicit-route-hop
The following new leaves have been added to the 'explicit-route-hop' grouping:
  - node-id-uri;
  - link-tp-id-uri;
The following leaves, already defined in [RFC8776], have been updated in the 'explicit-route-hop':
  - node-id;
  - link-tp-id.
The mandatory true statements for the node-id and link-tp-id have been replaced by must statements that requires at least the presence of:
    - node-id or node-id-uri;
    - link-tp-id or link-tp-id-uri.
- explicit-route-hop
The following new leaves have been added to the 'explicit-route-hop' grouping:
  - node-id-uri;
  - link-tp-id-uri;
The following leaves, already defined in [RFC8776], have been updated in the 'explicit-route-hop':
  - node-id;
  - link-tp-id.
The mandatory true statements for the node-id and link-tp-id have been replaced by must statements that requires at least the presence of:
    - node-id or node-id-uri;
    - link-tp-id or link-tp-id-uri.
- optimization-metric-entry:
The following leaves, already defined in [RFC8776], have been updated in the 'optimization-metric-entry':
  - metric-type;
The base identity has been updated without impacting the set of derived identities that are allowed.
- tunnel-constraints;
The following new leaf have been added to the 'tunnel-constraints' grouping:
  - network-id;
- path-constraints-route-objects:
The following container, already defined in [RFC8776], has been updated in the 'path-constraints-route-objects':
  - explicit-route-objects-always;
The container has been renamed as 'explicit-route-objects'. This change is not affecting any IETF standard YANG models since this grouping has not yet been used by any YANG model defined in existing IETF RFCs.
- generic-path-metric-bounds:
The following leaves, already defined in [RFC8776], have been updated in the 'optimization-metric-entry':
  - metric-type;
The base identity has been updated to:
    - increase the set of derived identities that are allowed and;
    - remove from this set the 'path-metric-optimize-includes' and the 'path-metric-optimize-excludes' identities (bug fixing)
- generic-path-optimization
The following new leaf have been added to the 'generic-path-optimization' grouping:
  - tiebreaker;
The following container, already defined in [RFC8776], has been deprecated:
  - tiebreakers.
The following identities, already defined in [RFC8776], have been obsoletes in the 'ietf-te-types' module for bug fixing:
- of-minimize-agg-bandwidth-consumption;
- of-minimize-load-most-loaded-link;
- of-minimize-cost-path-set;
- lsp-protection-reroute-extra;
- lsp-protection-reroute.
TE Types YANG Diffs
RFC Editor: please remove this appendix before publication.
This section provides the diff between the YANG module in section 3.1 of [RFC8776] and the YANG model revision in Section 4.
The intention of this appendix is to facilitate focusing the review of the YANG model in Section 4 to the changes compared with the YANG model in [RFC8776].
This diff has been generated using the following UNIX commands to compare the YANG module revisions in section 3.1 of [RFC8776] and in Section 4:

diff ietf-te-types@2020-06-10.yang ietf-te-types.yang
     > model-diff.txt
sed 's/^/    /' model-diff.txt > model-diff-spaces.txt
sed 's/^    >   /    >   /' model-diff-spaces.txt
    > model-updates.txt

The output (model-updates.txt) is reported here:

21a22,33
>   import ietf-network {
>     prefix "nw";
>     reference
>       "RFC 8345: A YANG Data Model for Network Topologies";
>   }
>
>   import ietf-network-topology {
>     prefix "nt";
>     reference
>       "RFC 8345: A YANG Data Model for Network Topologies";
>   }
>
30c42
<                <mailto:tsaad@juniper.net>
---
>                <mailto:tsaad.net@gmail.com>
55c67
<      Copyright (c) 2020 IETF Trust and the persons identified as
---
>      Copyright (c) 2024 IETF Trust and the persons identified as
60c72
<      the license terms contained in, the Simplified BSD License set
---
>      the license terms contained in, the Revised BSD License set
65,66c77,166
<      This version of this YANG module is part of RFC 8776; see the
<      RFC itself for full legal notices.";
---
>      This version of this YANG module is part of RFC XXXX
>      (https://www.rfc-editor.org/info/rfcXXXX); see the RFC itself
>      for full legal notices.";
>   revision 2024-07-23 {
>     description
>       "This revision adds the following new identities:
>       - lsp-provisioning-error-reason;
>       - association-type-diversity;
>       - tunnel-admin-state-auto;
>       - lsp-restoration-restore-none;
>       - restoration-scheme-rerouting;
>       - path-metric-optimization-type;
>       - link-path-metric-type;
>       - link-metric-type and its derived identities;
>       - path-computation-error-reason and its derived identities;
>       - protocol-origin-type and its derived identities;
>       - svec-objective-function-type and its derived identities;
>       - svec-metric-type and its derived identities.
>
>       This revision adds the following new data types:
>       - path-type;
>       - te-gen-node-id.
>
>       This revision adds the following new groupings:
>       - encoding-and-switching-type;
>       - te-generic-node-id.
>
>       This revision updates the following identities:
>       - objective-function-type;
>       - action-exercise;
>       - path-metric-type;
>       - path-metric-te;
>       - path-metric-igp;
>       - path-metric-hop;
>       - path-metric-delay-average;
>       - path-metric-delay-minimum;
>       - path-metric-residual-bandwidth;
>       - path-metric-optimize-includes;
>       - path-metric-optimize-excludes;
>       - te-optimization-criterion.
>
>       This revision updates the following data types:
>       - te-node-id.
>
>       This revision updates the following groupings:
>       - explicit-route-hop:
>         - adds the following leaves:
>           - node-id-uri;
>           - link-tp-id-uri;
>         - updates the following leaves:
>           - node-id;
>           - link-tp-id;
>       - record-route-state:
>         - adds the following leaves:
>           - node-id-uri;
>           - link-tp-id-uri;
>         - updates the following leaves:
>           - node-id;
>           - link-tp-id;
>       - optimization-metric-entry:
>         - updates the following leaves:
>           - metric-type;
>       - tunnel-constraints;
>         - adds the following leaves:
>           - network-id;
>       - path-constraints-route-objects:
>         - updates the following containers:
>           - explicit-route-objects-always;
>       - generic-path-metric-bounds:
>         - updates the following leaves:
>           - metric-type;
>       - generic-path-optimization
>         - adds the following leaves:
>           - tiebreaker;
>         - deprecate the following containers:
>           - tiebreakers.
>
>       This revision obsoletes the following identities:
>       - of-minimize-agg-bandwidth-consumption;
>       - of-minimize-load-most-loaded-link;
>       - of-minimize-cost-path-set;
>       - lsp-protection-reroute-extra;
>       - lsp-protection-reroute.
>
>       This revision provides also few editorial changes.";
>     reference
>       "RFC XXXX: Common YANG Data Types for Traffic Engineering";
>   }
>   // RFC Editor: replace XXXX with actual RFC number, update date
>   // information and remove this note
70c170
<       "Latest revision of TE types.";
---
>       "Initial Version of TE types.";
86a187
>
92c193
<        Version 2
---
>                  Version 2
95c196
<        Engineering (MPLS-TE)";
---
>                  Engineering (MPLS-TE)";
111a213
>
117c219
<        Engineering (MPLS-TE)";
---
>                  Engineering (MPLS-TE)";
157,158c259,260
<        Routed Label Switched Paths (LSPs) Using TE Metric
<        Extensions
---
>                  Routed Label Switched Paths (LSPs) Using TE Metric
>                  Extensions
168c270
<        Multi-Protocol Label Switching (GMPLS)
---
>                  Multi-Protocol Label Switching (GMPLS)
170c272
<        Multi-Protocol Label Switching (GMPLS)";
---
>                  Multi-Protocol Label Switching (GMPLS)";
193c295
<            Traffic Engineering Networks";
---
>                      Traffic Engineering Networks";
244,245c346,347
<        ITU-T Recommendation G.709: Interfaces for the
<        optical transport network";
---
>        ITU-T G.709: Interfaces for the optical transport network -
>                     Edition 6.0 (06/2020)";
256c358
<        MPLS Traffic Engineering, Section 4.3.1";
---
>                  MPLS Traffic Engineering, Section 4.3.1";
263a366
>
264a368
>
269c373
<        Aggregation
---
>                  Aggregation
288c392
<        Section 4.3.3";
---
>                  Section 4.3.3";
306c410
<        Version 2";
---
>                  Version 2";
349c453
<        second MPLS Traffic Engineering (TE) Metric";
---
>                  second MPLS Traffic Engineering (TE) Metric";
351a456,458
>   // CHANGE NOTE: The typedef te-node-id below has been
>   // updated in this module revision
>   // RFC Editor: remove the note above and this note
353c460,463
<     type yang:dotted-quad;
---
>     type union {
>       type yang:dotted-quad;
>       type inet:ipv6-address-no-zone;
>     }
357,358c467,471
<        The identifier is represented as 4 octets in dotted-quad
<        notation.
---
>
>        The identifier is represented either as 4 octets in
>        dotted-quad notation, or as 16 octets in full, mixed,
>        shortened, or shortened-mixed IPv6 address notation.
>
362,363c475,478
<        Router ID TLV described in Section 4.3 of RFC 5305, or the
<        TE Router ID TLV described in Section 3.2.1 of RFC 6119.
---
>        Router ID TLV described in Section 4.3 of RFC 5305, the TE
>        Router ID TLV described in Section 3.2.1 of RFC 6119, or the
>        IPv6 TE Router ID TLV described in Section 4.1 of RFC 6119.
>
368c483
<        Version 2, Section 2.4.1
---
>                  Version 2, Section 2.4.1
370c485
<        Section 4.3
---
>                  Section 4.3
373c488
<        Routing for OSPFv2 Protocols, Section 3";
---
>                  Routing for OSPFv2 Protocols, Section 3";
412c527,528
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
472c588,589
<        for Generalized Multi-Protocol Label Switching (GMPLS)
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)
519a637
>
537a656
>
542c661
<        Version 2
---
>                  Version 2
545a665,705
>   // CHANGE NOTE: The typedef path-type below has been
>   // added in this module revision
>   // RFC Editor: remove the note above and this note
>   typedef path-type {
>     type enumeration {
>       enum primary-path {
>         description
>           "Indicates that the TE path is a primary path.";
>       }
>       enum secondary-path {
>         description
>           "Indicates that the TE path is a secondary path.";
>       }
>       enum primary-reverse-path {
>         description
>           "Indicates that the TE path is a primary reverse path.";
>       }
>       enum secondary-reverse-path {
>         description
>           "Indicates that the TE path is a secondary reverse path.";
>       }
>     }
>     description
>       "The type of TE path, indicating whether a path is a primary,
>        or a reverse primary, or a secondary, or a reverse secondary
>        path.";
>   }
>
>   // CHANGE NOTE: The typedef te-gen-node-id below has been
>   // added in this module revision
>   // RFC Editor: remove the note above and this note
>   typedef te-gen-node-id {
>     type union {
>       type te-node-id;
>       type inet:ip-address;
>       type nw:node-id;
>     }
>     description
>       "Generic type that identifies a node in a TE topology.";
>   }
>
553,554c713,714
<        Traffic Engineering (RSVP-TE) for Point-to-Multipoint TE
<        Label Switched Paths (LSPs)";
---
>                  Traffic Engineering (RSVP-TE) for
>                  Point-to-Multipoint TE Label Switched Paths (LSPs)";
570c730
<        Engineering (MPLS-TE)";
---
>                  Engineering (MPLS-TE)";
606a767,774
>   // CHANGE NOTE: The base identity lsp-provisioning-error-reason
>   // has been added in this module revision
>   // RFC Editor: remove the note above and this note
>   identity lsp-provisioning-error-reason {
>     description
>       "Base identity for LSP provisioning errors.";
>   }
>
618c786
<        Section 4.7.1";
---
>                  Section 4.7.1";
636c804
<        Section 4.7.1";
---
>                  Section 4.7.1";
664,665c832,833
<        (MPLS) Traffic Engineering (TE) Loosely Routed Label Switched
<        Path (LSP)";
---
>                  (MPLS) Traffic Engineering (TE) Loosely Routed Label
>                  Switched Path (LSP)";
690c858
<        RSVP-TE
---
>                  RSVP-TE
692,693c860,861
<        Using Resource Reservation Protocol Traffic Engineering
<        (RSVP-TE)
---
>                  Using Resource Reservation Protocol Traffic
>                  Engineering (RSVP-TE)
695c863
<        Route Object (ERO)";
---
>                  Route Object (ERO)";
711c879
<        RSVP-TE
---
>                  RSVP-TE
713,714c881,882
<        Using Resource Reservation Protocol Traffic Engineering
<        (RSVP-TE)
---
>                  Using Resource Reservation Protocol Traffic
>                  Engineering (RSVP-TE)
716c884
<        Route Object (ERO)";
---
>                  Route Object (ERO)";
727c895
<        RSVP-TE
---
>                  RSVP-TE
729,730c897,898
<        Using Resource Reservation Protocol Traffic Engineering
<        (RSVP-TE)
---
>                  Using Resource Reservation Protocol
>                  Traffic Engineering (RSVP-TE)
732c900
<        Route Object (ERO)";
---
>                  Route Object (ERO)";
741,742c909,910
<        Traffic Engineering (RSVP-TE) for Point-to-Multipoint TE
<        Label Switched Paths (LSPs)
---
>                  Traffic Engineering (RSVP-TE) for
>                  Point-to-Multipoint TE Label Switched Paths (LSPs)
744c912
<        Route Object (ERO)";
---
>                  Route Object (ERO)";
753,754c921,922
<        Resource Reservation Protocol-Traffic Engineering (RSVP-TE)
<        Extensions
---
>                  Resource Reservation Protocol-Traffic Engineering
>                  (RSVP-TE) Extensions
756c924
<        Route Object (ERO)";
---
>                  Route Object (ERO)";
765c933,934
<        Multiprotocol Label Switching Traffic Engineering (GMPLS TE)
---
>                  Multiprotocol Label Switching Traffic Engineering
>                  (GMPLS TE)
767c936
<        Route Object (ERO)";
---
>                  Route Object (ERO)";
777c946
<        Multi-Layer and Multi-Region Networks (MLN/MRN)
---
>                  Multi-Layer and Multi-Region Networks (MLN/MRN)
779c948
<        Route Object (ERO)";
---
>                  Route Object (ERO)";
789c958
<        Mapping for RSVP-TE Label Switched Paths
---
>                  Mapping for RSVP-TE Label Switched Paths
791c960
<        Route Object (ERO)";
---
>                  Route Object (ERO)";
801c970
<        Mapping for RSVP-TE Label Switched Paths
---
>                  Mapping for RSVP-TE Label Switched Paths
803c972
<        Route Object (ERO)";
---
>                  Route Object (ERO)";
813c982
<        Route Object (ERO)";
---
>                  Route Object (ERO)";
823c992,993
<        Administration, and Maintenance (OAM) Configuration";
---
>                  Administration, and Maintenance (OAM)
>                  Configuration";
833c1003,1004
<        Administration, and Maintenance (OAM) Configuration";
---
>                  Administration, and Maintenance (OAM)
>                  Configuration";
842c1013
<        Route Object (ERO)
---
>                  Route Object (ERO)
844c1015
<        Link Group (SRLG) Information";
---
>                  Link Group (SRLG) Information";
855c1026
<        Loopback";
---
>                  Loopback";
864,865c1035,1036
<        Point-to-Multipoint Traffic Engineering Label Switched Paths
<        (LSPs)";
---
>                  Point-to-Multipoint Traffic Engineering Label
>                  Switched Paths (LSPs)";
887c1058,1059
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
896c1068,1069
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
905c1078,1079
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
914c1088,1089
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
923c1098,1099
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
945c1121,1122
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery
967c1144
<        Label Switched Paths (LSPs)";
---
>                  Label Switched Paths (LSPs)";
980c1157,1171
<        Label Switched Paths (LSPs)";
---
>                  Label Switched Paths (LSPs)";
>   }
>
>   // CHANGE NOTE: The identity association-type-diversity below has
>   // been added in this module revision
>   // RFC Editor: remove the note above and this note
>   identity association-type-diversity {
>     base association-type;
>     description
>       "Association Type diversity used to associate LSPs whose
>        paths are to be diverse from each other.";
>     reference
>       "RFC 8800: Path Computation Element Communication Protocol
>                  (PCEP) Extension for Label Switched Path (LSP)
>                  Diversity Constraint Signaling";
982a1174,1177
>   // CHANGE NOTE: The description of the base identity
>   // objective-function-type has been updated
>   // in this module revision
>   // RFC Editor: remove the note above and this note
985c1180
<       "Base objective function type.";
---
>       "Base identity for path objective function types.";
994c1189
<        Computation Element Communication Protocol (PCEP)";
---
>                  Computation Element Communication Protocol (PCEP)";
1004c1199
<        Computation Element Communication Protocol (PCEP)";
---
>                  Computation Element Communication Protocol (PCEP)";
1013c1208
<        Computation Element Communication Protocol (PCEP)";
---
>                  Computation Element Communication Protocol (PCEP)";
1015a1211,1213
>   // CHANGE NOTE: The identity of-minimize-agg-bandwidth-consumption
>   // below has been obsoleted in this module revision
>   // RFC Editor: remove the note above and this note
1017a1216
>     status obsolete;
1020c1219,1223
<        consumption.";
---
>        consumption.
>
>        This identity has been obsoleted: the
>        'svec-of-minimize-agg-bandwidth-consumption' identity SHOULD
>        be used instead.";
1023c1226
<        Computation Element Communication Protocol (PCEP)";
---
>                  Computation Element Communication Protocol (PCEP)";
1025a1229,1231
>   // CHANGE NOTE: The identity of-minimize-load-most-loaded-link
>   // below has been obsoleted in this module revision
>   // RFC Editor: remove the note above and this note
1027a1234
>     status obsolete;
1030c1237,1241
<        is carrying the highest load.";
---
>        is carrying the highest load.
>
>        This identity has been obsoleted: the
>        'svec-of-minimize-load-most-loaded-link' identity SHOULD
>        be used instead.";
1033c1244
<        Computation Element Communication Protocol (PCEP)";
---
>                  Computation Element Communication Protocol (PCEP)";
1035a1247,1249
>   // CHANGE NOTE: The identity of-minimize-cost-path-set
>   // below has been obsoleted in this module revision
>   // RFC Editor: remove the note above and this note
1037a1252
>     status obsolete;
1039c1254,1258
<       "Objective function for minimizing the cost on a path set.";
---
>       "Objective function for minimizing the cost on a path set.
>
>        This identity has been obsoleted: the
>        'svec-of-minimize-cost-path-set' identity SHOULD
>        be used instead.";
1042c1261
<        Computation Element Communication Protocol (PCEP)";
---
>                  Computation Element Communication Protocol (PCEP)";
1049a1269,1271
>   // CHANGE NOTE: The reference of the identity path-locally-computed
>   // below has been updated in this module revision
>   // RFC Editor: remove the note above and this note
1056,1057c1278,1279
<       "RFC 3272: Overview and Principles of Internet Traffic
<        Engineering, Section 5.4";
---
>       "RFC 9522: Overview and Principles of Internet Traffic
>                  Engineering, Section 4.4";
1059a1282,1285
>   // CHANGE NOTE: The reference of the identity
>   // path-externally-queried below has been updated
>   // in this module revision
>   // RFC Editor: remove the note above and this note
1071,1072c1297,1298
<       "RFC 3272: Overview and Principles of Internet Traffic
<        Engineering
---
>       "RFC 9522: Overview and Principles of Internet Traffic
>                  Engineering
1074c1300
<        Protocol Generic Requirements";
---
>                  Protocol Generic Requirements";
1076a1303,1306
>   // CHANGE NOTE: The reference of the identity
>   // path-explicitly-defined below has been updated
>   // in this module revision
>   // RFC Editor: remove the note above and this note
1085,1086c1315,1316
<        RFC 3272: Overview and Principles of Internet Traffic
<        Engineering";
---
>        RFC 9522: Overview and Principles of Internet Traffic
>                  Engineering";
1102c1332
<        Protocol Generic Requirements";
---
>                  Protocol Generic Requirements";
1112c1342
<        Protocol Generic Requirements";
---
>                  Protocol Generic Requirements";
1123c1353
<        Protocol Generic Requirements";
---
>                  Protocol Generic Requirements";
1145,1146c1375,1376
<        Traffic Engineering (RSVP-TE) for Point-to-Multipoint TE
<        Label Switched Paths (LSPs)";
---
>                  Traffic Engineering (RSVP-TE) for
>                  Point-to-Multipoint TE Label Switched Paths (LSPs)";
1216a1447,1458
>   // CHANGE NOTE: The identity tunnel-admin-state-auto below
>   // has been added in this module revision
>   // RFC Editor: remove the note above and this note
>   identity tunnel-admin-state-auto {
>     base tunnel-admin-state-type;
>     description
>       "Tunnel administrative auto state. The administrative status
>        in state datastore transitions to 'tunnel-admin-up' when the
>        tunnel used by the client layer, and to 'tunnel-admin-down'
>        when it is not used by the client layer.";
>   }
>
1305c1547
<        Section 2.5";
---
>                  Section 2.5";
1314c1556
<        Section 2.5";
---
>                  Section 2.5";
1321a1564,1572
>     // CHANGE NOTE: The identity lsp-restoration-restore-none
>     // below has been added in this module revision
>     // RFC Editor: remove the note above and this note
>     identity lsp-restoration-restore-none {
>       base lsp-restoration-type;
>       description
>         "No LSP affected by a failure is restored.";
>     }
>
1339a1591,1606
>     // CHANGE NOTE: The identity restoration-scheme-rerouting
>     // below has been added in this module revision
>     // RFC Editor: remove the note above and this note
>     identity restoration-scheme-rerouting {
>       base restoration-scheme-type;
>       description
>         "Restoration LSP is computed after the failure detection.
>
>          This restoration scheme is also known as
>          'Full LSP Re-routing.'";
>       reference
>         "RFC 4427: Recovery (Protection and Restoration) Terminology
>                    for Generalized Multi-Protocol Label Switching
>                    (GMPLS)";
>     }
>
1346c1613,1614
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1355c1623,1624
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1364c1633,1634
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1372c1642,1643
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
1381c1652,1653
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
1383a1656,1658
>   // CHANGE NOTE: The identity lsp-protection-reroute-extra
>   // below has been obsoleted in this module revision
>   // RFC Editor: remove the note above and this note
1385a1661
>     status obsolete;
1387c1663,1667
<       "'(Full) Rerouting' LSP protection type.";
---
>       "'(Full) Rerouting' LSP protection type.
>
>        This identity has been obsoleted: the
>        'restoration-scheme-rerouting' identity SHOULD be used
>        instead.";
1390c1670,1671
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
1392a1674,1676
>   // CHANGE NOTE: The identity lsp-protection-reroute
>   // below has been obsoleted in this module revision
>   // RFC Editor: remove the note above and this note
1394a1679
>     status obsolete;
1396c1681,1685
<       "'Rerouting without Extra-Traffic' LSP protection type.";
---
>       "'Rerouting without Extra-Traffic' LSP protection type.
>
>        This identity has been obsoleted: the
>        'restoration-scheme-rerouting' identity SHOULD be used
>        instead.";
1399c1688,1689
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
1408c1698,1699
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
1417c1708,1709
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
1426c1718,1719
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
1435c1728,1729
<        Generalized Multi-Protocol Label Switching (GMPLS) Recovery";
---
>                  Generalized Multi-Protocol Label Switching (GMPLS)
>                  Recovery";
1444c1738,1739
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1466c1761,1762
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1475c1771,1772
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1484c1781,1782
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1494c1792,1793
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1504c1803,1804
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1513c1813,1814
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1522c1823,1824
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1532c1834,1835
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1542c1845,1846
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1559c1863,1864
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1568c1873,1874
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1579c1885,1886
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1589c1896,1897
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1601c1909,1910
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1613c1922,1923
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1626c1936,1937
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1628a1940,1943
>   // CHANGE NOTE: The description and reference of the
>   // identity action-exercise have been updated in this module
>   // revision
>   // RFC Editor: remove the note above and this note
1632,1633c1947,1949
<       "An action that starts testing whether or not APS communication
<        is operating correctly.  It is of lower priority than any
---
>       "An action that starts testing whether or not Automatic
>        Protection Switching (APS) communication is operating
>        correctly.  It is of lower priority than any
1636,1637c1952,1953
<       "RFC 4427: Recovery (Protection and Restoration) Terminology
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>       "ITU-T G.808.1: Generic protection switching - Linear trail and
>                       subnetwork protection - Edition 4.0 (05/2014)";
1648c1964,1965
<        for Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                  for Generalized Multi-Protocol Label Switching
>                  (GMPLS)";
1656c1973
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1665c1982
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1674c1991
<        Forum and G.8011 Ethernet Service Switching";
---
>                  Forum and G.8011 Ethernet Service Switching";
1683c2000
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1692c2009
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1701c2018,2019
<        Control of Evolving G.709 Optical Transport Networks";
---
>                  Control of Evolving G.709 Optical Transport
>                  Networks";
1710c2028,2029
<        Switching Capable (DCSC) and Channel Set Label Extensions";
---
>                  Switching Capable (DCSC) and Channel Set Label
>                  Extensions";
1719c2038
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1728c2047
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1736c2055
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1745c2064
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1754c2073
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1763c2082
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1772c2091
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1781c2100
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1790c2109
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1799c2118
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1808c2127
<        Signaling Functional Description";
---
>                  Signaling Functional Description";
1817,1818c2136,2137
<        Signaling Extensions for G.709 Optical Transport Networks
<        Control";
---
>                  Signaling Extensions for G.709 Optical Transport
>                  Networks Control";
1827,1828c2146,2147
<        Signaling Extensions for G.709 Optical Transport Networks
<        Control";
---
>                  Signaling Extensions for G.709 Optical Transport
>                  Networks Control";
1837c2156,2157
<        Ethernet Forum and G.8011 Ethernet Service Switching";
---
>                  Ethernet Forum and G.8011 Ethernet Service
>                  Switching";
1905c2225
<        Protocol-Traffic Engineering (RSVP-TE)";
---
>                  Protocol-Traffic Engineering (RSVP-TE)";
1914c2234
<        Protocol-Traffic Engineering (RSVP-TE)";
---
>                  Protocol-Traffic Engineering (RSVP-TE)";
1917c2237,2240
<   identity path-metric-type {
---
>   // CHANGE NOTE: The path-metric-optimization-type base identity
>   // has been added in this module revision
>   // RFC Editor: remove the note above and this note
>   identity path-metric-optimization-type {
1919c2242,2243
<       "Base identity for the path metric type.";
---
>       "Base identity used to define the path metric optimization
>        types.";
1922,1923c2246,2249
<   identity path-metric-te {
<     base path-metric-type;
---
>   // CHANGE NOTE: The link-path-metric-type base identity
>   // has been added in this module revision
>   // RFC Editor: remove the note above and this note
>   identity link-path-metric-type {
1925,1928c2251,2257
<       "TE path metric.";
<     reference
<       "RFC 3785: Use of Interior Gateway Protocol (IGP) Metric as a
<        second MPLS Traffic Engineering (TE) Metric";
---
>       "Base identity used to define the link and the path metric
>        types.
>
>        The unit of the path metric value is interpreted in the
>        context of the path metric type and the derived identities
>        SHOULD describe the unit of the path metric types they
>        define.";
1931,1938c2260,2268
<   identity path-metric-igp {
<     base path-metric-type;
<     description
<       "IGP path metric.";
<     reference
<       "RFC 3785: Use of Interior Gateway Protocol (IGP) Metric as a
<        second MPLS Traffic Engineering (TE) Metric";
<   }
---
>     // CHANGE NOTE: The link-metric-type base identity
>     // and its derived identities
>     // have been added in this module revision
>     // RFC Editor: remove the note above and this note
>     identity link-metric-type {
>       base link-path-metric-type;
>       description
>         "Base identity for the link metric types.";
>     }
1940,1944c2270,2279
<   identity path-metric-hop {
<     base path-metric-type;
<     description
<       "Hop path metric.";
<   }
---
>       identity link-metric-te {
>         base link-metric-type;
>         description
>           "Traffic Engineering (TE) Link Metric.";
>         reference
>           "RFC 3630: Traffic Engineering (TE) Extensions to OSPF
>                      Version 2, Section 2.5.5
>            RFC 5305: IS-IS Extensions for Traffic Engineering,
>                      Section 3.7";
>       }
1946,1952c2281,2289
<   identity path-metric-delay-average {
<     base path-metric-type;
<     description
<       "Average unidirectional link delay.";
<     reference
<       "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions";
<   }
---
>       identity link-metric-igp {
>         base link-metric-type;
>         description
>           "Interior Gateway Protocol (IGP) Link Metric.";
>         reference
>           "RFC 3785: Use of Interior Gateway Protocol (IGP) Metric
>                      as a second MPLS Traffic Engineering (TE)
>                      Metric";
>       }
1954,1960c2291,2301
<   identity path-metric-delay-minimum {
<     base path-metric-type;
<     description
<       "Minimum unidirectional link delay.";
<     reference
<       "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions";
<   }
---
>       identity link-metric-delay-average {
>         base link-metric-type;
>         description
>           "Unidirectional Link Delay, measured in units of
>            microseconds.";
>         reference
>           "RFC 7471: OSPF Traffic Engineering (TE) Metric
>                      Extensions, Section 4.1
>            RFC 8570: IS-IS Traffic Engineering (TE) Metric
>                      Extensions, Section 4.1";
>       }
1962,1972c2303,2313
<   identity path-metric-residual-bandwidth {
<     base path-metric-type;
<     description
<       "Unidirectional Residual Bandwidth, which is defined to be
<        Maximum Bandwidth (RFC 3630) minus the bandwidth currently
<        allocated to LSPs.";
<     reference
<       "RFC 3630: Traffic Engineering (TE) Extensions to OSPF
<        Version 2
<        RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions";
<   }
---
>       identity link-metric-delay-minimum {
>         base link-metric-type;
>         description
>           "Minimum unidirectional Link Delay, measured in units of
>            microseconds.";
>         reference
>           "RFC 7471: OSPF Traffic Engineering (TE) Metric
>                      Extensions, Section 4.2
>            RFC 8570: IS-IS Traffic Engineering (TE) Metric
>                      Extensions, Section 4.2";
>       }
1974,1979c2315,2325
<   identity path-metric-optimize-includes {
<     base path-metric-type;
<     description
<       "A metric that optimizes the number of included resources
<        specified in a set.";
<   }
---
>       identity link-metric-delay-maximum {
>         base link-metric-type;
>         description
>           "Maximum unidirectional Link Delay, measured in units of
>            microseconds.";
>         reference
>           "RFC 7471: OSPF Traffic Engineering (TE) Metric
>                      Extensions, Section 4.2
>            RFC 8570: IS-IS Traffic Engineering (TE) Metric
>                      Extensions, Section 4.2";
>       }
1981,1986c2327,2461
<   identity path-metric-optimize-excludes {
<     base path-metric-type;
<     description
<       "A metric that optimizes to a maximum the number of excluded
<        resources specified in a set.";
<   }
---
>       identity link-metric-residual-bandwidth {
>         base link-metric-type;
>         description
>           "Unidirectional Residual Bandwidth, measured in units of
>            bytes per second.
>
>            It is defined to be Maximum Bandwidth minus the bandwidth
>            currently allocated to LSPs.";
>         reference
>           "RFC 7471: OSPF Traffic Engineering (TE) Metric
>                      Extensions, Section 4.5
>            RFC 8570: IS-IS Traffic Engineering (TE) Metric
>                      Extensions, Section 4.5";
>       }
>
>     // CHANGE NOTE: The base and the description of the
>     // path-metric-type identity
>     // has been updated in this module revision
>     // RFC Editor: remove the note above and this note
>     identity path-metric-type {
>       base link-path-metric-type;
>       base path-metric-optimization-type;
>       description
>         "Base identity for the path metric types.";
>     }
>
>       // CHANGE NOTE: The description and the reference of the
>       // path-metric-te identity have been updated
>       // in this module revision
>       // RFC Editor: remove the note above and this note
>       identity path-metric-te {
>         base path-metric-type;
>         description
>           "Traffic Engineering (TE) Path Metric.";
>         reference
>           "RFC 5440: Path Computation Element (PCE) Communication
>                      Protocol (PCEP), Section 7.8";
>       }
>
>       // CHANGE NOTE: The description and the reference of the
>       // path-metric-igp identity have been updated
>       // in this module revision
>       // RFC Editor: remove the note above and this note
>       identity path-metric-igp {
>         base path-metric-type;
>         description
>           "Interior Gateway Protocol (IGP) Path Metric.";
>         reference
>           "RFC 5440: Path Computation Element (PCE) Communication
>                      Protocol (PCEP), section 7.8";
>       }
>
>       // CHANGE NOTE: The description and the reference of the
>       // path-metric-hop identity have been updated
>       // in this module revision
>       // RFC Editor: remove the note above and this note
>       identity path-metric-hop {
>         base path-metric-type;
>         description
>           "Hop Count Path Metric.";
>         reference
>           "RFC 5440: Path Computation Element (PCE) Communication
>                      Protocol (PCEP), Section 7.8";
>       }
>
>       // CHANGE NOTE: The description and the reference of the
>       // path-metric-delay-average identity have been updated
>       // in this module revision
>       // RFC Editor: remove the note above and this note
>       identity path-metric-delay-average {
>         base path-metric-type;
>         description
>           "The Path Delay Metric, measured in units of
>            microseconds.";
>         reference
>           "RFC8233: Extensions to the Path Computation Element
>                     Communication Protocol (PCEP) to Compute
>                     Service-Aware Label Switched Paths (LSPs),
>                     Section 3.1.1";
>       }
>
>       // CHANGE NOTE: The description and the reference of the
>       // path-metric-delay-minimum identity have been updated
>       // in this module revision
>       // RFC Editor: remove the note above and this note
>       identity path-metric-delay-minimum {
>         base path-metric-type;
>         description
>           "The Path Min Delay Metric, measured in units of
>            microseconds.";
>         reference
>           "RFC YYYY: Carrying SR-Algorithm information in PCE-based
>                      Networks, Section 3.5.1";
>       }
>       // RFC Editor: replace YYYY with actual RFC number assigned to
>       // [I-D.ietf-pce-sid-algo] and remove this note
>
>       // CHANGE NOTE: The description and the reference of the
>       // path-metric-residual-bandwidth identity have been updated
>       // in this module revision
>       // RFC Editor: remove the note above and this note
>       identity path-metric-residual-bandwidth {
>         base path-metric-type;
>         description
>           "The Path Residual Bandwidth, defined as the minimum Link
>            Residual Bandwidth all the links along the path.
>
>            The Path Residual Bandwidth can be seen as the path
>            metric associated with the Maximum residual Bandwidth Path
>            (MBP) objective function.";
>         reference
>           "RFC 5541: Encoding of Objective Functions in the Path
>                      Computation Element Communication Protocol
>                      (PCEP)";
>       }
>
>     // CHANGE NOTE: The base of the path-metric-optimize-includes
>     // identity has been updated in this module revision
>     // RFC Editor: remove the note above and this note
>     identity path-metric-optimize-includes {
>       base path-metric-optimization-type;
>       description
>         "A metric that optimizes the number of included resources
>          specified in a set.";
>     }
>
>     // CHANGE NOTE: The base of the path-metric-optimize-excludes
>     // identity has been updated in this module revision
>     // RFC Editor: remove the note above and this note
>     identity path-metric-optimize-excludes {
>       base path-metric-optimization-type;
>       description
>         "A metric that optimizes to a maximum the number of excluded
>          resources specified in a set.";
>     }
1996c2471,2472
<       "Min-Fill LSP path placement.";
---
>       "Min-Fill LSP path placement: selects the path with most
>        available bandwidth (load balance LSPs over more links).";
2002c2478,2479
<       "Max-Fill LSP path placement.";
---
>       "Max-Fill LSP path placement: selects the path with less
>        available bandwidth (packing more LSPs over few links).";
2049a2527,2530
>   // CHANGE NOTE: The reference of the identity
>   // te-optimization-criterion below has been updated
>   // in this module revision
>   // RFC Editor: remove the note above and this note
2054,2055c2535,2536
<       "RFC 3272: Overview and Principles of Internet Traffic
<        Engineering";
---
>       "RFC 9522: Overview and Principles of Internet Traffic
>                  Engineering";
2070c2551
<        Computation Element Communication Protocol (PCEP)";
---
>                  Computation Element Communication Protocol (PCEP)";
2079c2560
<        Computation Element Communication Protocol (PCEP)";
---
>                  Computation Element Communication Protocol (PCEP)";
2110a2592,3043
>   // CHANGE NOTE: The base identity path-computation-error-reason
>   // and its derived identities below have been
>   // added in this module revision
>   // RFC Editor: remove the note above and this note
>   identity path-computation-error-reason {
>     description
>       "Base identity for path computation error reasons.";
>   }
>
>     identity path-computation-error-path-not-found {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because of an unspecified
>          reason.";
>       reference
>         "RFC 5440: Path Computation Element (PCE) Communication
>                    Protocol (PCEP), Section 7.5";
>     }
>
>     identity path-computation-error-no-topology {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because there is no topology
>          with the provided topology-identifier.";
>     }
>
>     identity path-computation-error-no-dependent-server {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because one or more dependent
>          path computation servers are unavailable.
>
>          The dependent path computation server could be
>          a Backward-Recursive Path Computation (BRPC) downstream
>          PCE or a child PCE.";
>       reference
>         "RFC 5441: A Backward-Recursive PCE-Based Computation (BRPC)
>                    Procedure to Compute Shortest Constrained
>                    Inter-Domain Traffic Engineering Label Switched
>                    Paths
>          RFC 8685: Path Computation Element Communication Protocol
>                    (PCEP) Extensions for the Hierarchical Path
>                    Computation Element (H-PCE) Architecture";
>     }
>
>     identity path-computation-error-pce-unavailable {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because PCE is not available.
>
>          It corresponds to bit 31 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 5440: Path Computation Element (PCE) Communication
>                    Protocol (PCEP)
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-no-inclusion-hop {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because there is no
>          node or link provided by one or more inclusion hops.";
>     }
>
>     identity path-computation-error-destination-unknown-in-domain {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because the destination node is
>          unknown in indicated destination domain.
>
>          It corresponds to bit 19 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 8685: Path Computation Element Communication Protocol
>                    (PCEP) Extensions for the Hierarchical Path
>                    Computation Element (H-PCE) Architecture
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-no-resource {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because there is no
>          available resource in one or more domains.
>
>          It corresponds to bit 20 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 8685: Path Computation Element Communication Protocol
>                    (PCEP) Extensions for the Hierarchical Path
>                    Computation Element (H-PCE) Architecture
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-child-pce-unresponsive {
>       base path-computation-error-no-dependent-server;
>       description
>         "Path computation has failed because child PCE is not
>          responsive.
>
>          It corresponds to bit 21 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 8685: Path Computation Element Communication Protocol
>                    (PCEP) Extensions for the Hierarchical Path
>                    Computation Element (H-PCE) Architecture
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-destination-domain-unknown {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because the destination domain
>          was unknown.
>
>          It corresponds to bit 22 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 8685: Path Computation Element Communication Protocol
>                    (PCEP) Extensions for the Hierarchical Path
>                    Computation Element (H-PCE) Architecture
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-p2mp {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because of P2MP reachability
>          problem.
>
>          It corresponds to bit 24 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 8306: Extensions to the Path Computation Element
>                    Communication Protocol (PCEP) for
>                    Point-to-Multipoint Traffic Engineering Label
>                    Switched Paths
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-no-gco-migration {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because of no Global Concurrent
>          Optimization (GCO) migration path found.
>
>          It corresponds to bit 26 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 5557: Path Computation Element Communication Protocol
>                    (PCEP) Requirements and Protocol Extensions in
>                    Support of Global Concurrent Optimization
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-no-gco-solution {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because of no GCO solution
>          found.
>
>          It corresponds to bit 25 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 5557: Path Computation Element Communication Protocol
>                    (PCEP) Requirements and Protocol Extensions in
>                    Support of Global Concurrent Optimization
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-pks-expansion {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because of Path-Key Subobject
>          (PKS)  expansion failure.
>
>          It corresponds to bit 27 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 5520: Preserving Topology Confidentiality in
>                    Inter-Domain Path Computation Using a
>                    Path-Key-Based Mechanism
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-brpc-chain-unavailable {
>       base path-computation-error-no-dependent-server;
>       description
>         "Path computation has failed because PCE BRPC chain
>          unavailable.
>
>          It corresponds to bit 28 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 5441: A Backward-Recursive PCE-Based Computation (BRPC)
>                    Procedure to Compute Shortest Constrained
>                    Inter-Domain Traffic Engineering Label Switched
>                    Paths
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-source-unknown {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because source node is
>          unknown.
>
>          It corresponds to bit 29 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 5440: Path Computation Element (PCE) Communication
>                    Protocol (PCEP);
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-destination-unknown {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because destination node is
>          unknown.
>
>          It corresponds to bit 30 of the Flags field of the
>          NO-PATH-VECTOR TLV.";
>       reference
>         "RFC 5440: Path Computation Element (PCE) Communication
>         Protocol (PCEP);
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>     identity path-computation-error-no-server {
>       base path-computation-error-reason;
>       description
>         "Path computation has failed because path computation
>          server is unavailable.";
>       reference
>         "RFC 5440: Path Computation Element (PCE) Communication
>                    Protocol (PCEP);
>
>          https://www.iana.org/assignments/pcep
>          /pcep.xhtml#no-path-vector-tlv";
>     }
>
>   // CHANGE NOTE: The base identity protocol-origin-type and
>   // its derived identities below have been
>   // added in this module revision
>   // RFC Editor: remove the note above and this note
>   identity protocol-origin-type {
>     description
>       "Base identity for protocol origin type.";
>   }
>
>     identity protocol-origin-api {
>       base protocol-origin-type;
>       description
>         "Protocol origin is via Application Programming Interface
>          (API).";
>     }
>
>     identity protocol-origin-pcep {
>       base protocol-origin-type;
>       description
>         "Protocol origin is Path Computation Engine Protocol
>          (PCEP).";
>       reference
>         "RFC 5440: Path Computation Element (PCE) Communication
>                    Protocol (PCEP)";
>     }
>
>     identity protocol-origin-bgp {
>       base protocol-origin-type;
>       description
>         "Protocol origin is Border Gateway Protocol (BGP).";
>       reference
>         "RFC 9012: The BGP Tunnel Encapsulation Attribute";
>     }
>
>   // CHANGE NOTE: The base identity svec-objective-function-type
>   // and its derived identities below have been
>   // added in this module revision
>   // RFC Editor: remove the note above and this note
>   identity svec-objective-function-type {
>     description
>       "Base identity for SVEC objective function type.";
>     reference
>       "RFC 5541: Encoding of Objective Functions in the Path
>                  Computation Element Communication Protocol (PCEP)";
>   }
>
>     identity svec-of-minimize-agg-bandwidth-consumption {
>       base svec-objective-function-type;
>       description
>         "Objective function for minimizing aggregate bandwidth
>          consumption (MBC).";
>       reference
>         "RFC 5541: Encoding of Objective Functions in the Path
>                    Computation Element Communication Protocol
>                    (PCEP)";
>     }
>
>     identity svec-of-minimize-load-most-loaded-link {
>       base svec-objective-function-type;
>       description
>         "Objective function for minimizing the load on the link that
>          is carrying the highest load (MLL).";
>       reference
>         "RFC 5541: Encoding of Objective Functions in the Path
>                    Computation Element Communication Protocol
>                    (PCEP)";
>     }
>
>     identity svec-of-minimize-cost-path-set {
>       base svec-objective-function-type;
>       description
>         "Objective function for minimizing the cost on a path set
>          (MCC).";
>       reference
>         "RFC 5541: Encoding of Objective Functions in the Path
>                    Computation Element Communication Protocol
>                    (PCEP)";
>     }
>
>     identity svec-of-minimize-common-transit-domain {
>       base svec-objective-function-type;
>       description
>         "Objective function for minimizing the number of common
>          transit domains (MCTD).";
>       reference
>         "RFC 8685: Path Computation Element Communication Protocol
>                    (PCEP) Extensions for the Hierarchical Path
>                    Computation Element (H-PCE) Architecture.";
>     }
>
>     identity svec-of-minimize-shared-link {
>       base svec-objective-function-type;
>       description
>         "Objective function for minimizing the number of shared
>          links (MSL).";
>       reference
>         "RFC 8685: Path Computation Element Communication Protocol
>                    (PCEP) Extensions for the Hierarchical Path
>                    Computation Element (H-PCE) Architecture.";
>     }
>
>     identity svec-of-minimize-shared-srlg {
>       base svec-objective-function-type;
>       description
>         "Objective function for minimizing the number of shared
>          Shared Risk Link Groups (SRLG) (MSS).";
>       reference
>         "RFC 8685: Path Computation Element Communication Protocol
>                    (PCEP) Extensions for the Hierarchical Path
>                    Computation Element (H-PCE) Architecture.";
>     }
>
>     identity svec-of-minimize-shared-nodes {
>       base svec-objective-function-type;
>       description
>         "Objective function for minimizing the number of shared
>          nodes (MSN).";
>       reference
>         "RFC 8685: Path Computation Element Communication Protocol
>                    (PCEP) Extensions for the Hierarchical Path
>                    Computation Element (H-PCE) Architecture.";
>     }
>
>   // CHANGE NOTE: The base identity svec-metric-type and
>   // its derived identities below have been
>   // added in this module revision
>   // RFC Editor: remove the note above and this note
>   identity svec-metric-type {
>     description
>       "Base identity for SVEC metric type.";
>     reference
>       "RFC 5541: Encoding of Objective Functions in the Path
>                  Computation Element Communication Protocol (PCEP)";
>   }
>
>     identity svec-metric-cumulative-te {
>       base svec-metric-type;
>       description
>         "Cumulative TE cost.";
>       reference
>         "RFC 5541: Encoding of Objective Functions in the Path
>                    Computation Element Communication Protocol
>                    (PCEP)";
>     }
>
>     identity svec-metric-cumulative-igp {
>       base svec-metric-type;
>       description
>         "Cumulative IGP cost.";
>       reference
>         "RFC 5541: Encoding of Objective Functions in the Path
>                    Computation Element Communication Protocol
>                    (PCEP)";
>     }
>
>     identity svec-metric-cumulative-hop {
>       base svec-metric-type;
>       description
>         "Cumulative Hop path metric.";
>       reference
>         "RFC 5541: Encoding of Objective Functions in the Path
>                    Computation Element Communication Protocol
>                    (PCEP)";
>     }
>
>     identity svec-metric-aggregate-bandwidth-consumption {
>       base svec-metric-type;
>       description
>         "Aggregate bandwidth consumption.";
>       reference
>         "RFC 5541: Encoding of Objective Functions in the Path
>                    Computation Element Communication Protocol
>                    (PCEP)";
>     }
>
>     identity svec-metric-load-of-the-most-loaded-link {
>       base svec-metric-type;
>       description
>         "Load of the most loaded link.";
>       reference
>         "RFC 5541: Encoding of Objective Functions in the Path
>                    Computation Element Communication Protocol
>                    (PCEP)";
>     }
>
2223,2224c3156,3157
<        Routed Label Switched Paths (LSPs) Using TE Metric
<        Extensions
---
>                  Routed Label Switched Paths (LSPs) Using TE Metric
>                  Extensions
2248,2249c3181,3182
<        Routed Label Switched Paths (LSPs) Using TE Metric
<        Extensions
---
>                  Routed Label Switched Paths (LSPs) Using TE Metric
>                  Extensions
2273,2274c3206,3207
<        Routed Label Switched Paths (LSPs) Using TE Metric
<        Extensions
---
>                  Routed Label Switched Paths (LSPs) Using TE Metric
>                  Extensions
2286c3219
<          Version 2";
---
>                    Version 2";
2350c3283
<          Version 2";
---
>                    Version 2";
2405,2406c3338,3339
<          Routed Label Switched Paths (LSPs) Using TE Metric
<          Extensions
---
>                    Routed Label Switched Paths (LSPs) Using TE Metric
>                    Extensions
2416c3349
<          Networks";
---
>                    Networks";
2437,2438c3370,3371
<          Routed Label Switched Paths (LSPs) Using TE Metric
<          Extensions
---
>                    Routed Label Switched Paths (LSPs) Using TE Metric
>                    Extensions
2472c3405
<            Extensions, Section 6";
---
>                      Extensions, Section 6";
2506a3440,3442
>   // CHANGE NOTE: The explicit-route-hop grouping below has been
>   // updated in this module revision
>   // RFC Editor: remove the note above and this note
2514a3451,3459
>           must "node-id-uri or node-id" {
>             description
>               "At least one node identifier MUST be present.";
>           }
>           leaf node-id-uri {
>             type nw:node-id;
>             description
>               "The identifier of a node in the topology.";
>           }
2517d3461
<             mandatory true;
2531c3475
<              Section 4.3, EXPLICIT_ROUTE in RSVP-TE
---
>                        Section 4.3, EXPLICIT_ROUTE in RSVP-TE
2533c3477,3478
<              ReSerVation Protocol - Traffic Engineering (RSVP-TE)";
---
>                        ReSerVation Protocol - Traffic Engineering
>                        (RSVP-TE)";
2560c3505
<              Section 4.3, EXPLICIT_ROUTE in RSVP-TE
---
>                        Section 4.3, EXPLICIT_ROUTE in RSVP-TE
2562c3507,3508
<              ReSerVation Protocol - Traffic Engineering (RSVP-TE)";
---
>                        ReSerVation Protocol - Traffic Engineering
>                        (RSVP-TE)";
2566a3513,3523
>           must "(link-tp-id-uri or link-tp-id) and " +
>                 "(node-id-uri or node-id)" {
>             description
>               "At least one node identifier and at least one Link
>               Termination Point (LTP) identifier MUST be present.";
>           }
>           leaf link-tp-id-uri {
>             type nt:tp-id;
>             description
>               "Link Termination Point (LTP) identifier.";
>           }
2569d3525
<             mandatory true;
2574a3531,3535
>           leaf node-id-uri {
>             type nw:node-id;
>             description
>               "The identifier of a node in the topology.";
>           }
2577d3537
<             mandatory true;
2597c3557
<              Section 4.3, EXPLICIT_ROUTE in RSVP-TE
---
>                        Section 4.3, EXPLICIT_ROUTE in RSVP-TE
2599c3559,3560
<              ReSerVation Protocol - Traffic Engineering (RSVP-TE)";
---
>                        ReSerVation Protocol - Traffic Engineering
>                        (RSVP-TE)";
2631a3593,3595
>   // CHANGE NOTE: The explicit-route-hop grouping below has been
>   // updated in this module revision
>   // RFC Editor: remove the note above and this note
2646a3611,3614
>           must "node-id-uri or node-id" {
>             description
>               "At least one node identifier MUST be present.";
>           }
2648a3617,3621
>           leaf node-id-uri {
>             type nw:node-id;
>             description
>               "The identifier of a node in the topology.";
>           }
2651d3623
<             mandatory true;
2662c3634
<                Tunnels
---
>                          Tunnels
2664c3636
<                Node-Id Sub-Object";
---
>                          Node-Id Sub-Object";
2687c3659
<                Tunnels
---
>                          Tunnels
2689c3661
<                Node-Id Sub-Object";
---
>                          Node-Id Sub-Object";
2696a3669,3679
>           must "(link-tp-id-uri or link-tp-id) and " +
>               "(node-id-uri or node-id)" {
>             description
>               "At least one node identifier and at least one Link
>               Termination Point (LTP) identifier MUST be present.";
>           }
>           leaf link-tp-id-uri {
>             type nt:tp-id;
>             description
>               "Link Termination Point (LTP) identifier.";
>           }
2699d3681
<             mandatory true;
2704a3687,3691
>           leaf node-id-uri {
>             type nw:node-id;
>             description
>               "The identifier of a node in the topology.";
>           }
2717c3704
<                Tunnels
---
>                          Tunnels
2719c3706
<                Node-Id Sub-Object";
---
>                          Node-Id Sub-Object";
2725c3712,3713
<              ReSerVation Protocol - Traffic Engineering (RSVP-TE)";
---
>                        ReSerVation Protocol - Traffic Engineering
>                        (RSVP-TE)";
2742c3730
<                Tunnels
---
>                          Tunnels
2744c3732
<                Node-Id Sub-Object";
---
>                          Node-Id Sub-Object";
2842a3831,3841
>
>          In case the restriction is 'inclusive', the bit-position is
>          set if the corresponding mapped label is available.
>          In this case, if the range-bitmap is not present, all the
>          labels in the range are available.
>
>          In case the restriction is 'exclusive', the bit-position is
>          set if the corresponding mapped label is not available.
>          In this case, if the range-bitmap is not present, all the
>          labels in the range are not available.
>
2876c3875
<            for GMPLS-Controlled Networks";
---
>                      for GMPLS-Controlled Networks";
2881a3881,3883
>   // CHANGE NOTE: The grouping optimization-metric-entry below has
>   // been updated in this module revision
>   // RFC Editor: remove the note above and this note
2887c3889
<         base path-metric-type;
---
>         base path-metric-optimization-type;
2933c3935,3936
<          Generalized Multi-Protocol Label Switching (GMPLS)";
---
>                    Generalized Multi-Protocol Label Switching
>                    (GMPLS)";
2964a3968,3970
>   // CHANGE NOTE: The grouping tunnel-constraints below has
>   // been updated in this module revision
>   // RFC Editor: remove the note above and this note
2968a3975,3979
>     leaf network-id {
>       type nw:network-id;
>       description
>         "The network topology identifier.";
>     }
2972a3984,3986
>   // CHANGE NOTE: The grouping path-constraints-route-objects below
>   // has been updated in this module revision
>   // RFC Editor: remove the note above and this note
2977c3991
<     container explicit-route-objects-always {
---
>     container explicit-route-objects {
2979c3993
<         "Container for the 'exclude route' object list.";
---
>         "Container for the explicit route object lists.";
3101a4116,4118
>   // CHANGE NOTE: The grouping generic-path-metric-bounds below
>   // has been updated in this module revision
>   // RFC Editor: remove the note above and this note
3107c4124
<         "TE path metric bounds container.";
---
>         "Top-level container for the list of path metric bounds.";
3111c4128,4136
<           "List of TE path metric bounds.";
---
>           "List of path metric bounds, which can apply to link and
>            path metrics.
>
>            TE paths which have at least one path metric which
>            exceeds the specified bounds MUST NOT be selected.
>
>            TE paths that traverse TE links which have at least one
>            link metric which exceeds the specified bounds MUST NOT
>            be selected.";
3114c4139
<             base path-metric-type;
---
>             base link-path-metric-type;
3124,3126c4149,4155
<             "Upper bound on the end-to-end TE path metric.  A zero
<              indicates an unbounded upper limit for the specific
<              'metric-type'.";
---
>             "Upper bound on the specified 'metric-type'.
>
>              A zero indicates an unbounded upper limit for the
>              specificied 'metric-type'.
>
>              The unit of is interpreted in the context of the
>              'metric-type' identity.";
3131a4161,4163
>   // CHANGE NOTE: The grouping generic-path-metric-bounds below
>   // has been updated in this module revision
>   // RFC Editor: remove the note above and this note
3152a4185
>             status deprecated;
3154c4187,4190
<               "Container for the list of tiebreakers.";
---
>               "Container for the list of tiebreakers.
>
>                This container has been deprecated by the tiebreaker
>                leaf.";
3156a4193
>               status deprecated;
3164a4202
>                 status deprecated;
3189a4228,4236
>     leaf tiebreaker {
>       type identityref {
>         base path-tiebreaker-type;
>       }
>       default "te-types:path-tiebreaker-random";
>       description
>         "The tiebreaker criteria to apply on an equally favored set
>          of paths, in order to pick the best.";
>     }
3376a4424,4484
>     }
>   }
>
>   // NOTE: The grouping encoding-and-switching-type below has been
>   // added in this module revision
>   // RFC Editor: remove the note above and this note
>   grouping encoding-and-switching-type {
>     description
>       "Common grouping to define the LSP encoding and
>        switching types";
>     leaf encoding {
>       type identityref {
>         base te-types:lsp-encoding-types;
>       }
>       description
>         "LSP encoding type.";
>       reference
>         "RFC 3945: Generalized Multi-Protocol Label Switching (GMPLS)
>                    Architecture";
>     }
>     leaf switching-type {
>       type identityref {
>         base te-types:switching-capabilities;
>       }
>       description
>         "LSP switching type.";
>       reference
>         "RFC 3945: Generalized Multi-Protocol Label Switching (GMPLS)
>                    Architecture";
>     }
>   }
>
>   // CHANGE NOTE: The typedef te-gen-node-id below has been
>   // added in this module revision
>   // RFC Editor: remove the note above and this note
>   grouping te-generic-node-id {
>     description
>       "A reusable grouping for a TE generic node identifier.";
>     leaf id {
>       type te-gen-node-id;
>       description
>         "The identifier of the node. Can be represented as IP
>          address or dotted quad address or as an URI.";
>     }
>     leaf type {
>       type enumeration {
>         enum ip {
>           description
>             "IP address representation of the node identifier.";
>         }
>         enum te-id {
>           description
>             "TE identifier of the node";
>         }
>         enum node-id {
>           description
>             "URI representation of the node identifier.";
>         }
>       }
>       description
>         "Type of node identifier representation.";

Packet TE Types YANG Diffs
RFC Editor: please remove this appendix before publication.
This section provides the diff between the YANG module in section 3.2 of [RFC8776] and the YANG model revision in Section 5.
The intention of this appendix is to facilitate focusing the review of the YANG model in Section 5 to the changes compared with the YANG model in [RFC8776].
This diff has been generated using the following UNIX commands to compare the YANG module revisions in section 3.2 of [RFC8776] and in Section 5:

diff ietf-te-packet-types@2020-06-10.yang ietf-te-packet-types.yang
     > model-diff.txt
sed 's/^/    /' model-diff.txt > model-diff-spaces.txt
sed 's/^    >   /    >   /' model-diff-spaces.txt
    > model-updates.txt

The output (model-updates.txt) is reported here:

6c6,10
<   /* Import TE generic types */
---
>   import ietf-yang-types {
>     prefix yang;
>     reference
>       "RFC 6991: Common YANG Data Types";
>   }
11c15
<       "RFC 8776: Common YANG Data Types for Traffic Engineering";
---
>       "RFC XXXX: Common YANG Data Types for Traffic Engineering";
12a17,18
>   // RFC Editor: replace XXXX with actual RFC number
>   // and remove this note
22c28
<                <mailto:tsaad@juniper.net>
---
>                <mailto:tsaad.net@gmail.com>
37,39c43,53
<      data type definitions specific to MPLS TE.  The model fully
<      conforms to the Network Management Datastore Architecture
<      (NMDA).
---
>      data type definitions specific to Packet Traffic Enginnering
>      (TE).
>
>      The model fully conforms to the Network Management Datastore
>      Architecture (NMDA).
>
>      The key words 'MUST', 'MUST NOT', 'REQUIRED', 'SHALL', 'SHALL
>      NOT', 'SHOULD', 'SHOULD NOT', 'RECOMMENDED', 'NOT RECOMMENDED',
>      'MAY', and 'OPTIONAL' in this document are to be interpreted as
>      described in BCP 14 (RFC 2119) (RFC 8174) when, and only when,
>      they appear in all capitals, as shown here.
41c55
<      Copyright (c) 2020 IETF Trust and the persons identified as
---
>      Copyright (c) 2024 IETF Trust and the persons identified as
46c60
<      the license terms contained in, the Simplified BSD License set
---
>      the license terms contained in, the Revised BSD License set
51,52c65,86
<      This version of this YANG module is part of RFC 8776; see the
<      RFC itself for full legal notices.";
---
>      This version of this YANG module is part of RFC XXXX
>      (https://www.rfc-editor.org/info/rfcXXXX); see the RFC itself
>      for full legal notices.";
>   revision 2024-07-23 {
>     description
>       "This revision adds the following new identities:
>        - bandwidth-profile-type;
>        - link-metric-delay-variation;
>        - link-metric-loss;
>        - path-metric-delay-variation;
>        - path-metric-loss.
>
>       This revision adds the following new groupings:
>        - te-packet-path-bandwidth;
>        - te-packet-link-bandwidth.
>
>       This revision provides also few editorial changes.";
>     reference
>       "RFC XXXX: Common YANG Data Types for Traffic Engineering";
>   }
>   // RFC Editor: replace XXXX with actual RFC number, update date
>   // information and remove this note
61c95,201
<   /**
---
>   /*
>    * Identities
>    */
>
>   // CHANGE NOTE: The base identity bandwidth-profile-type and
>   // its derived identities below have been
>   // added in this module revision
>   // RFC Editor: remove the note above and this note
>   identity bandwidth-profile-type {
>     description
>       "Bandwidth Profile Types";
>   }
>
>     identity mef-10 {
>       base bandwidth-profile-type;
>       description
>         "MEF 10 Bandwidth Profile";
>       reference
>         "MEF 10.3: Ethernet Services Attributes Phase 3";
>     }
>
>     identity rfc-2697 {
>       base bandwidth-profile-type;
>       description
>         "RFC 2697 Bandwidth Profile";
>       reference
>         "RFC 2697: A Single Rate Three Color Marker";
>     }
>
>     identity rfc-2698 {
>       base bandwidth-profile-type;
>       description
>         "RFC 2698 Bandwidth Profile";
>       reference
>         "RFC 2698: A Two Rate Three Color Marker";
>     }
>
>     identity rfc-4115 {
>       base bandwidth-profile-type;
>       description
>         "RFC 4115 Bandwidth Profile";
>       reference
>         "RFC 4115: A Differentiated Service Two-Rate, Three-Color
>                    Marker with Efficient Handling of in-Profile
>                    Traffic";
>     }
>
>     // CHANGE NOTE: The identity link-metric-delay-variation
>     // below has been added in this module revision
>     // RFC Editor: remove the note above and this note
>     identity link-metric-delay-variation {
>       base te-types:link-metric-type;
>       description
>         "The Unidirectional Delay Variation Metric,
>          measured in units of microseconds.";
>       reference
>         "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions,
>                    Section 4.3
>          RFC 8570: IS-IS Traffic Engineering (TE) Metric Extensions,
>                    Section 4.3";
>     }
>
>     // CHANGE NOTE: The identity link-metric-loss below has
>     // been added in this module revision
>     // RFC Editor: remove the note above and this note
>     identity link-metric-loss {
>       base te-types:link-metric-type;
>       description
>         "The Unidirectional Link Loss Metric,
>          measured in units of 0.000003%.";
>       reference
>         "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions,
>                    Section 4.4
>          RFC 8570: IS-IS Traffic Engineering (TE) Metric Extensions,
>                    Section 4.4";
>     }
>
>     // CHANGE NOTE: The identity path-metric-delay-variation
>     // below has been added in this module revision
>     // RFC Editor: remove the note above and this note
>     identity path-metric-delay-variation {
>       base te-types:path-metric-type;
>       description
>         "The Path Delay Variation Metric,
>          measured in units of microseconds.";
>       reference
>         "RFC 8233: Extensions to the Path Computation Element
>                    Communication Protocol (PCEP) to Compute
>                    Service-Aware Label Switched Paths (LSPs),
>                    Section 3.1.2";
>     }
>
>     // CHANGE NOTE: The identity path-metric-loss below has
>     // been added in this module revision
>     // RFC Editor: remove the note above and this note
>     identity path-metric-loss {
>       base te-types:path-metric-type;
>       description
>         "The Path Loss Metric, measured in units of 0.000003%.";
>       reference
>         "RFC 8233: Extensions to the Path Computation Element
>                    Communication Protocol (PCEP) to Compute
>                    Service-Aware Label Switched Paths (LSPs),
>                    Section 3.1.3";
>     }
>
>   /*
91c231
<        MPLS Traffic Engineering";
---
>                  MPLS Traffic Engineering";
102c242
<        MPLS Traffic Engineering";
---
>                  MPLS Traffic Engineering";
149c289
<        MPLS Traffic Engineering";
---
>                  MPLS Traffic Engineering";
177,178c317,318
<        Constraints Model for Diffserv-aware MPLS Traffic Engineering
<        & Performance Comparisons";
---
>                  Constraints Model for Diffserv-aware MPLS Traffic
>                  Engineering & Performance Comparisons";
180a321,324
>   /*
>    * Groupings
>    */
>
220c364
<              Statement, Section 4.2";
---
>                        Statement, Section 4.2";
229c373
<              Extensions
---
>                        Extensions
231,232c375,376
<              Explicitly Routed Label Switched Paths (LSPs) Using
<              TE Metric Extensions
---
>                        Explicitly Routed Label Switched Paths (LSPs)
>                        Using TE Metric Extensions
234c378
<              Extensions";
---
>                        Extensions";
247c391
<              Extensions, Section 4.4";
---
>                        Extensions, Section 4.4";
256c400
<              Extensions
---
>                        Extensions
258,259c402,403
<              Explicitly Routed Label Switched Paths (LSPs) Using
<              TE Metric Extensions
---
>                        Explicitly Routed Label Switched Paths (LSPs)
>                        Using TE Metric Extensions
261c405
<              Extensions";
---
>                        Extensions";
283c427
<              Extensions
---
>                        Extensions
285,286c429,430
<              Explicitly Routed Label Switched Paths (LSPs) Using
<              TE Metric Extensions
---
>                        Explicitly Routed Label Switched Paths (LSPs)
>                        Using TE Metric Extensions
288c432
<              Extensions";
---
>                        Extensions";
305c449
<              Extensions
---
>                        Extensions
307,308c451,452
<              Explicitly Routed Label Switched Paths (LSPs) Using
<              TE Metric Extensions
---
>                        Explicitly Routed Label Switched Paths (LSPs)
>                        Using TE Metric Extensions
310c454
<              Extensions";
---
>                        Extensions";
321c465
<              Statement, Section 4.2";
---
>                        Statement, Section 4.2";
330c474
<              Extensions
---
>                        Extensions
332,333c476,477
<              Explicitly Routed Label Switched Paths (LSPs) Using
<              TE Metric Extensions
---
>                        Explicitly Routed Label Switched Paths (LSPs)
>                        Using TE Metric Extensions
335c479
<              Extensions";
---
>                        Extensions";
358,363c502,508
<           "RFC 7471: OSPF Traffic Engineering (TE) Metric Extensions
<            RFC 7823: Performance-Based Path Selection for
<            Explicitly Routed Label Switched Paths (LSPs) Using
<            TE Metric Extensions
<            RFC 8570: IS-IS Traffic Engineering (TE) Metric
<            Extensions";
---
>             "RFC 7471: OSPF Traffic Engineering (TE) Metric
>                        Extensions
>              RFC 7823: Performance-Based Path Selection for
>                        Explicitly Routed Label Switched Paths (LSPs)
>                        Using TE Metric Extensions
>              RFC 8570: IS-IS Traffic Engineering (TE) Metric
>                        Extensions";
407a553,599
>   // CHANGE NOTE: The grouping
>   // one-way-performance-metrics-gauge-packet has been added in
>   // this module revision
>   // RFC Editor: remove the note above and this note
>   grouping one-way-performance-metrics-gauge-packet {
>     description
>       "One-way packet PM throttle grouping.
>
>        This grouping is used to report the same metrics defined in
>        the one-way-performance-metrics-packet grouping, using gauges
>        instead of uint32 data types and referencing IPPM RFCs
>        instead of IGP-TE RFCs.";
>     leaf one-way-min-delay {
>       type yang:gauge64;
>       description
>         "One-way minimum delay or latency in microseconds.";
>     }
>     leaf one-way-max-delay {
>       type yang:gauge64;
>       description
>         "One-way maximum delay or latency in microseconds.";
>       reference
>         "RFC 7679: A One-Way Delay Metric for IP Performance
>                    Metrics (IPPM)";
>     }
>     leaf one-way-delay-variation {
>       type yang:gauge64;
>       description
>         "One-way delay variation in microseconds.";
>       reference
>         "RFC 3393: IP Packet Delay Variation Metric for IP
>                    Performance Metrics (IPPM)";
>     }
>     leaf one-way-packet-loss {
>       type decimal64 {
>         fraction-digits 5;
>         range "0..100";
>       }
>       description
>         "The ratio of packets dropped to packets transmitted between
>          two endpoints.";
>       reference
>         "RFC 7680: A One-Way Loss Metric for IP Performance
>                    Metrics (IPPM)";
>     }
>   }
>
447a640,683
>   // CHANGE NOTE: The grouping
>   // two-way-performance-metrics-gauge-packet has been added in
>   // this module revision
>   // RFC Editor: remove the note above and this note
>   grouping two-way-performance-metrics-gauge-packet {
>     description
>       "Two-way packet PM throttle grouping.
>
>        This grouping is used to report the same metrics defined in
>        the two-way-performance-metrics-packet grouping, using gauges
>        instead of uint32 data types and referencing IPPM RFCs
>        instead of IGP-TE RFCs.";
>     leaf two-way-min-delay {
>       type yang:gauge64;
>       description
>         "Two-way minimum delay or latency in microseconds.";
>       reference
>         "RFC 2681: A Round-trip Delay Metric for IPPM";
>     }
>     leaf two-way-max-delay {
>       type yang:gauge64;
>       description
>         "Two-way maximum delay or latency in microseconds.";
>       reference
>         "RFC 2681: A Round-trip Delay Metric for IPPM";
>     }
>     leaf two-way-delay-variation {
>       type yang:gauge64;
>       description
>         "Two-way delay variation in microseconds.";
>       reference
>         "RFC 5481: Packet Delay Variation Applicability Statement";
>     }
>     leaf two-way-packet-loss {
>       type decimal64 {
>         fraction-digits 5;
>         range "0..100";
>       }
>       description
>         "The ratio of packets dropped to packets transmitted between
>          two endpoints.";
>     }
>   }
>
472a709,780
>     }
>   }
>
>   // CHANGE NOTE: The te-packet-path-bandwidth below has been
>   // added in this module revision
>   // RFC Editor: remove the note above and this note
>   grouping te-packet-path-bandwidth {
>     description
>       "Path bandwidth for Packet. ";
>     leaf bandwidth-profile-name {
>       type string;
>       description
>         "Name of Bandwidth Profile.";
>     }
>     leaf bandwidth-profile-type {
>       type identityref {
>         base bandwidth-profile-type;
>       }
>       description
>         "Type of Bandwidth Profile.";
>     }
>     leaf cir {
>       type uint64;
>       units "bits/second";
>       mandatory true;
>       description
>         "Committed Information Rate (CIR).";
>     }
>     leaf cbs {
>       type uint64;
>       units "bits/second";
>       mandatory true;
>       description
>         "Committed Burst Size (CBS).";
>     }
>     leaf eir {
>       type uint64;
>       units "bits/second";
>       description
>         "Excess Information Rate (EIR).";
>     }
>     leaf ebs {
>       type uint64;
>       units "bytes";
>       description
>         "Excess Burst Size (EBS).";
>     }
>     leaf pir {
>       type uint64;
>       units "bits/second";
>       description
>         "Peak Information Rate (PIR).";
>     }
>     leaf pbs {
>       type uint64;
>       units "bytes";
>       description
>         "Peak Burst Size (PBS).";
>     }
>   }
>
>   // CHANGE NOTE: The te-packet-path-bandwidth below has been
>   // added in this module revision
>   // RFC Editor: remove the note above and this note
>   grouping te-packet-link-bandwidth {
>     description
>       "Link Bandwidth for Packet. ";
>     leaf packet-bandwidth {
>       type uint64;
>       units "bits/second";
>       description
>         "Available bandwith value.";

Option Considered for updating RFC8776
RFC Editor: please remove this appendix before publication.
The concern is how to be able to update the ietf-te-types YANG module published in [RFC8776] without delaying too much the progress of the mature WG documents.
Three possible options have been identified to address this concern.
One option is to keep these definitions in the YANG modules where they have initially been defined: other YANG modules can still import them. The drawback of this approach is that it defeating the value of common YANG modules like ietf-te-types since common definitions will be spread around multiple specific YANG modules.
A second option is to define them in a new common YANG module (e.g., ietf-te-types-ext). The drawback of this approach is that it will increase the number of YANG modules providing tiny updates to the ietf-te-types YANG module.
A third option is to develop a revision of the ietf-te-types YANG module within an RFC8776-bis. The drawback of this approach is that the process for developing a big RFC8776-bis just for a tiny update is too high. Moreover, as suggested during IETF 113 Netmod WG discussion, a new revision of the ietf-te-packet-types YANG module, which is also defined in [RFC8776] but it does not need to be revised, needs to be published just to change its reference to RFC8776-bis (see [RFC9314]).
A fourth option, considered in the -00 WG version, was to:
- describe within the document only the updates to the ietf-te-types YANG module proposed by this document;
- include the whole updated YANG model within the main body;
- add some notes, to be removed before publication, within updated YANG model to focus the review only to the updates to the ietf-te-types YANG module proposed by this document.
Based on the feedbacks from IETF 114 discussion, this version has been restructured to become an RFC8776-bis, with some notes, to be removed before publication, to focus the review only to the updates to the ietf-te-types YANG module proposed by this document.
During the Netmod WG session at IETF 114, an alternative process has been introduced:
https://datatracker.ietf.org/meeting/114/materials/slides-114-netmod-ad-topic-managing-the-evolution-of-ietf-yang-modules-00.pdf
Future updates of this document could align with the proposed approach.
Acknowledgements
The authors would like to thank Robert Wilton, Lou Berger, Mahesh Jethanandani and Jeff Haas for their valuable input to the discussion about the process to follow to provide tiny updates to a YANG module already published as an RFC.
This document was prepared using kramdown.
Contributors
Vishnu Pavan Beeram
Juniper Networks
vbeeram@juniper.net
Rakesh Gandhi
Cisco Systems, Inc.
rgandhi@cisco.com