# How to set up Audacity

### From Audacity Manual

If you are recording from a USB turntable or USB interface, please go to the set up instructions at Recording with USB turntables.

## Setting Up Audacity

The Device toolbar is displayed by default in a new installation of Audacity. If the Device toolbar is not visible, click on View > Toolbars > Device Toolbar.

You may want to expand the size of the Device toobar by dragging right on the drag handle.

1. Click on the Input Channels drop-down menu and choose whether to record in stereo or mono
2. Set the Output Device and Input Device drop-down menus to the built-in computer sound device, or to the specific sound device your cable is plugged into. Do NOT select "Microsoft Sound Mapper" or "Primary Sound Driver" on Windows machines:
   - Windows 7/Vista: Choose the line-in option for your connected sound device (for example, "Line-In: Realtek HD Device")
   - Windows XP or earlier or Linux: Select the connected sound device.
   - OS X: Select the "Built-in Audio: Line In" input device, or "USB Audio CODEC" if you are using an external USB audio adapter
3. If you cannot choose your input source as described above, or if the line-in input won't record, you can use the operating system mixer device to choose the required input. For instructions, see the further help for Windows, Mac OS X or Linux on our Wiki.

## Monitoring

1. Decide if you want to "monitor" your recording, that is, hear it played back as you make it:
   - Windows or Linux: Try "hardware playthrough". To use this, open the operating system sound mixer, then the Playback section, then unmute line-in and turn the volume up. You can find the system mixer in the Control Panel at Sound on Windows 7 or Vista, or Sounds and Audio Devices on Windows XP. On Linux, you can use ALSAmixer.
   - OS X: Try "software playthrough" in Recording Preferences or under the Transport menu

   If hardware playthrough does not work, or if the playback and recording devices in Preferences are different, choose "software playthrough" in Recording Preferences. If neither playthrough works on OS X, obtain the free LineIn software playthrough tool from Rogue Amoeba. Note: software playthrough will have a slight delay, and causes some extra load on the computer.

2. Set the volume level of your recording input. Click on the downward pointing arrow in the right hand (red) VU recording level meters:
   and click "Start Monitoring". While playing a loud part of your tape or record, adjust the Input Slider on the Mixer Toolbar so the recording meters are almost reaching the right-hand end of the scale. Don't let the meter bars actually reach the right edge, or the red hold lights to right of the meter will come on, indicating you'll have distortion in the recording. If the recording level meters are not visible, click View > Toolbars and check Meter Toolbar.
   Try to aim for a maximum peak of around –6.0 dB (or 0.5 if you have your meters set to linear rather than dB). Tip: enlarging the Meter Toolbar by clicking and dragging helps with this task.
3. If the Mixer Toolbar Input Slider does not control the input level correctly, or is greyed out on maximum, use the input slider in the operating system mixer device to regulate the input level. For instructions, see the further help for Windows, Mac OS X or Linux on our Wiki.

## Links

> Forward to: Basic Recording, Editing and Exporting

< Back to: How to connect your equipment

|< Tutorial - Copying tapes, LPs or MiniDiscs to CD

##### Views

##### Help Location

- Local manual in use
- Internet manual